## NTIC001

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

NTIC001 The command /CHANGE-TASK-CPU-LIMIT could not be executed successfully for the specified task.

### Meaning

Possible reasons are:
- the specified task does not exist
- the MONJV does not identify an existing task
- the MONJV is owned by another system in the MSCF network
- parameter error (wrong value: seconds or percent)

### Response

Correct the command!

## NTITD01

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD01 SHORTAGE OF RESOURCES. FUNCTION TERMINATED ABNORMALLY.

## NTITD02

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD02 INVALID CALL OF SUBSYSTEM TASKDATE.

## NTITD03

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD03 SYSTEM FUNCTION '(&00)' COULD NOT BE EXECUTED SUCCESSFULLY . RETURNCODE '(&01)'.

## NTITD04

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD04 COMMAND NOT ALLOWED WHILE PROGRAM IS LOADED.

## NTITD05

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD05 VALUE OF PARAMETER 'DATE' NOT IN THE ALLOWED RANGE.

## NTITD06

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NTITD06 LOADING OF SUBSYSTEM ABORTED BECAUSE OF MISSING REPS IN SUBSYSTEM GET-TIME (PM A0394142).

### Meaning

It is necessary to include the Reps A0394142 into the subsystem ^
GET-TIME, before starting TASKDATE

## NTITD07

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NTITD07 LOADING OF SUBSYSTEM ABORTED BECAUSE OF MISSING REPS IN BS2000-GA (PM A0394142).

### Meaning

It is necessary to include the Reps A0394142 into BS2000-GA, ^
before starting TASKDATE

## NTITD08

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD08 INSTALLATION OF TASKDATE FAILED. REPLY: <tsn>.

### Meaning

Please inform the system administrator.

## NTITD09

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD09 TERMINATION OF SUBSYSTEM NOT POSSIBLE NOW. TERMINATE ALL THE ENTER-JOBS INDICATED BY /SHOW-TASK-CLOCK *TSN(TSN=*ALL). AFTERWARDS: TRY AGAIN TO TERMINATE THE SUBSYSTEM.

## NTITD10

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD10 NO INFORMATION AVAILABLE BECAUSE NO SIMULATED TIME IS DEFINED

## NTITD11

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NTITD11 SPECIFIED TASK NOT (RESP.: NO MORE) EXISTING

## NTIX100

Destination: CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

NTIX100 Join of XCS can not be performed. System error occured in run of task "TIME".

### Meaning

An internal error inhibits the join of a XCS.
Diagnose data are generated automatically.

### Response

To make possible the joining of XCS the system has to be
restarted (STARTUP).

## NTIX101

Destination: CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

NTIX101 '(&00)' seconds wait time for synchronization of system time with the time of the XCS

### Meaning

Before the system can join the XCS, the system time has to be adjusted
to XCS time. This adjustment requires the given time span.

### Response

If the systems building the XCS are already started with synchronized
times, the wait time diminishes to unsignificant value.

## NTIX102

Destination: CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

NTIX102 Join of XCS not possible. Difference between the system times of the local system and the XCS node system too large.

### Meaning

For joining the XCS the maximal difference between
the system times must not be exceeded.

### Response

New startup with convenient system time.

## NTIX103

Destination: CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

NTIX103 Join of XCS not possible. TimeServer/radio clock disables synchronisation and the actual difference between system times is too large

### Response

Before the next try of join connect the TimeServer/radio clock to the
XCS or disconnect the TimeServer/radio clock from the local system.

## NTIX104

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NTIX104 XCS-TIME aborts XCS-session, Reason: '(&00)'

### Meaning

XCS-TIME will abort the actual XCS-session
(&00): Reason for abort:
1: Internal error during resource allocation
2: Time synchronisation during join failed
3: Time difference during join to large
4: No time synchronisation possible for a long time
due to communication failure
5: Internal error during load of subsystem XCS-TIME
6: A radio-clock is installed, the XCS-time is greater
than the local time and at least one XCS-partner
has OSD before V4.0
7: Time difference to large

### Response

Reason 3,6,7:
Correct the time of the existing XCS.
Else:
Save the Serslogfile and inform the diagnosegroup.

## NTIX110

Destination: CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

NTIX110 Abort of XCS. The difference between the system times of the local system and the XCS node systems is too large.

### Meaning

The time supported from any partner system is larger than
the local system time plus a allowed difference.
A possible reason is the configuration error, that only a few
systems in the XCS have a radio clock.

### Response

The configuration error must be corrected.

## NTIX112

Destination: CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

NTIX112 Warning: no time synchronisation for a long time.

### Meaning

No time update from other hosts of the XCS arrived during a long time.
A possible reason is that the token of NSM is broken.

### Response

The configuration error must be corrected.

©2025 Fujitsu | BS2000 System Messages