## ROBN001

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN001 SYNTAX ERROR

### Meaning

AML returns an error code due to :
- syntax error
- command invalid
- the specified requestor is not known to AMU
- the message with the sequence number is unknown

### Response

Contact the maintenance staff if necessary.

## ROBN002

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN002 UNEXPECTED RESPONSE FROM ROBOT

### Meaning

AML returns an error code due to :
- A command in wrong format was sent.
- The given command contains an unknown option.
Command cannot be executed.

### Response

Contact the maintenance staff if necessary.

## ROBN003

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN003 SERIOUS ERROR IN SETUP FILE

### Meaning

AML returns an error code due to :
- There is no entry in AMU.INI.
- AMUP can't open a file.

### Response

Look at the installation guide and check your
entries in the configuration submenu. Contact the maintenance
staff if necessary.

## ROBN004

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN004 SERIOUS ERROR IN ARCHIVE DATABASE

### Meaning

AML returns an error code due to :
- A severe error in the archive database has occurred.
- The Data Base Manager reports a warning or an error.
- A database module wasn't bound successfully.

### Response

Contact the maintenance staff if necessary.

## ROBN005

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN005 ROBOT NOT READY

### Meaning

AML returns an error code due to :
- Initialisation error : the modules .DLL cannot be loaded or
linked, perhaps due to PATH problems.
- Configuration error : cannot find the robot or drive.
- The robot is not available for the moment.
- Buffer overflow or unknown communication partner.

### Response

Contact the maintenance staff if necessary.

## ROBN006

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN006 ROBOT ERROR, SEE PRECEDING WARNING

### Meaning

AML returns an error code due to :
- Command has been cancelled by AMU.
- Illegal argument.

### Response

Contact the maintenance staff if necessary.

## ROBN007

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN007 ERROR CONDITION CANNOT BE DIAGNOSED

### Meaning

AML returns an error code due to :
- A sequence number has been used twice. Therefore, the second
command cannot be processed.
- The host sent more commands than executable all at once.
- Command cannot be executed in simulation or configuration mode.
- The desired robot is not known to AMU.

### Response

Contact the maintenance staff if necessary.

## ROBN008

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN008 ROBOT EMERGENCY SHUTDOWN

### Response

Contact the maintenance staff if necessary.

## ROBN009

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN009 ROBOT SWITCHED INTO SETUP MODE

### Response

Contact the maintenance staff if necessary.

## ROBN010

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN010 UNKNOWN ROBOT COMMAND

### Meaning

AML returns an error code due to :
- The given message could not be identified. Try to detect,
whether the syntax of the message command was correct.
- Not supported command.
- The host command format was wrong.

### Response

Contact the maintenance staff if necessary.

## ROBN011

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN011 INVALID ASSIGNMENT E.G. ROBOT-VOLSER

### Meaning

AML returns an error code due to :
- Coordinate is out of range.
- The desired coordinate is wrong.
- No robot could be selected. Either there is no robot attached
to the given coordinate(s) or these cannot be handled by the
same robot.

### Response

Contact the maintenance staff if necessary.

## ROBN012

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN012 COMMAND INTERRUPTED BY MANUAL INTERVENTION

### Response

Contact the maintenance staff if necessary.

## ROBN014

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN014 COMMAND INTERRUPTED BY PROGRAM REQUEST

### Meaning

AML returns an error code due to :
- The command in process is being cancelled.
- A currently active mount request in CentricStor
was aborted by a KEEP request.

### Response

Save diagnostic files and contact the maintenance staff if necessary.

## ROBN015

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN015 TOWER HAS NOT TURNED INTO POSITION

### Response

Contact the maintenance staff if necessary.

## ROBN016

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN016 ROBOT HARDWARE ERROR

### Meaning

AML returns an error code due to :
- Gripper problems (position, open/closed).
- Camera or vision system problems.
- Robot coordinate problems (out of range)
- Mismatch between robot entries in archive database and configuration

### Response

Contact the maintenance staff if necessary.

## ROBN017

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN017 COMMAND IS NOT EXECUTABLE

### Meaning

A command sent from ROBAR to the AML system
could not be executed.

### Response

Contact the maintenance staff if necessary.

## ROBN100

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN100 UNEXPECTED ROBOT CRASH

### Response

Contact the maintenance staff if necessary.

## ROBN101

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN101 ROBOT CRASH AT VOLUME REMOVAL/REPLACEMENT

### Meaning

AML returns an error code due to :
Crash sensor.

### Response

Contact the maintenance staff if necessary.

## ROBN102

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN102 TIMEOUT ROBOT

### Meaning

AML returns an error code due to :
Timeout-error with robot/ tower / I/O box control

### Response

Contact the maintenance staff if necessary.

## ROBN103

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN103 TIMEOUT PC-IC COMMUNICATION

### Response

Contact the maintenance staff if necessary.

## ROBN104

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN104 VOLUME LOST

### Meaning

AML returns an error code due to :
- Volume not in gripper.
- Volume lost.

### Response

Contact the maintenance staff if necessary.

## ROBN105

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN105 VOLUME STUCK IN GRAB

### Meaning

AML returns an error code due to :
Volume in gripper.

### Response

Contact the maintenance staff if necessary.

## ROBN110

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN110 CRASH AT TAKING A VOLUME FROM A STORAGE LOCATION

### Response

Contact the maintenance staff if necessary.

## ROBN111

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN111 CRASH AT INSERTING A VOLUME INTO A STORAGE LOCATION

### Response

Contact the maintenance staff if necessary.

## ROBN112

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN112 CRASH AT TAKING A VOLUME FROM A DEVICE

### Response

Contact the maintenance staff if necessary.

## ROBN113

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN113 CRASH AT INSERTING A VOLUME INTO A DEVICE

### Response

Contact the maintenance staff if necessary.

## ROBN201

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN201 UNKNOWN TAPE DEVICE

### Meaning

AML returns an error code due to :
The device is unknown to the archive database.

### Response

Contact the maintenance staff if necessary.

## ROBN202

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN202 DEVICE OCCUPIED (DETECTED BY SOFTWARE)

### Meaning

AML returns an error code due to :
- The requested tape device is not empty (AMU archive database).

### Response

Check the command, make an inventory on the requested
tape device. Contact the maintenance staff if necessary.

## ROBN203

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN203 DEVICE EMPTY (DETECTED BY SOFTWARE)

### Meaning

AML returns an error code due to :
The requested tape device is empty (AMU archive database).

### Response

Check the command, make an inventory on the requested
tape device. Contact the maintenance staff if necessary.

## ROBN204

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN204 DEVICE OCCUPIED (DETECTED BY ROBOT)

### Meaning

AML returns an error code due to :
- The requested device is not empty (detected by robot).

### Response

Check the command, make an inventory on the requested
device. Contact the maintenance staff if necessary.

## ROBN205

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN205 DEVICE EMPTY (DETECTED BY ROBOT)

### Meaning

AML returns an error code due to :
The requested position does not contain a tape (detected by
robot.

### Response

Check the command, make an inventory on the requested
device. Contact the maintenance staff if necessary.

## ROBN206

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN206 VOLUME CANNOT BE REMOVED FROM DEVICE

### Meaning

AML returns an error code due to :
- Requested device is empty.
- Cover of requested device is closed.

### Response

Contact the maintenance staff if necessary.

## ROBN207

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN207 DRIVE DOOR CANNOT BE CLOSED

### Meaning

AML returns an error code due to :
- Cover of requested device is open.
- The device cannot be closed.

### Response

Contact the maintenance staff if necessary.

## ROBN208

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN208 VOLUME CANNOT BE TAKEN FROM STACK

### Meaning

Only involves devices with stacker (3490/3590)

### Response

Contact the maintenance staff if necessary.

## ROBN209

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN209 DEVICE/MEDIUM MISMATCH

### Meaning

AML returns an error code due to a mount request for
a cartridge whose medium type does not match with
the medium type of the device

## ROBN301

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN301 UNKNOWN VOLSER

### Meaning

AML returns an error code due to :
- The given volser could not be found in the database.

### Response

Contact the maintenance staff if necessary.

## ROBN302

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN302 VOLSER NOT IN LIBRARY

### Meaning

AML returns an error code due to :
- The requested position does not contain a volume (archive database).
- The requested source device is empty (archive database).
- The insert array does not contain a volume.
- The requested volume is not in a storage (ejected or mounted ?)
- There was no clean tape found in database.
- In conjunction with CentricStor a logical volume could have been
placed on a physical volume which is not accessible because of
a drive or volume error.

### Response

Contact the maintenance staff if necessary.

## ROBN303

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN303 VOLUME ALREADY MOUNTED ON THIS DEVICE

### Meaning

AML returns an error code because the cartridge is
already mounted on the device.

### Response

ROBAR will check if the tape is inside the device
or only in front of the device.

## ROBN304

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN304 BARCODE LABEL NOT READABLE

### Meaning

AML returns an error code due to :
- Barcode not recognised.
- Illegal barcode.
- Illegal range.

### Response

Contact the maintenance staff if necessary.

## ROBN305

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN305 NO BARCODE LABEL DETECTED OR NOT FOUND IN STORAGE POSITION

### Meaning

AML returns an error code due to :
- Volume barcode label not recognised.
- The currently running insertion of volume is finished.
There wasn't found any volume in insert positions.

### Response

Check the logfile for further information.

## ROBN306

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN306 WRONG VOLSER ON SPECIFIED COORDINATE

### Meaning

AML returns an error code due to :
- Illegal barcode.
- Inconsistency during inventory detected.

### Response

Make an update to the archive database.
Contact the maintenance staff if necessary.

## ROBN307

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN307 KEEP WAS SUCCESSFUL BUT A WRONG VOLSER WAS IN THE DEVICE

## ROBN308

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN308 VOLUME EJECTED

### Meaning

AML returns an error code because the cartridge to
be mounted has been ejected in the I/O box of the
robot system.

## ROBN309

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN309 VOLUME ALREADY MOUNTED ON A DIFFERENT DEVICE

### Meaning

AML returns an error code because the cartridge is
already mounted on another device.

## ROBN401

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN401 COORDINATE NOT DEFINED

### Meaning

AML returns an error code due to :
The given position could not be found in database.

### Response

Contact the maintenance staff if necessary.

## ROBN402

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN402 NO VOLSER ON SPECIFIED COORDINATE

### Meaning

AML returns an error code due to :
Requested position is empty.

### Response

Contact the maintenance staff if necessary.

## ROBN403

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN403 COORDINATE SLOT NOT EMPTY

### Meaning

AML returns an error code due to :
- The requested position is not empty (archive database).
- The requested target device is not empty (archive database).

### Response

Contact the maintenance staff if necessary.

## ROBN404

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN404 COORDINATE/MEDIUM MISMATCH

### Meaning

AML returns an error code due to a request for a
cartridge whose medium type does not match with
the medium type of the specified coordinate.

## ROBN405

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN405 NO MORE DYNAMIC POSITION IN THE ARCHIVE

### Meaning

AML returns an error code because there is no more
free dynamic position in the robot system.

### Response

Free place or add new dynamic positions in the
robot system.

## ROBN408

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN408 GRIPPER ERROR, CARTRIDGE MAY HAVE BEEN DROPPED

## ROBN501

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN501 DOOR OF I/O-UNIT NOT CLOSED

### Response

Contact the maintenance staff if necessary.

## ROBN502

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN502 I/O-AREA DEFINITIONS DO NOT MATCH

## ROBN503

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN503 EJECT DEVICE OVERRUN

### Meaning

AML returns an error code due to :
There is no free eject position in I/O box.

### Response

Empty the I/O box. Try the command later.

## ROBN504

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN504 VOLUME PUT INTO WASTE BOX

### Meaning

AML returns an error code due to :
- The tape was moved to the problem box because of a severe error.
In case of CentricStor:
- The order cannot be executed because of file system error.

### Response

Contact the maintenance staff if necessary.

## ROBN505

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN505 VOLUME IN WASTE BOX NOW OCCUPIED

### Response

Contact the maintenance staff if necessary.

## ROBN507

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN507 COMMAND ABORTED. PROBLEMBOX FULL

## ROBN700

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN700 NO CLEANING CARTRIDGES AVAILABLE

## ROBN701

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN701 CLEAN POOL DOES NOT EXIST

## ROBN900

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN900 AML COMMAND REJECTED

## ROBN901

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN901 NO FREE STORAGE SLOT IN LIBRARY SYSTEM FOR IMPORT

### Meaning

IMPORT cannot be started or continued because all
storage slots in the library system are occupied.

## ROBN902

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN902 VOLUME TO BE EJECTED ALREADY EJECTED

## ROBN903

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN903 VSN TO BE IMPORTED ALREADY EXISTS IN LIBRARY SYSTEM

### Meaning

One of the volumes to be imported is labeled a volser,
which already exists in the library system.
This volume was not imported.

## ROBN904

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROBN904 COMMUNICATION BETWEEN ROBAR-SV AND AML FAILED

### Meaning

From ROBAR point of view the communication to a library
system with SCSI interface has failed. Possible reasons:
Problem in the library (e.g. Scalar i2000).
I/O blade failure.
Problems with the fibre channel path (e.g. switch).
Problems with the HBA of the ROBAR-SV host.

### Response

If the problem cannot be solved contact the maintenance.
If the failure persists ROBAR-SV stops.

## ROB0SAT

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB0SAT FROM ROBAR VIEW TAPE CARTRIDGE mmmm DEVICE IS ATTACHED

### Meaning

When restarting, ROBAR requests the device status of the hosts
it is connected to. ROBAR sends an information message
when it considers a device to be attached to a BS2000 host.
Additional information:
- mmmm: device mnemonic

## ROB0SER

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB0SER INCONSISTENCY IN AML DATABASE FOR DEVICE mmmm

### Meaning

When restarting, ROBAR reports that BS2000 has found
a cartridge in the device, but the AML database
indicates that the device is empty.
Additional information:
- mmmm: device mnemonic

### Response

Correct the AML database or contact the maintenance.

## ROB0SKE

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB0SKE REMOVING TAPE CARTRIDGE FROM DEVICE mmmm

### Meaning

When restarting, ROBAR has detected that a cartridge has to be
removed from the mentioned device.
Additional information:
- mmmm: device mnemonic

## ROB0009

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0009 HOST UNKNOWN:

### Meaning

The configuration file and the parameter file do not match.
Generate a new configuration file.

## ROB0010

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0010 NO RESPONSE FROM AML FOR:

### Meaning

AML has not sent a response within a certain time
(ROBAR_WAIT). Processing of the job by ROBAR is aborted.
Check whether the input/output window is open or whether
the robot is no longer operable.

## ROB0011

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0011 MESSAGE CODE NOT FOUND IN MESSAGE_FILE:

### Meaning

Error in the file message_file. Check message_file.

## ROB0012

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0012 MESSAGE CODE NOT FOUND IN MESSAGE_XREF:

### Meaning

Error in the file message_xref. Check message_xref.

## ROB0013

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0013 MESSAGE CODE NOT FOUND IN ROBOTER_CMDS:

### Meaning

Error in the file roboter_cmds. Check roboter_cmds.

## ROB0014

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0014 ERROR IN COMMAND FILE:

### Meaning

Error in the file roboter_cmds. Check roboter_cmds.

## ROB0015

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0015 MESSAGE CODE NOT FOUND IN MESSAGE_RESP:

### Meaning

Error in the file message_resp. Check message_resp.

## ROB0016

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0016 Internal error detected in ROBAR-SV at (&00)

### Meaning

ROBAR-SV has reported an internal error.
Diagnosis information is written into ROBAR-SV logging.
(&00): date and time of the error

## ROB0018

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0018 INVALID MESSAGE CODE IN MESSAGE_XREF:

### Meaning

The file message_xref contains an error. Check message_xref.

## ROB0020

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0020 NO DEVICE FREE

### Meaning

The mount job could not be performed as no drive is free.
The job is suspended if the appropriate specification was
made in the action list (REPEAT).

## ROB0021

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0021 DEVICE UNKNOWN:

### Meaning

The drive is not specified in the configuration file.
Modify the configuration file.

## ROB0023

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0023 CONNECTION TO HOST SEVERED:

### Meaning

The connection to the specified BS2000 system has been
severed.

## ROB0024

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0024 ROBAR FREEPOOL NOT CREATED

### Meaning

The specified freepool does not exist. Create the freepool.

## ROB0027

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0027 ROBAR FREEPOOL IS EMPTY

### Meaning

The freepool is empty. Extend the freepool.

## ROB0028

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0028 FREEPOOL MINIMUM (MIN_SCRATCH) VIOLATED

### Meaning

The freepool contains fewer volume serial numbers than are
specified in the MIN_SCRATCH variable. Extend the freepool.

## ROB0029

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0029 ERROR IN DECLARE STATEMENT:

### Meaning

An invalid keyword has been specified in DECLARE statement.
Correct the DECLARE statement in message_resp

## ROB0030

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0030 DOOR OF I/O UNIT OPEN --> PLEASE CLOSE THE DOOR

### Meaning

No cartridge can be ejected anymore.

### Response

Close the door of the I/O box
and notify ROBAR after closing by means of the command
/INFORM-OPERATOR MESSAGE='<T I/O-BOX EMPTY'
or by the activation of the function that automatically
restarts the EJECT after an HICAP door has been closed
(this function has to be activated in the MRV30 option
of the file message_resp of ROBAR-SV).

## ROB0031

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0031 ROBAR STOPPED

### Meaning

The ROBAR system has been terminated.

## ROB0032

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0032 CONFIRM EXECUTION (<CR>/N)

### Meaning

This error only occurs in conjunction with simulation.

## ROB0033

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0033 EXECUTED

### Meaning

This error only occurs in conjunction with simulation.

## ROB0034

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0034 NOT EXECUTED

### Meaning

This error only occurs in conjunction with simulation.

## ROB0035

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0035 I/O UNIT FULL --> PLEASE REMOVE CARTRIDGES

### Meaning

No cartridge can be ejected anymore.

### Response

Remove the cartridges from the I/O box
and notify ROBAR when it is empty by means of the command
/INFORM-OPERATOR MESSAGE='<T I/O-BOX EMPTY'
or by the activation of the function that automatically
restarts the EJECT after a HICAP door has been closed
(this function has to be activated in the MRV30 option
of the file message_resp of ROBAR-SV).

## ROB0036

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0036 ERROR DETECTED DURING CLEANING ! DEV =

### Meaning

An error has occurred while cleaning the specified drive.
Check the return code of the AML system.

## ROB0037

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0037 INSERT COMMAND EXECUTED

## ROB0038

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0038 ILLEGAL KEYWORD:

### Meaning

The keyword defined in message_resp is not known in ROBAR.
Correct the file message_resp.

## ROB0039

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0039 CLEAN CARTRIDGE EJECTED --> PLEASE INSERT NEW ONE

## ROB0040

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0040 PROBLEM BOX FULL --> PLEASE REMOVE CARTRIDGES

## ROB0042

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0042 ROBOT STATE CHANGED TO >OFF< : (&00)

## ROB0043

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0043 ROBOT STATE CHANGED TO >ON< : (&00)

## ROB0044

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0044 AMU STATE IS >PASSIVE<

## ROB0045

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0045 AMU STATE IS >ACTIVE<

## ROB0048

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB0048 HOST NOT AUTHORIZED TO USE THIS VSN: (&00)

### Meaning

The format of (&00) is: vvvvvv,PARTNER=pppppppp,LOCATON=llllllll.
vvvvvv : VSN
pppppppp: TNS partner name
llllllll: location of the robot system.
A request received from ROBAR-CL with the TNS partner name pppppppp
is not authorized to use the cartridge vvvvvv in the configured
environment.
This message is issued only if vvvvvv is known in ROBAR_ARCHIV.

### Response

Check ROBAR_ARCHIV and the section gen_hosts_vsn in the
configuration file of ROBAR-SV. Change if necessary.

## ROB1000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1000 USER ID HAS NO PRIVILEGE FOR TAPE ADMINISTRATION

### Meaning

System privilege for tape administration is mandatory
for the desired function.

### Response

Contact the system administrator.

## ROB1010

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1010 CREATE-ROBAR-FREEPOOL POOL=(&00),VOLUME=(&01)

### Meaning

Creation of a ROBAR freepool.
(&00) : type of freepool (*STD or *TSN)
(&01) : VSN of the tape cartridge

## ROB1011

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1011 CREATE-ROBAR-FREEPOOL POOL=(&00),VOLUME=*INTERVAL((&01),(&02))

### Meaning

Creation of a ROBAR freepool.
(&00) : type of freepool (*STD or *TSN)
(&01) : first VSN of the interval
(&02) : last VSN of the interval

## ROB1013

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1013 ADD-ROBAR-VOLUME STATE=(&00),VOLUME=(&01),POSITION=(&02),ROB=(&03)

### Meaning

Declaration of a foreign tape cartridge.
(&00) : classification (FOREIGN)
(&01) : VSN of the tape cartridge
(&02) : location of the tape cartridge (<integer 3..3>)
(&03) : robot system (1 or 2)

## ROB1019

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB1019 END-ROBAR-FREEPOOL

### Meaning

Internal termination message.

## ROB1020

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1020 DELETE-ROBAR-FREEPOOL POOL=(&00)

### Meaning

Deletion of a ROBAR freepool.
(&00) : type of freepool (TSN)

## ROB1021

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1021 REMOVE-ROBAR-VOLUME STATE=(&00),VOLUME=(&01),LOCATION=(&02)

### Meaning

Removal of a foreign tape cartridge.
(&00) : classification (FOREIGN)
(&01) : VSN of the tape cartridge
(&02) : location of the tape cartridge to be removed

## ROB1030

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1030 EXPORT-ROBAR-VOLUME VOLUME=(&00),ROB=(&01),LOCATION=(&02)

### Meaning

Export of a tape cartridge.
(&00) : VSN of the tape cartridge
(&01) : robot (1 or 2)
(&02) : location of the tape cartridge to be ejected

## ROB1031

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1031 EXPORT-ROBAR-VOLUME KEEP-POSITION=*NO,VOLUME=(&00),ROB=(&01),LOCATION=(&02)

### Meaning

Export of a tape cartridge.
(&00) : VSN of the tape cartridge
(&01) : robot (1 or 2)
(&02) : location of tape cartridge to be ejected

## ROB1040

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1040 IMPORT-ROBAR-VOLUME STATE=(&00),ROB=(&01),LOCATION=(&02)

### Meaning

Import of a tape cartridge
(&00) : classification (OWN)
(&01) : robot (1 or 2)
(&02) : location of tape cartridge to be imported

## ROB1050

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

ROB1050 SHOW-ROBAR-VOLUME VOLUME=(&00),POSITION=(&01),LOCATION=(&02),ELEMENT=(&03)

### Meaning

Show of FOREIGN definition in ROBAR-SV
(&00) : requested VSN or *ALL
(&01) : requested foreign position (*FRnnn) or *ALL
(&02) : location or *ANY
(&03) : sequence number of element in case of list

## ROB1100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1100 ROBAR-CL VERSION (&00) READY

## ROB1105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1105 ERROR WHEN READING STATEMENT (CODE: '(&00)')

### Meaning

(&00): content of the register 15 when returning
from the call to RDSTMT interface.
ROBAR cannot handle any special action for this return code.

### Response

- Look for a previous SDF message (CMDnnnn) that explains the error.
- Correct and retry.

## ROB1110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1110 COMMAND ACCEPTED

### Meaning

The specified ROBAR command has been read, checked and accepted.

## ROB1111

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1111 END OF FOREIGN VOLUME DEFINITION FOR SELECTION=(&00) AND LOCATION=(&01)

## ROB1112

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1112 NO FOREIGN VOLUME DEFINITION EXISTS FOR SELECTION=(&00) AND LOCATION=(&01)

## ROB1113

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1113 NO ROBAR_FOREIGN DEFINED IN ROBAR-SV. REQUESTED INFORMATION NOT AVAILABLE

### Meaning

Possible reason: SCSI interface.
Foreign volumes are not supported in ROBAR-SV for SCSI interface.

## ROB1114

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1114 ERROR IN FOREIGN DEFINITIONS. REQUESTED INFORMATION NOT AVAILABLE

## ROB1115

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1115 INVALID COMMAND - PLEASE RETRY

### Meaning

The specified command is invalid or illegal.

### Response

Check the command and enter it again.

## ROB1116

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1116 INVALID RESPONSE

### Meaning

The response to the ROBAR message is invalid.

### Response

Please do not manually respond to it.

## ROB1120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1120 ROBAR MESSAGE COULD NOT BE ISSUED

### Meaning

An error has occurred in the MSG7 macro.

### Response

Prepare the necessary documents for diagnosis.

## ROB1121

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1121 ROBAR COULD NOT WRITE ON SYSOUT

### Meaning

An error has occurred in the WROUT macro.

### Response

Prepare the necessary documents for diagnosis.

## ROB1122

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1122 ROBAR COULD NOT WRITE ON SYSLST01

### Meaning

An error has occurred in the WRLST macro.

### Response

Prepare the necessary documents for diagnosis.

## ROB1125

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1125 ROBAR DOES NOT EXIST IN YOUR ACTIVATED SYNTAX FILES

### Meaning

The ROBAR program is not known in the currently activated syntax files
as a collective term for all possible command inputs.

### Response

Check the activated syntax files for the existence of the ROBAR
program. If necessary, merge the supplied syntax files again.

## ROB1130

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1130 REQUESTED FILE IS EMPTY

### Meaning

The specified file, which should contain the freepool specifications, is
empty.

### Response

Recreate the file with the freepool specifications.

## ROB1135

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1135 REQUESTED FILE IS PASSWORD-PROTECTED (READPASS)

### Meaning

The file containing the freepool specifications is protected
by a read password.

### Response

Either enter the required password or lift the password protection
before issuing the command.

## ROB1140

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1140 OPEN ERROR

### Meaning

The specified file could not be opened.

### Response

Check the file access rights.

## ROB1145

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1145 REQUESTED FILE IS NOT PRESENT

### Meaning

The specified file does not exist.

### Response

Create a file with the freepool specifications.

## ROB1150

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1150 REQUESTED FILE IS NOT SHAREABLE

### Meaning

The requested file is not shareable.

### Response

Make the file shareable.

## ROB1155

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1155 FSTAT MACRO EXECUTED WITH ERRORS

### Meaning

An error occurred during executing of the FSTAT macro.

### Response

Prepare the necessary documents for diagnosis.

## ROB1160

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1160 FILE MACRO EXECUTED WITH ERRORS

### Meaning

An error occurred during executing of the FILE macro.

### Response

Prepare the necessary documents for diagnosis.

## ROB1165

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1165 USER ERROR

### Meaning

Control has branched to the USERERR exit of the file containing
the freepool specifications.

### Response

Check the file and prepare the necessary documents for diagnosis.

## ROB1170

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1170 VOLUME SERIAL NUMBERS HAVE DIFFERENT LENGTHS

### Meaning

The VSN specifications have different lengths.

### Response

Correct the VSN specifications so that they all have the same length.

## ROB1175

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1175 ALPHANUMERIC VSN SPECIFICATIONS ARE INCONSISTENT

### Meaning

The VSN specifications have different alphanumeric identifiers.

### Response

Correct the VSN specifications so that they have the same identifiers.

## ROB1180

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1180 FIRST VSN IS SAME AS SECOND VSN

### Meaning

Two identical VSN's have been entered for the range specification.

### Response

Correct the VSN entries so that they are not identical.

## ROB1185

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1185 FIRST VSN IS GREATER THAN SECOND VSN

### Meaning

The range specifications are not in ascending order.

### Response

Correct the VSN specifications so that they are in ascending order.

## ROB1190

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1190 PLEASE SPECIFY EXPORT-ROBAR-VOLUME COMMAND FOR EACH VSN OF THIS TYPE

### Meaning

It is not possible to specify a range of EXPORT-ROBAR-VOLUME
commands for VSN's of the type G01A01 (alphanumeric identifier
not only at the beginning or end of the VSN).

### Response

Enter the EXPORT-ROBAR-VOLUME commands individually.

## ROB1195

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1195 POSITION OPERAND MUST CONTAIN 3 CHARACTERS

### Meaning

The position specification in the output chute must contain 3 characters.

### Response

Correct the position specification.

## ROB1200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1200 ROBAR TERMINATED

## ROB1205

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1205 ROBAR TERMINATED WITH ERRORS

### Response

Prepare the necessary documents for diagnosis.

## ROB1500

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1500 A REFERENCE HAS BEEN CREATED TO THE FOREIGN TAPE CARTRIDGE

## ROB1505

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1505 FOREIGN FILE ALREADY EXISTS

## ROB1506

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1506 VSN OR POSITION INVALID OR ALREADY DEFINED

### Meaning

Either the given POSITION is not defined in the
file ROBAR_FOREIGN or the given VSN or POSITION
is already used by a previous FOREIGN definition.
Foreign volumes and freepools are not supported in
ROBAR-SV for SCSI interface.

### Response

Check the actual content of the FOREIGN definitions
by means of the command //SHOW-ROBAR-VOLUME
and retry with correct definition.

## ROB1507

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1507 FOREIGN POSITION IS NOT UNIQUE

## ROB1510

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1510 NO REFERENCE HAS BEEN CREATED TO FOREIGN TAPE CARTRIDGE

## ROB1520

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1520 FOREIGN VSN '(&00)' RELEASED

## ROB1525

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1525 CANNOT REMOVE FOREIGN DEFINITION (&00)

### Meaning

Possible reasons:
- The specified volume does not exist in foreign definitions.
- The specified volume is mounted.

## ROB1526

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1526 ROBAR-SV ERROR DURING REMOVAL OF FOREIGN DEFINITION OR WRONG LOCATION SPECIFIED

### Meaning

Possible reasons:
- The specified LOCATION is wrong or rejected by ROBAR-SV
- The specified foreign definition cannot be removed by ROBAR-SV
Foreign volumes and freepools are not supported in
ROBAR-SV for SCSI interface.

### Response

Check the foreign definitions with //SHOW-ROBAR-VOLUME

## ROB1530

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1530 FOREIGN VSN '(&00)' NOT RELEASED

## ROB1540

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1540 IMPORT OPERATION STARTED

## ROB1550

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1550 IMPORT OPERATION NOT STARTED OR NOT COMPLETELY PROCESSED

## ROB1560

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1560 VSN '(&00)' EXPORTED

## ROB1565

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1565 ERROR AT MAREN SUBROUTINE CALL (VSN=(&00), RC=(&01))

### Meaning

(&00): VSN of the tape cartridge
(&01): return code from MAREN. Possible values:
D : DMS error
I : Not allowed at the moment (for example,
because the imported volume is not yet declared
in the MAREN catalog)
M : MAREN internal error
N : Volume not found
O : Offline operation: only logging is activated.
The operation is not really registered in the
MAREN catalog
P : Concurrent access to the volume in the
MAREN catalog
T : Volume still allocated by another task
X : Request rejected by MAREN administrator
(MAREN exit routine)
0 : Operator reply: EXIT
1 : Operator reply: RETRY
2 : Operator reply: CONTINUE

## ROB1570

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1570 VSN '(&00)' NOT EXPORTED

## ROB1580

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1580 EXPORT OPERATION ABORTED OR WRONG LOCATION SPECIFIED

## ROB1590

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1590 VSN '(&00)' ADDED TO FREEPOOL

## ROB1593

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1593 INCONSISTENCY DETECTED WHEN CREATING THE FREEPOOL

## ROB1594

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1594 SYNTAX ERROR IN VSN SPECIFICATION

## ROB1595

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1595 VSN '(&00)' IS NOT UNIQUE IN THE FREEPOOL

## ROB1596

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1596 VSN '(&00)' IS NOT KNOWN IN ROBAR_ARCHIV

## ROB1599

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1599 ERROR IN OPENING FREEPOOL FILE

## ROB1600

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1600 FREEPOOL NOT CREATED

## ROB1605

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1605 FREEPOOL CREATED

## ROB1610

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1610 TSN FREEPOOL DELETED

## ROB1620

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1620 CANNOT DELETE TSN FREEPOOL

## ROB1630

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1630 TSN FREEPOOL WAS NOT CREATED

## ROB1640

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB1640 INCONSISTENCY DETECTED WHEN DELETING THE TSN FREEPOOL

## ROB2000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2000 ROBAR CONNECTION STARTED

### Meaning

Connection to ROBAR-SV has been established.

## ROB2001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2001 ROBAR CONNECTION CLOSED

### Meaning

Connection to ROBAR-SV has been severed.

## ROB2005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2005 FILE (&00).TEXT MISSING

### Meaning

(&00): Prefix of TEXT file

## ROB2010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2010 APPLICATION (&00) COULD NOT BE OPENED (RC=(&01))

### Meaning

The $CONSOLE interface is locked for this application.
(&00): application name
(&01): DCAM return code

## ROB2020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2020 CONNECTION TO ROBAR-SV COULD NOT BE SET UP (RC=(&00))

### Meaning

(&00): DCAM return code

## ROB2030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2030 CONNECTION ATTEMPT FROM WRONG STATION: (&00)/(&01)

### Meaning

(&00): station name
(&01): processor name

## ROB2040

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2040 ERROR IN PASSWORD FROM ROBAR-SV

## ROB2050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2050 ERROR DURING SENDING A MESSAGE (RC=(&00))

### Meaning

(&00): DCAM return code

## ROB2051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2051 ERROR DURING PICKING UP A MESSAGE (RC=(&00))

### Meaning

(&00): DCAM return code

## ROB2052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2052 CONNECTION TO ROBAR-SV COULD NOT BE TORN DOWN (RC=(&00))

### Meaning

ROBAR-CL has received the negative return code (&00) from DCAM.
The connection to ROBAR-SV will NOT be reestablished automatically.

### Response

The system administrator should solve the DCAM problem.
Then ROBAR-CL can be stopped and restarted.

## ROB2100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2100 ROBAR-CL-DCAM (&00) READY

## ROB2110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2110 CONNECTION SET UP ( ROBAR-SV ) CPUS=(&00) (&01) STATION: (&02)/(&03)

## ROB2120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2120 CONNECTION SET UP (UCON: (&00) ) (&01)

## ROB2130

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2130 CONNECTION CLEARED DOWN ( ROBAR-SV ) (&00)

## ROB2140

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2140 CONNECTION CLEARED DOWN (UCON) (&00)

## ROB2200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2200 PARAMETER ERROR

## ROB2210

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2210 -C=(&00) IS NOT FOUR CHARACTERS LONG

### Meaning

(&00): name of $CONSOLE application

## ROB2220

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2220 CONNECTION TO $CONSOLE COULD NOT BE SET UP (RC=(&00))

### Meaning

(&00): DCAM return code

## ROB2225

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2225 CONNECTION TO $CONSOLE VIA DYNAMIC AUTHORISATION NAME REJECTED

### Meaning

possible reasons:
- password for Operator-Id (TSOS) invalid or missing
- connection to UCON severed

### Response

check password for Operator-Id, restart ROBAR-CL

## ROB2226

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2226 REQ-OPERATOR-ROLE REJECTED BY NBR0984. REASON: (&00)

### Meaning

For further informations enter /HELP-MSG NBR0984.
Invalid combination of parameters OPEROLE (operator role)
and OPERID (operator identifier). ROBAR-CL is terminated.

### Response

Change parameters OPERID and/or OPEROLE in ROBAR-CL start procedure

## ROB2230

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2230 JOB VARIABLE >(&00)< UNKNOWN OR JV SOFTWARE NOT INSTALLED

## ROB2240

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2240 PROGRAM CANNOT BE STARTED IN BS2000 V9.5

## ROB2250

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2250 ERROR AT MAREN CALL FOR VSN (&01): RETURN CODE = >(&00)<

### Meaning

(&00): return code from MAREN. Possible values:
D : DMS error
I : Not allowed at the moment (for example,
because the imported volume is not declared
in the MAREN catalog yet)
M : MAREN internal error
N : Volume not found
O : Offline operation: only logging is activated.
The operation is not really registered in the MAREN catalog
P : Concurrent access to the volume in the MAREN catalog
T : Volume still allocated by another task
X : Request rejected by MAREN administrator (MAREN exit routine)
0 : Operator reply: EXIT
1 : Operator reply: RETRY
2 : Operator reply: CONTINUE
(&01): VSN of the tape cartridge
The next ROBAR message also gives a MAREN message number
that explains the cause of the error

## ROB2260

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2260 MAREN MESSAGE NUMBER: >(&00)<

## ROB2270

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2270 FILE >(&00)< CANNOT BE OPENED

## ROB2280

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2280 GET-TIME RETURNS VALUE 0. ROBAR-CL CANNOT BE STARTED

### Meaning

The time returned by CRTE is not correct so that
ROBAR cannot properly run.

### Response

Check the load address of GET-TIME subsystem.

## ROB2290

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ROB2290 ERROR IN FILE >(&00)< FOR >(&01)<

## ROB4001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4001 THE DEVICE IS IN NOT-READY STATUS (DEV=mmmm)

### Meaning

The possible reasons are:
1. The device is not installed.
2. The device is not on-line.
3. No cartridge is loaded.
4. The READY/NOT-READY switch of the device has been set to NOT-READY.
5. The device is not functional.
6. The device is performing a REWIND-UNLOAD operation.
Additional information:
- mmmm: device mnemonic

### Response

Check the READY/NOT-READY switch of the device.
If the problem cannot be solved, contact the maintenance.

## ROB4002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4002 THE POSITION OF THE TAPE DURING OPERATION IS NOT KNOWN ANYMORE (DEV=mmmm / TSN=tttt / VSN=vvvvvv)

### Meaning

ROBAR has cancelled the remounting of the tape and the current I/O is
terminated with error.
Additional information:
- mmmm: device mnemonic
- tttt: Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Check the cause for the loss of position.

## ROB4004

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4004 TAPE CARTRIDGE DEVICE UNLOADED (DEV=mmmm / VSN=vvvvvv)

### Meaning

The AML system has moved the cartridge from the device to its
home place in the archive.
Additional information:
- mmmm: device mnemonic
- vvvvvv: Volume Serial Number

## ROB4005

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4005 TAPE CARTRIDGE DEVICE UNLOADED (DEV=mmmm)

### Meaning

The AML system has moved a cartridge from the device
to its home place in the archive.
Additional information:
- mmmm: device mnemonic

## ROB4006

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4006 TAPE CARTRIDGE DEVICE NOT UNLOADED (DEV=mmmm / ffff)

### Meaning

The AML system could not move the cartridge from the device
to its home place in the archive.
Additional information:
- mmmm: device mnemonic
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)

## ROB4008

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4008 TAPE CARTRIDGE MOUNTED (DEV=mmmm / TSN=tttt / VSN=vvvvvv)

### Meaning

Additional information:
- mmmm : device mnemonic
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

## ROB4010

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4010 VOLUME ALLOCATED FROM ROBAR FREE-POOL (VSN=vvvvvv / TSN=tttt)

### Meaning

Additional information:
- vvvvvv: Volume Serial Number
- tttt : Task Serial Number

## ROB4011

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4011 ROBAR FREEPOOL IS EMPTY. REQUEST REJECTED (TSN=tttt)

### Meaning

The freepool is empty. Extend the freepool.
Additional information:
- tttt: Task Serial Number

## ROB4014

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4014 TAPE CARTRIDGE DEVICE IS UNEXPECTEDLY EMPTY (TSN=tttt / ffff)

### Meaning

The AML system has returned an error code according to which
the concerned device is unexpectedly empty.
Additional information:
- tttt: Task Serial Number
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)

### Response

Check a possible inconsistency between the real device
status and the AML system data base. In case of
inconsistency, correct the data base.

## ROB4018

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4018 TAPE CARTRIDGE DEVICE CLEANED (DEV=mmmm)

### Meaning

The device has been cleaned.
Additional information:
- mmmm: device mnemonic

## ROB4019

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4019 TAPE CARTRIDGE DEVICE CLEANING WILL BE STARTED (DEV=mmmm)

### Meaning

The device will be cleaned.
Additional information:
- mmmm: device mnemonic

## ROB4020

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4020 TAPE CARTRIDGE DEVICE CLEANING FAILED (DEV=mmmm)

### Meaning

The device cleaning has failed.
Additional information:
- mmmm: device mnemonic

### Response

Check the problem with the device (see previous messages).
Check the cleaning information on the robot.

## ROB4021

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4021 NEW CLEANING CARTRIDGES REQUIRED (CLEANPOOL=aaa)

### Meaning

New cleaning cartridges are required for the specified cleanpool.
Additional information:
- aaa: cleanpool

### Response

Insert new cleaning cartridges for the specified cleanpool.

## ROB4022

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4022 NO CLEANING CARTRIDGE AVAILABLE (DEV=mmmm)

### Meaning

No cleaning cartridges are available for the device.
Additional information:
- mmmm: device mnemonic

### Response

Insert cleaning cartridges into the I/O box.

## ROB4024

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4024 THE DEVICE IS UNEXPECTEDLY IN OFFLINE STATUS (DEV=mmmm)

### Meaning

The possible reasons are:
1. The device is not powered.
2. The ONLINE/OFFLINE switch of the device has been pressed.
3. Hardware malfunction of the device.
4. Incompatibility between the device and the control unit.
Additional information:
- mmmm: device mnemonic

### Response

Check the ONLINE/OFFLINE switch and the power of the device.
If the problem cannot be solved, contact the maintenance.

## ROB4028

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4028 AUTOMATIC INVENTORY COMPLETED (LOCATION=llllllll / I/O-UNIT=aaa-bb)

### Meaning

Automatic inventory completed after Hicap access.
Inventoried volumes are now available for mounting.
Additional information:
- llllllll : LOCATION
- aaa-bb : I/O box identification

## ROB4034

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4034 VOLUME ALREADY MOUNTED (DEV=mmmm / TSN=tttt / VSN=vvvvvv)

### Meaning

The volume is already mounted. ROBAR rejects the mount request.
Additional information:
- mmmm : device mnemonic
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

## ROB4036

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4036 MOUNT FOR NON-ASSIGNED DEVICE (DEV=mmmm)

### Meaning

ROBAR has detected that the requested device is not assigned
and has redirected the mount request to another device by
means of a /CHANGE-TAPE-MOUNT ACTION=*MOVE command.
Additional information:
- mmmm: device mnemonic

## ROB4038

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4038 HARDWARE ERROR ON DEVICE CONTROLLER

### Meaning

A previous BS2000 error message reported a hardware error.
If no alternative path is possible, ROBAR detaches the device.
Additional information:
- mmmm: device mnemonic

### Response

Check the connection between the device and its controller.
If the problem cannot be solved, contact the maintenance.

## ROB4040

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4040 BECAUSE OF A /SECURE-RESOURCE-ALLOCATION NO /CHANGE-TAPE-MOUNT IS ALLOWED (DEV=mmmm / VSN=vvvvvv)

### Meaning

To bypass a problem with a device, ROBAR has issued a
/CHANGE-TAPE-MOUNT command.
But a previous /SECURE-RESOURCE-ALLOCATION prevents the usage
of another device and the request remains pending.
Additional information:
- mmmm : device mnemonic
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Check the problem with the device (see previous messages).
- If it can be solved, REMOUNT the cartridge.
- If it cannot be solved, reject the MOUNT request.

## ROB4045

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4045 NO FREE STORAGE PLACE IN ARCHIVE FOR IMPORT

### Meaning

IMPORT cannot be started or continued because all storage places in
the archive are occupied.

## ROB4046

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4046 VSN OF VOLUME TO BE IMPORTED ALREADY EXISTS IN ARCHIVE

### Meaning

One of the volumes to be imported is labeled a volser, which already
exists in the archive. This volume was not imported.

## ROB4047

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4047 EXPIRED CLEANING CARTRIDGE EJECTED. INSERT NEW ONE

### Meaning

An expired cleaning cartridge has been ejected and should be replaced
by a new one.

## ROB4050

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4050 HICAP REQUEST BY OPERATOR (LOCATION=llllllll / I/O-UNIT=aaa)

### Meaning

An Hicap request has been initiated .
Further robot requests will be stacked until the robot will be
available again.
Additional information:
- llllllll : LOCATION of the ROBOT
- aaa : I/O box identification

## ROB4051

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4051 EIF OR HICAP OPENED BY OPERATOR (LOCATION=llllllll / I/O-UNIT=aaa-bb)

### Meaning

Additional information:
- llllllll : LOCATION of the ROBOT
- aaa-bb : I/O box identification

## ROB4052

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4052 HICAP CAN NOW BE OPENED BY OPERATOR (LOCATION=llllllll)

### Meaning

Additional information:
- llllllll : LOCATION of the ROBOT

## ROB4054

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4054 ROBOT AVAILABLE AGAIN AFTER HICAP REQUEST (LOCATION=llllllll)

### Meaning

A Hicap request has been completed.
The robot is available again.
Additional information:
- llllllll : LOCATION of the ROBOT

## ROB4060

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4060 AMU SWITCHING STARTED - ROBAR_RESTART INITIATED

### Meaning

An AMU switching is currently in progress.
ROBAR-SV is now trying to restart the connection with the new AMU.

## ROB4064

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4064 SWITCHING FAILED - NO AMU TO AMU COMMUNICATION

### Meaning

Communication to the other AMU could not be established.
The previous AMU remains active.
The switching operation terminates.

### Response

Check the error cause of the AML system.
If the problem cannot be solved, contact the maintenance.

## ROB4068

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4068 ADS SWITCHING FAILED

### Meaning

An error occurred during a switch operation of the ADS.
The switching operation cannot be executed and terminates.
The previously active AMU remains active.

### Response

Check the error cause of the AML system.
If the problem cannot be solved, contact the maintenance.

## ROB4070

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4070 WARNING : DEVICE NOT READY (DEVICE = hhh)

### Meaning

The switching operation for the ADS succeeded,
but the hardware check reported following error:
One or more devices are not ready.
The device that did not report a ready state requires activation.
Additional information:
hhh : device identification in the AML

## ROB4074

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4074 AMU SWITCHING COMPLETED

### Meaning

The switching operation completed. The ADS was switched
successfully and a hardware check was issued.

## ROB4078

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4078 CONNECTION TO AML SYSTEM LOST - RESTART OPTION SET

### Meaning

The connection to the AML system has been lost.
For ROBAR-SV the automatic restart has been activated by
SET_RESTART_OPTION YES.
ROBAR-SV will be stopped and restarted.
The restart can only be successful, if the connection to the AML system
can be reestablished.
If an alternative AMU address is defined in the current configuration,
this address will be used for restart.

## ROB4079

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4079 CONNECTION TO AML SYSTEM LOST - RESTART OPTION NOT SET

### Meaning

The connection to the AML system has been lost.
For ROBAR-SV the automatic restart has been deactivated by
SET_RESTART_OPTION NO.
ROBAR-SV will be stopped.

## ROB4080

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4080 AMU TO AMU COMMUNICATION LOST

### Meaning

The communication path between the two AMU is interrupted.
The databases cannot be synchronised.

### Response

Check the communication path between the two AMU.
If the problem cannot be solved, contact the maintenance.

## ROB4084

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4084 AMU TO AMU COMMUNICATION ESTABLISHED

### Meaning

Interrupted communication path between the two AMU is operable again.

## ROB4090

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB4090 COMMUNICATION BETWEEN ROBAR-SV AND AML FAILED

### Meaning

From ROBAR point of view the communication to an archive system with
SCSI interface has failed. Possible reasons:
Problem in the library (e.g. Scalar i2000).
I/O blade failure.
Problems with the fibre channel path (e.g. switch).
Problems with the HBA of the ROBAR-SV host.

### Response

If the problem cannot be solved contact the maintenance.
If the failure persists ROBAR-SV stops.

## ROB5004

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5004 ERROR IN AML SYSTEM DATA BASE (ffff / VSN=vvvvvv), CONTACT MAINTENANCE

### Meaning

The AML system has an internal error in its data base and has reported
it by means of an error code.
Additional information:
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- vvvvvv: Volume Serial Number, if known by ROBAR

### Response

Check the integrity of the data base of the AML system.
If the problem cannot be solved, contact the maintenance.

## ROB5005

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5005 AML NOT READY FOR OPERATION (VSN=vvvvvv / ffff). CONTACT SYSTEM ADMINISTRATOR

### Meaning

The AML system is not ready and has reported its status by means of
an error code.
Additional information:
- vvvvvv: Volume Serial Number, if known by ROBAR
- ffff : error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)

### Response

Check the cause of the error of the AML system.
If the problem cannot be solved, contact the maintenance.

## ROB5011

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5011 INVALID ASSIGNMENT (DEV=mmmm / ffff / VSN=vvvvvv). CONTACT SYSTEM ADMINISTRATOR

### Meaning

The AML system has received a request for a device or cartridge
whose coordinate is not accessible by the specified robot arm.
Possible reasons:
1. The declaration of the cartridge in the MAREN catalog is wrong.
2. The cartridge has been inserted into the AML system via a wrong
Input Box.
3. The AML configuration is wrong.
4. The device is assigned to the wrong robot arm in the ROBAR
configuration.
Additional information:
- mmmm: device mnemonic
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- vvvvvv: Volume Serial Number

### Response

Declare the cartridge with the correct LOCATION in MAREN or eject it
from the AML system and insert it again via the right Input Box.

## ROB5025

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5025 CANNOT EMPTY THE DEVICE (DEV=mmmm). CONTACT SYSTEM ADMINISTRATOR

### Meaning

A cartridge remains in the device and cannot be removed by the AML
system.
The device is probably defective and cannot be used without
risk of additional problems. Either ROBAR has therefore issued
a DETACH-DEVICE command or ROBAR has set an internal indicator
to prevent any further usage of the device.
Additional information:
- mmmm: device mnemonic

### Response

Remove the cartridge manually from the device and update the
AML system data base to keep consistent information.
Check the previous error messages to find the source of error.
When it is eliminated, the device has to be attached again.
Thereby the internal lock in ROBAR will also be reset.
If the problem cannot be solved, contact the maintenance.

## ROB5026

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5026 CANNOT REMOVE TAPE CARTRIDGE FROM DEVICE, INIT REJECTED (DEV=mmmm / ffff). CONTACT SYSTEM ADMINISTRATOR

### Meaning

A cartridge remains in the device and cannot be removed by the AML system.
The current INIT or LIST request has been rejected because it cannot be
fulfilled on another device.
The device is probably defective and cannot be used without risk of
additional problems. ROBAR has therefore issued a DETACH-DEVICE
command to prevent any further usage of the device.
Additional information:
- mmmm: device mnemonic
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)

### Response

Remove the cartridge from the device manually and update the AML system
database to keep consistent information.
Check with previous error messages the error cause and attach
the device when it is corrected.
Issue the INIT or LIST request again.
If the problem cannot be solved, contact the maintenance.

## ROB5027

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5027 CANNOT CLOSE COVER. (DEV=mmmm / ffff / VSN=vvvvvv). CONTACT SYSTEM ADMINISTRATOR

### Meaning

The AML system cannot close the cover of the device.
Either the mount request has been redirected to another device
by means of a /CHANGE-TAPE-MOUNT ACTION=*MOVE command or,
in case of an INIT or LIST, the request has been rejected
because another device cannot be used.
The device cannot be used without risk of additional problems.
ROBAR has therefore issued a DETACH-DEVICE command to prevent
any further usage of the device.
Additional information:
- mmmm : device mnemonic
- ffff : error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- vvvvvv: Volume Serial Number

### Response

Check the device cover and verify the teaching of the AML system.
Attach the device when the error is corrected.
In case of INIT or LIST request, issue it again.
If the problem cannot be solved, contact the maintenance.

## ROB5101

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5101 ROBOT CRASH IN TOWER OR DEVICE OR STORAGE LOCATION (DEV=mmmm / ffff /VSN=vvvvvv). CONTACT SYSTEM ADMINISTRATOR

### Meaning

The AML system cannot remove or replace a cartridge.
The current request for the device is pended.
In some cases, ROBAR has issued a DETACH-DEVICE command to prevent
usage of a defective device.
Additional information:
- mmmm: device mnemonic
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- vvvvvv: Volume Serial Number

### Response

Check the AML system. Especially control the teaching and
the robot sensor. Attach the device when the error is corrected.
If the problem cannot be solved, contact the maintenance.

## ROB5104

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5104 LOST CARTRIDGE FROM GRIPPER (DEV=mmmm / ffff / VSN=vvvvvv). CONTACT SYSTEM ADMINISTRATOR

### Meaning

The cartridge has been lost from the gripper of the robot.
Possible reasons are:
1. The sensor of the robot is defective.
2. The gripper of the robot is defective.
3. There is a teaching problem of the robot.
4. The cartridge cannot be taken by the robot because it is defective.
5. The cartridge cannot be taken by the robot because a device is
defective.
Additional information:
- mmmm: device mnemonic
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- vvvvvv: Volume Serial Number

### Response

Check the AML system. Especially control the teaching, the robot sensor
and the gripper.
Check the device and cartridge status.
If the problem cannot be solved, contact the maintenance.

## ROB5209

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5209 MISMATCH BETWEEN CARTRIDGE TO BE MOUNTED AND THE DEVICE TYPE (DEV=mmmm / ffff / VSN=vvvvvv).

### Meaning

The device does not support the cartridge type.
The declaration of the cartridge in the MAREN catalog is wrong or the
cartridge has been inserted into the AML system via a wrong I/O Box.
Additional information:
- mmmm : device mnemonic
- ffff : error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- vvvvvv: Volume Serial Number

### Response

Declare the cartridge with the correct DEVICE-TYPE in MAREN catalog
or eject it from the AML system and insert it again via the
appropiate Input Box.

## ROB5301

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5301 VOLUME IS UNKNOWN TO AML SYSTEM DATA BASE (TSN=tttt / ffff / VSN=vvvvvv)

### Meaning

Possible reasons are:
1. The cartridge has not been inserted in the AML system.
2. The definition of the volume in the MAREN catalog is wrong.
3. The data base of the AML system is damaged.
Additional information:
- tttt: Task Serial Number
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- vvvvvv: Volume Serial Number

### Response

Check the integrity of the data base of the AML system, the MAREN
definition of the volume or insert the cartridge into the AML system.
If the problem cannot be solved, contact the maintenance.

## ROB5302

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5302 CARTRIDGE STORAGE PLACE IS EMPTY (TSN=tttt / ffff / VSN=vvvvvv)

### Meaning

Possible reasons are:
1. The cartridge is not at the right place in the AML system.
2. The cartridge has been ejected from the AML system.
3. The cartridge is already mounted on another device.
4. The cartridge is already mounted on the device.
5. The data base of the robot system is damaged.
6. In conjunction with CentricStor a logical volume could have been
placed on a physical volume which is not accessible because
of a drive or volume error.
Additional information:
- tttt : Task Serial Number
- ffff : error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- vvvvvv: Volume Serial Number

### Response

If the cartridge is already mounted on a device, check with
previous messages if two mount requests have been issued
for the same volume. Otherwise check the consistency of the
data base of the AML system with the real cartridge position.
If the problem cannot be solved, contact the maintenance.

## ROB5303

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5303 CARTRIDGE ALREADY MOUNTED ON OTHER DEVICE (TSN=tttt / VSN=vvvvvv)

### Meaning

Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Check by means of the previous messages if two mount requests have
been issued for the VSN.

## ROB5304

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5304 ROBOT SYSTEM CANNOT READ BARCODE LABEL (VSN=vvvvvv / ffff)

### Meaning

Possible reasons:
1. The barcode of the cartridge is damaged.
2. The barcode reader of the AML system is defective.
3. There is no barcode on the cartridge.
Additional information:
- vvvvvv: Volume Serial Number
- ffff : error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)

### Response

The problem can be temporarily bypassed by an option in the
roboter_cmds file of ROBAR-SV that allows to switch reading of
barcode to OFF for all operations, the initialisation excepted.
If the same error occurs several times, check the barcode reader
of the AML system.
If the problem cannot be solved, contact the maintenance.

## ROB5305

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5305 NO CARTRIDGE FOUND IN SPECIFIED INSERT AREA (TSN=tttt / ffff)

### Meaning

Possible reasons are:
1. The cartridge(s) to be inserted is (are) not in INPUT area of the
I/O box of the AML system.
2. The cartridge(s) to be inserted is (are) in the I/O box of the other
robot-arm.
3. The number of I/O box is not correctly specified in the
ROBOT_INPUT_AREA shell variable of ROBAR.
Additional information:
- tttt: Task Serial Number
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)

### Response

Check if the cartridge(s) is (are) in the correct I/O box.
If the robot has several I/O boxes (multimedia robot system), check if
the ROBOT_INPUT_AREA shell variable of ROBAR is correct.

## ROB5306

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5306 UNEXPECTED CARTRIDGE IS FOUND AT THE STORAGE PLACE OF VOLUME=vvvvvv

### Meaning

The possible reasons are:
1. The label of the volume is damaged and could not be read.
2. Some cartridges have been interchanged in the AML system.
3. The data base of the AML system is damaged or incorrect.
Additional information:
- vvvvvv: Volume Serial Number

### Response

Check for the consistency of the data base of the AML system
with regard to the real position of the cartridges and correct
either the data base or the position of the cartridges.
If the problem cannot be solved, contact the maintenance.

## ROB5503

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB5503 I/O-BOX IS FULL (VSN=vvvvvv / ffff). CONTACT OPERATOR

### Meaning

No cartridge can be ejected anymore.
Additional information:
- vvvvvv: Volume Serial Number
- ffff : error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)

### Response

Remove the cartridges from the output area of the I/O box
and notify ROBAR when it is empty by means of the command
/SEND-MESSAGE TO=OPERATOR,MESSAGE='<T I/O-BOX EMPTY'.

## ROB6060

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6060 WRONG VOLUME MOUNTED (DEV=mmmm / TSN=tttt / VSN=vvvvvv)

### Meaning

A volume has been mounted that does not fulfill the
system request. According to the options set by the user :
- the mount request cannot be satisfied. Volume processing
is terminated.
- the system protection is bypassed
Additional information:
- mmmm : device mnemonic
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number of requested volume

### Response

Contact the system administrator, if necessary.

## ROB6062

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6062 VOLUME IS WRITE-PROTECTED (VSN=vvvvvv / TSN=tttt)

### Meaning

The volume processing is terminated and the volume is put back at
its storage place.
Additional information:
- vvvvvv: Volume Serial Number
- tttt : Task Serial Number

### Response

Possible action:
Remove the write protection on the medium.

## ROB6068

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6068 AN IRRECOVERABLE ERROR HAS OCCURRED (DEV=mmmm / ffff / TSN=tttt / VSN=vvvvvv)

### Meaning

The AML system has sent an error code that ROBAR cannot handle
autonomously.
Additional information:
- mmmm : device mnemonic
- ffff : error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Contact the maintenance, if necessary.

## ROB6069

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6069 EITHER TOO MANY OR UNRECOVERABLE HARDWARE ERRORS ON DEVICE (DEV=mmmm)

### Meaning

Too many hardware errors occurred, in sequence, on the same device.
The action requested by options MRV26 has been started for the job and
MRV24 has been started for the device.
These options can be found and modified in the file
message/message_resp of ROBAR-SV.
Exception: if the mount has been directly requested by MAREN,
it is always rejected with the response "N".
Additional information:
- mmmm: device mnemonic

### Response

Fix the error. Contact the maintenance, if necessary.
After the error has been fixed, in certain circumstances the
device error counter has to be reset manually by the command
/SEND-MESSAGE TO=OPERATOR,MESSAGE='<T DEVICE mmmm REPAIRED'
resp. INFORM-OPERATOR MSG='<T DEVICE mmmm REPAIRED'.

## ROB6070

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6070 EITHER TOO MANY OR UNRECOVERABLE HARDWARE ERRORS ON VOLUME (VSN=vvvvvv)

### Meaning

Too many hardware errors occurred, in sequence, on the same volume.
The action requested by options MRV27 has been started for
the JOB and MRV25 has been started for the volume.
These options can be found and modified in the file
message/message_resp of ROBAR-SV.
Exception: if the mount has been directly requested by MAREN,
it is always rejected with the response "N".
Additional information:
- vvvvvv: Volume Serial Number

### Response

Fix the error. Contact the maintenance, if necessary.
After the error has been fixed, in certain circumstances the
volume error counter has to be reset manually by the command
/SEND-MESSAGE TO=OPERATOR,MESSAGE='<T VOLUME vvvvvv REPAIRED'
resp. INFORM-OPERATOR MSG='<T VOLUME vvvvvv REPAIRED'.

## ROB6071

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6071 DEVICE ERROR COUNTER RESET (DEV=mmmm)

### Meaning

ROBAR now considers the device as repaired.
- mmmm: Device Mnemonic

## ROB6072

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6072 HARDWARE ERROR DETECTED (DEV=mmmm / TSN=tttt / VSN=vvvvvv)

### Meaning

ROBAR detected a hardware error on device or volume.
Possible reason :
The mounted volume got a wrong type.
Additional information:
- mmmm : device mnemonic
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Details on the HW error are given in the preceding EXC0858
message. It is perhaps necessary to initialise the volume again.

## ROB6073

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6073 VOLUME ERROR COUNTER RESET (VSN=vvvvvv)

### Meaning

ROBAR now considers the volume as repaired or new.
- vvvvvv: Volume Serial Number

## ROB6074

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6074 VOLUME INIT ONLY PERMITTED WITH MAREN (VSN=vvvvvv / TSN=tttt)

### Meaning

The mounted volume can only be initialised with MAREN. It is
automatically dismounted.
Additional information:
- vvvvvv: Volume Serial Number
- tttt : Task Serial Number

### Response

Try to initialise the volume by using MARENADM.

## ROB6076

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6076 NO DEVICE ACCESS PATH IS AVAILABLE, DEVICE DETACHED (DEV=mmmm)

### Meaning

No path is available to access the device. Possible reason:
- no switch of device to virtual machine
Additional information:
- mmmm: device mnemonic

### Response

Possible actions :
1. Switch the device to the involved virtual machine.
2. Attach the corresponding controller.

## ROB6507

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6507 VOLUME HAS A TAPE LENGTH ERROR AND IS UNLOADED (TSN=tttt / VSN=vvvvvv)

### Meaning

After the device has been unloaded, the volume is put back to
its storage place. It cannot be mounted for write operation on
the specified device.
Possible reasons are:
1. An attempt to write on a TAPE-C1 or TAPE-C2 tape with a TAPE-C4
device, but this latter can only read these volume types.
2. Inversely, a TAPE-C1 or TAPE-C2 device is not able to deal
with TAPE-C4 volumes.
3. An error occurred with the medium.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Change the volume definition in MAREN catalog if possible, or
eject the volume from the AML system to manage it manually, or
copy the volume on a support of appropriate type.
Contact the system administrator, if necessary.

## ROB6508

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB6508 VOLUME HAS A TAPE LENGTH ERROR AND IS EJECTED (TSN=tttt / VSN=vvvvvv)

### Meaning

The current tape length is too short. The volume must be removed from
the robot system because it cannot be mounted on a device managed
by the robot without a risk of damage.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Replace the defective volume.
Contact the system administrator, if necessary.

## ROB7005

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7005 COMMAND SUCCESSFULLY PROCESSED (TSN=tttt)

### Meaning

The ROBAR-SDF command has been successfully processed.
Additional information:
- tttt: Task Serial Number

## ROB7010

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7010 ERROR OCCURRED. COMMAND NOT PROCESSED (TSN=tttt, ERROR=ffff)

### Meaning

An error occurred so that the ROBAR-SDF command could not be processed.
Additional information:
- tttt: Task Serial Number
- ffff: error code returned by the AML system
(issue a /HELP-MSG ROBffff command to get its meaning)

### Response

Contact the maintenance, if necessary.

## ROB7014

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7014 VSN IS ALREADY DEFINED (TSN=tttt / VSN=vvvvvv)

### Meaning

Possible reasons:
- volume already belongs to a freepool
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Possible actions :
- use another volume identifier to issue the command

## ROB7015

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7015 VSN OR POSITION IS ALREADY ASSIGNED (TSN=tttt / VSN=vvvvvv / POSITION=aaaaaa)

### Meaning

Possible reasons:
- The volume is already defined as a foreign.
- The foreign position is already used by ROBAR or another host.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number
- aaaaaa: Foreign Cartridge Storage Place

### Response

Possible actions :
- Use another volume identifier to issue the command.
- Use another position to issue the command.
- Make sure that the position is released by the other host (DAS,...).

## ROB7016

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7016 INCONSISTENCY DETECTED WHEN MANAGING THE FREEPOOL (TSN=tttt)

### Meaning

The command could not be processed because it induces an inconsistency
in the existing definitions.
Possible reason:
- The VSN ranges overlap.
Additional information:
- tttt: Task Serial Number

## ROB7017

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7017 ERROR OCCURRED WHEN ACCESSING THE VOLUME DEFINITIONS (TSN=tttt)

### Meaning

An error occurred when accessing to the volume definitions.
Possible reasons :
1. The foreign/freepool directory is locked or secured.
2. The foreign/freepool definitions are inconsistent.
3. The foreign/freepool definitions do not exist.
4. The foreign/freepool definitions are already erased.
Additional information:
- tttt: Task Serial Number

### Response

Possible actions :
1. Correct the access right to the definition files.
2. Erase the existing definitions and create new ones.
3. Contact the maintenance if necessary.

## ROB7018

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7018 SYNTAX ERROR IN VSN SPECIFICATION (TSN=tttt)

### Meaning

At least one given volume name is in error.
Possible reasons :
1. The VSN is over 6 characters in length.
2. The VSNs in the freepool range have different lengths.
3. The VSN range boundaries have different prefix or suffix.
4. The range part used to define the boundaries does not only
contain digits.
Additional information:
- tttt: Task Serial Number

### Response

Correct the VSN definition and try again.

## ROB7019

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7019 VSN NOT KNOWN IN ROBAR_ARCHIV OR POSITION NOT KNOWN IN ROBAR_FOREIGN (TSN=tttt / VSN=vvvvvv)

### Meaning

The VSN must be defined in ROBAR_ARCHIV or the POSITION in ROBAR_FOREIGN
but they are not.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Define the VSN in ROBAR_ARCHIV or the POSITION in ROBAR_FOREIGN and try
the command again.

## ROB7020

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7020 VSN IS MOUNTED OR IN INCONSISTENCY STATE. REMOVAL OF ITS FOREIGN DEFINITION IS NOT ALLOWED (TSN=tttt / VSN=vvvvvv)

### Meaning

The specified volume has a foreign position indicated as shared.
To keep consistent information for usage of the position by
other hosts, it is forbidden to remove its foreign definition
as long as the volume is mounted.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Remove the definition when the volume is not mounted any more.

## ROB7060

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7060 VOLUME EJECTED (TSN=tttt / VSN=vvvvvv)

### Meaning

The volume has been successfully ejected.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

## ROB7061

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7061 VOLUME IS DEFECTIVE (VSN=vvvvvv)

### Meaning

A previous BS2000 error message describes the error.
Additional information:
- vvvvvv: Volume Serial Number

## ROB7062

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7062 VOLUME WAS ALREADY EJECTED (TSN=tttt / VSN=vvvvvv)

### Meaning

The volume has been previously ejected.
It is already in the I/O box. Nothing to do.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

## ROB7063

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7063 WARNING: VOLUME UNKNOWN IN ROBOT DATA BASE (TSN=tttt / VSN=vvvvvv)

### Meaning

The volume is unknown in the robot system data base.
Either it is already in the I/O box after an Eject Total (EJT),
or there is an inconsistency.
Nothing to do.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

## ROB7064

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7064 VOLUME MOUNTED ON DEVICE. EJECT NOT POSSIBLE (TSN=tttt / VSN=vvvvvv)

### Meaning

The volume is mounted on a device.
Eject is not possible. Command rejected.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Enter /UNLOAD in BS2000 or KE in MANUAL menu.

## ROB7065

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7065 EJECT NOT PROCESSED (TSN=tttt / VSN=vvvvvv)

### Meaning

The volume ejection could not be performed. Possible reasons :
- The output box is full.
- The volume is unknown or already ejected.
- An unknown AML system error occurred during volume ejection.
- In the config file of ROBAR-SV the parameter robot_output_area
- has a wrong value.
Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

## ROB7066

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7066 OUTPUT BOX IS FULL

### Meaning

Eject command cannot be processed.

### Response

Empty the output box and try the command again.

## ROB7070

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB7070 INSERT STARTED (TSN=tttt)

### Meaning

The cartridge insertion will be processed asynchronously.
Additional information:
- tttt: Task Serial Number

## ROB8010

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB8010 EMERGENCY UNLOAD WAS UNSUCCESSFUL (DEV=mmmm)

### Meaning

Additional information:
- mmmm: device mnemonic

## ROB8015

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB8015 EMERGENCY UNLOAD ACTIVATED (DEV=mmmm), PLEASE WAIT

### Meaning

Due to the running context and possibly previous hardware errors,
ROBAR decides to make the device empty. Please wait.
Additional information:
- mmmm: device mnemonic

## ROB8020

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB8020 EMERGENCY UNLOAD WAS SUCCESSFUL

## ROB9000

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9000 TAPE CARTRIDGE HAS DMS WRITE PROTECTION (TSN=tttt / VSN=vvvvvv)

### Meaning

Additional information:
- tttt : Task Serial Number
- vvvvvv: Volume Serial Number

### Response

Contact the system administrator, if necessary.

## ROB9003

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9003 EXPORT-COMMAND RESUMED

### Meaning

The previous export command was interrupted, but it is correctly
resumed now.

## ROB9004

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9004 EXPORT-COMMAND CANNOT BE RESUMED

### Meaning

Due to an AML system error, the export command cannot be resumed.

### Response

Possible actions:
1. Make the AML system ready for work.
2. Make the output box empty.

## ROB9600

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9600 ROBAR COUNTS A GRAVE ERROR ON DEVICE mmmm

### Meaning

ROBAR counted a grave error on the device.
When the number of errors hits the limit given in the
ROBAR-SV configuration file (device_error_limit=),
special actions are started for the BS2000 job and the device.
The action on the BS2000 job is defined in the MRV26 option of the
file message/message_resp of ROBAR-SV.
The action on the device is defined in the MRV24 option of the file
message/message_resp of ROBAR-SV.
The default value for device_error_limit is 3.
The default action on BS2000 job is to move it on another device.
The default action on the device is to detach it.
Exception: if the mount has been directly requested by MAREN,
it is always rejected with the response "N".
If the next job on the device is error free, the error counter
will be decreased.
Additional information:
- mmmm: device mnemonic

### Response

Possible actions :
1. Analyse the error origin by a conslog analysis.
2. Contact the maintenance if necessary.

## ROB9601

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9601 ROBAR DEDUCTS A GRAVE ERROR FOR DEVICE mmmm

### Meaning

Robar counted grave errors in sequence on the device. Since the last
operation was successfully processed, the error counter has been
decreased.
Additional information:
- mmmm: device mnemonic

## ROB9602

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9602 ROBAR COUNTS A GRAVE ERROR ON VOLUME vvvvvv

### Meaning

ROBAR counted a grave error on the volume.
When the number of errors reaches the limit given in the
ROBAR-SV configuration file (volume_error_limit=),
special actions are started for the BS2000 job and the volume.
The action on BS2000 job is defined in the MRV27 option of the
file message/message_resp of ROBAR-SV.
The action on volume is defined in the MRV25 option of the file
message/message_resp of ROBAR-SV.
The default value for volume_error_limit is 3.
The default action on BS2000 job is to cancel it.
The default action on the device is to eject it.
Exception: if the mount has been directly requested by MAREN,
it is always rejected with the response "N".
If the next job on the volume is error free, the error counter
will be decreased.
Additional information:
- vvvvvv: Volume Serial Number

### Response

Possible actions :
1. Analyse the error origin by a conslog analysis
2. Contact the maintenance if necessary

## ROB9603

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9603 ROBAR DEDUCTS A GRAVE ERROR FOR VOLUME vvvvvv

### Meaning

Robar counted grave errors in sequence on the VSN. Since the last
operation was successfully processed, the error counter has been
decreased.
Additional information:
- vvvvvv: Volume Serial Number

## ROB9800

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9800 CENTRICSTOR IS UNABLE TO EXECUTE COMMAND

### Response

A problem occurred in CentricStor. Please contact your CentricStor
system engineer.

## ROB9801

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9801 COMMAND IS NOT PERMITTED

### Meaning

A command has been requested to a CentricStor configuration
but either the ROBAR RULE FILE is not the one dedicated to such a
CentricStor configuration or the MAREN catalogue is configured
for a location with type "ROBAR-2" but should not.
The command cannot be executed and is negatively acknowleged.

### Response

Either install the ROBAR RULE FILE for a CentricStor
configuration or correct your location attribute in MAREN.

## ROB9802

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ROB9802 A PROBLEM OCCURRED IN CENTRICSTOR. LOCATION : (&00)

### Meaning

(&00): LOCATION of the CentricStor

### Response

Please check CentricStor console for detailed information.

## ROB9803

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ROB9803 COMMAND NOT PERMITTED: FOREIGN VOLUMES AND FREEPOOLS NOT SUPPORTED

### Meaning

Foreign volumes and freepools are not supported in ROBAR-SV for
SCSI interface.

©2025 Fujitsu | BS2000 System Messages