## HEL0001

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0001 HW ERROR LOGGING FILE '(&00)' OPENED WITH 'SPACE=(&01)'

### Meaning

The HEL file has been opened by means of the command /START-HEL-LOGGING
or /CHANGE-HEL-FILE or during the startup.
(&00): name of the HEL file
(&01): primary allocation

## HEL0002

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0002 HW ERROR LOGGING FILE '(&00)' CLOSED

### Meaning

The HEL file has been closed by means of the command /STOP-HEL-LOGGING
or /CHANGE-HEL-FILE or during the shutdown.
(&00): name of the HEL file

## HEL0003

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0003 HW ERROR LOGGING IS ACTIVE. FILE : '(&00)'

### Meaning

(&00): name of the HEL file

## HEL0004

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0004 HW ERROR LOGGING INACTIVE

## HEL0005

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0005 TELESERVICE ALARM BY HEL IS ACTIVE. MONITORING INTERVALL FROM (&00) TO (&01)

### Meaning

The threshold monitoring of HEL and calling of teleservice is active.
Calling of teleservice is done only in the specified time interval.

## HEL0006

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0006 TELESERVICE ALARM BY HEL IS DEACTIVATED.

### Meaning

The threshold monitoring of HEL and calling of teleservice
is deactivated.

## HEL0010

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0010 HW ERROR LOGGING NOT ACTIVE. (&00) COMMAND REJECTED

### Meaning

All HEL commands except for /START-HEL-LOGGING and /SHOW-HEL-STATUS
are only permitted if HW error logging is active.

### Response

Issue a /START-HEL-LOGGING command and retry command.

## HEL0011

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0011 HW ERROR LOGGING ALREADY ACTIVE. /START-HEL-LOGGING COMMAND IGNORED

### Meaning

The /START-HEL-LOGGING command is only permitted if HW error logging
is not active.

## HEL0012

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0012 HW ERROR LOGGING ALREADY STOPPED. /STOP-HEL-LOGGING COMMAND IGNORED

### Meaning

The /STOP-HEL-LOGGING command is only permitted if HW error logging is
active.

## HEL0050

Destination: CONSOLE Routing code: H Weight: 50

Warranty : NO

HEL0050 CALL TELESERVICE. THRESHOLD FOR CTID (&00), PRIO (&01), (&02), SEQ# (&03) REACHED

## HEL0100

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0100 INTERNAL ERROR. COMMAND PROCESSING ABORTED

## HEL0101

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0101 SYSTEM ERROR. (&00) NOT AVAILABLE. /START-HEL-LOGGING COMMAND NOT PROCESSED

### Meaning

HW error logging could not be activated because a necessary resource was
not available for the HEL system.
(&00): memory, HEL task, bourse, slotpool, slot.

## HEL0102

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0102 SYSTEM ERROR. (&00) COULD NOT BE RELEASED BY HW ERROR LOGGING. /STOP-HEL-LOGGING COMMAND NOT PROCESSED

### Meaning

A resource could not be released by HEL.
(&00): memory, task, bourse or slotpool.

## HEL0105

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0105 BOURSE CALLING ERROR. COMMAND PROCESSING ABORTED

### Meaning

A bourse calling error occurred while trying to communicate with the
HEL system task.

## HEL0106

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0106 SYSTEM ERROR. HW ERROR LOGGING NOT ACTIVATED. DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00). COMMAND PROCESSING ABORTED

### Meaning

While processing the HEL file a DMS error occurred.
(&00): DMS error code
(&01): file name

### Response

Remove error cause and try /START-HEL-LOGGING.

## HEL0107

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HEL0107 SYSTEM ERROR. DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00). DATA NOT STORED

### Meaning

While processing the HEL file a DMS error occurred.
(&00): DMS error code
(&01): file name

### Response

Try /CHANGE-HEL-FILE.

## HEL0108

Destination: CONSOLE Routing code: H Weight: 70

Warranty : YES

HEL0108 INTERNAL TABLE FOR THRESHOLD MODIFICATIONS FULL. NO MODIFICATION PERFORMED

### Meaning

The limit of number of entries for modification of threshold is reached.
No modification performed.

### Response

All additional settings could be cleared by /MODIFY-HEL-CHECK
CHECK=*STD.

## HEL0109

Destination: CONSOLE Routing code: H Weight: 70

Warranty : YES

HEL0109 INTERNAL TABLE FOR LOGGING MODIFICATIONS FULL. NO MODIFICATION PERFORMED

### Meaning

The limit of number of entries for modification of logging is reached.
No modification performed.

### Response

All additional settings could be cleared by /MODIFY-HEL-LOGGING
LOGGING=*STD.

## HEL0110

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HEL0110 USER IS NOT AUTHORIZED TO ISSUE THE COMMAND. COMMAND REJECTED

### Meaning

The user does not have the privilege to issue the command.

## HEL1001

Destination: CONSOLE Routing code: H Weight: 50

Warranty : NO

HEL1001 STARTUP ERROR. HW ERROR LOGGING NOT ACTIVATED. (&00) NOT AVAILABLE. STARTUP CONTINUES

### Meaning

HW error logging could not be activated because a necessary resource was
not available for the HEL system.
(&00): memory, HEL task, bourse, slotpool, slot.

### Response

Try /START-HEL-LOGGING later.

## HEL1002

Destination: CONSOLE Routing code: H Weight: 50

Warranty : NO

HEL1002 STARTUP ERROR. HW ERROR LOGGING NOT ACTIVATED. BOURSE CALLING ERROR. STARTUP CONTINUES

### Meaning

HW error logging could not be activated because a bourse calling error
occurred while trying to communicate with the HEL system task.

### Response

Try /START-HEL-LOGGING later.

## HEL1003

Destination: CONSOLE Routing code: H Weight: 50

Warranty : NO

HEL1003 STARTUP ERROR. HW ERROR LOGGING NOT ACTIVATED. DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

While processing the HEL file a DMS error occurred.
(&00): DMS error code
(&01): file name

### Response

Remove error cause and try /START-HEL-LOGGING.

## HEL9000

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HEL9000 SYSTEM ERROR. HW ERROR LOGGING ABORTED

### Meaning

A system error has resulted in an abnormal termination of the
HEL task.

## HEL9001

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HEL9001 SYSTEM ERROR. DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00).

### Meaning

A DMS error resulted in an abnormal HEL task termination. HW error
logging aborted.
(&00): DMS error code
(&01): file name

## HEL9002

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HEL9002 SYSTEM ERROR. BOURSE CALLING ERROR.

### Meaning

A bourse calling error resulted in an abnormal HEL task termination.
HW error logging aborted.

## HEL9003

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HEL9003 SYSTEM ERROR. HEL SPECIFIC DISC SPACE ON PUBSET USED UP.

### Meaning

HEL specific disc space is used up. HW error logging aborted.

### Response

Remove error cause (perhaps delete old HEL files) and reactivate HW error
logging with a /START-HEL-LOGGING.

©2025 Fujitsu | BS2000 System Messages