## NCL0001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0001 SYSTEM ERROR. LOGGING APPLICATION '(&00)' ABORTED

### Meaning

A system error has resulted in the abnormal termination of the
task connected to the logging application (&00).

### Response

Restart the logging application.

## NCL0002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0002 DMS ERROR '(&00)' ON FILE '(&01)'. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

In the case of an OPEN error the old file is not closed and the new one
not opened.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages' or one of the
BS2000 DMS manuals.

## NCL0003

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NCL0003 STOP PROCESSING OF LOGGING APPLICATION '(&00)' NOT YET COMPLETED. REPEAT START LATER

### Meaning

The logging application file could not be opened because STOP processing
of the logging application (&00) was not yet completed.

## NCL0004

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0004 SLOT POOL FOR LOGGING APPLICATION '(&00)' CANNOT BE CORRECTLY CLOSED

### Meaning

Not all slots requested by the logging application (&00) are released.
Therefore the slot pool for (&00) cannot be correctly closed.
This message is used in order to document a system error.

## NCL0005

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0005 NO MEMORY AVAILABLE

### Meaning

A $GETMEM could not be satisfied.

### Response

Restart the log application with an appropriate command.

## NCL0006

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0006 SYSTEM ERROR IN COMMON LOG TASK FACILITY

### Meaning

The system function $SRMREQ,
called by NRTCLTK, was not executed correctly.

### Response

Take dump.

## NCL0007

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0007 RESOURCES FOR THE COMMON LOG TASK NOT AVAILABLE

### Meaning

The Name Manager Class for the Common Log Task could not
be enabled.

### Response

Take dump.

## NCL0008

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0008 INCONSISTENCY IN COMMON LOG TASK FACILITY DATA

### Response

Take dump.

## NCL0009

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0009 SYSTEM ERROR IN COMMON LOG TASK FACILITY

### Meaning

One of the system functions $RETMEM or $NBDEST,
called by NRTCLTK, was not executed correctly.

### Response

Take dump.

## NCL0100

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0100 TASK RESTART NOT POSSIBLE DUE TO RECURSIVE ERROR

### Meaning

During the restart of this task an internal inconsistency or
an error in one of the functions Name Manager or Slot Pool occurred.

### Response

Restart the log application with an appropriate command.

## NCL0101

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0101 TASK RESTART NOT POSSIBLE BECAUSE THE TIME SINCE LAST RESTART IS TOO SHORT

### Meaning

Task restart is not allowed if the previous restart is less than
10 minutes ago.

### Response

Restart the log application with an appropriate command.

## NCL0102

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0102 TASK RESTART NOT POSSIBLE DUE TO REPEATED ERRORS

### Meaning

The same error has occurred repeatedly in this task :
exactly the same error initiated the previous task restart,
several restarts with DMS recovery have been activated
or slot pool recovery must be retried.

### Response

Restart the log application with an appropriate command.

## NCL0103

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0103 TASK RESTART IST NOT POSSIBLE BECAUSE NO MEMORY IS AVAILABLE

### Meaning

As no memory could be obtained by $GETMEM,
task restart is not possible.

### Response

Restart the log application with an appropriate command.

## NCL0104

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NCL0104 SEVERE ERROR PREVENTS TASK RESTART

### Meaning

An error in the Bourse function or in the module NRTCLTK prevents
task restart.

### Response

Restart the log application with an appropriate command.

©2025 Fujitsu | BS2000 System Messages