## POPAAAA

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : YES

POPAAAA Current DUMP-LIMIT-PER-HOUR ((&00)) of SYSTEMDUMP-MANAGERs reached or exceeded by (&01)! Continue? Response:Y/N

### Meaning

If you want this system error to be handled by the
SYSTEMDUMP-MANAGER despite the fact that DUMP-LIMIT-PER-HOUR
has been exceeded, respond with "Y".
You can also adjust DUMP-LIMIT-PER-HOUR to a changed situation
using the MODIFY-SDM-PARAMETER command.
If it no longer makes sense to use the SYSTEMDUMP-MANAGER, terminate,
the administration process by responding with "N"
Until this question has been answered, no new dump messages can
be processed by the SYSTEMDUMP-MANAGER.

## POPAAAB

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POPAAAB DUMP-LIMIT-PER-HOUR not in defined range of values (<integer 0..255>)

### Response

Correct and restart the administration process.

## POPAAAC

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POPAAAC DUMP-OCCURRENCE not in defined range of values (<integer 1..255> or *ANY)

### Response

Correct and restart the administration process.

## POPAAAD

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : YES

POPAAAD HISTORY-FILE not a SAM file. Command not executed

## POPAAAE

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POPAAAE Problems signing on to PROP-XT subsystem

### Meaning

The SYSTEMDUMP-MANAGER may only be used once per system or
PROP-XT is not installed.

### Response

Terminate any administration process that is running and restart the
SYSTEMDUMP-MANAGER using ENTER-PROCEDURE or install PROP-XT.

## POPAAAF

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POPAAAF OPERATOR-ROLE not specified or incorrect

### Response

Correct and restart the administration process.

## POPAAA1

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POPAAA1 SYSTEMDUMP MANAGER terminated (MC=(&00))

### Meaning

SYSTEMDUMP MANAGER was terminated.
Cause: See maincode MC (PROP-XT User Guide).

## POPAAA2

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : YES

POPAAA2 SYSTEMDUMP MANAGER working with empty HISTORY-FILE

## POPAAA3

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : YES

POPAAA3 MODUL-LIST-FILE not a SAM or ISAM file (KEY-LEN=8). Command not executed

## POPAAA4

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : YES

POPAAA4 SYSTEMDUMP MANAGER working with empty MODUL-LIST-FILE

## POP0A0A

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A0A Too many operands in command

### Meaning

The command defined as an event in the SDF-P variable
cannot be processed since the number of operands is greater than 20.

## POP0A0B

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A0B Command operands cannot be edited

### Meaning

The command defined as an event in the SDF-P variable
cannot be edited since the value of the operand(s) is neither
STRING nor INTEGER.

## POP0A0C

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A0C /BEGIN-PROP-PROCESS must be first PROP-XT command in an administration procedure.

## POP0A0D

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A0D Specified command is not a PROP-XT system command

### Meaning

The command received could not be identified as a PROP-XT
system command on account of the internal command name.
It might be a PROP-XT administration command, but if so
it may not be used in an administration procedure.

## POP0A0E

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A0E No such PROP-XT system command in syntax file

### Meaning

In the syntax file a command was marked as an PROP-XT
system command although it is not one.

## POP0A0F

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A0F Total length of inserts too great

### Meaning

The combined length of all the inserts in a system
message may not exceed 180 characters.

## POP0A00

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A00 No PROP-XT authorization

### Meaning

The user ID which was used to try to sign on to
PROP-XT does not have the PROP-ADMINISTRATION privilege.

## POP0A01

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A01 Administration process with this name has already signed on

## POP0A02

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A02 Memory bottleneck

### Meaning

The message buffer (MTBUFF) for communicating
with the main task cannot be created.

## POP0A03

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A03 Resource bottleneck on system

### Meaning

GENERAL
Access to initialized PROP-XT data is faulty.
BEGIN-PROP-PROCESS
Bourse error in communication between administration task
and main task.
System error in querying the user ID of the administration process.
System error in querying the TSN of the administration process.
END-PROP-PROCESS
Bourse error in communication between administration task
and main task.
Error in releasing AP name for NAME-MANAGER.
Error in releasing communication buffer (MTBUFF).
START-PROP-EVENT-MONITORING
Bourse error in communication between administration task and
main task. No acknowledgment was received within 600 sec when
signing on a command. A negative acknowledgment was received from
UCON when signing on a command as an event.
STOP-PROP-EVENT-MONITORING, STOP-PROP-OBJECT-MONITORING
Bourse error in communication between administration task
and main task. An internal error has occurred.
START-PROP-OBJECT-MONITORING
Bourse error in communication between administration task
and main task. No acknowledgment was received withihin 600 sec
when setting up a connection to the administration entity.
SEND-TO-PROP-ADMINISTRATOR, SIMULATE-PROP-EVENT
Bourse error in communication between administration task
and main task.
SEND-TO-PROP-OBJECT
Bourse error for main task.

## POP0A04

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A04 Event type specified cannot be handled by PROP-XT

## POP0A08

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A08 None of the specified events defined for administration process

### Meaning

No events that can be waited for have been defined by,
the administration process.
The events specified in the list are not defined.

## POP0A09

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A09 Invalid message received

### Meaning

Message received does not match the event type specified.

## POP0A1A

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A1A Simulation not possible for administration entities or events

## POP0A1B

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A1B No administration entities defined for administration process

### Meaning

WAIT-FOR-PROP-EVENTS, START-PROP-EVENT-MONITORING
None of the specified administration entities are defined
for the administration process.
STOP-PROP-OBJECT-MONITORING
None of the specified administration entities are defined
for the administration process.
NOTE: When *ALL is specified for the administration entities
there is no check to see which ones have been defined.

## POP0A1C

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A1C Port signals error when sending over administration connection

## POP0A1D

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A1D Error in connection to one or more administration entities

### Meaning

WAIT-FOR-PROP-EVENT, START-PROP-EVENT-MONITORING
The connection no longer exists to all the administration
entities specified in the command.
Message POP9A06 is output for each such administration entity.
START-PROP-OBJECT-MONITORING
A negative acknowledgment was received when setting up the
connection to the administration entity.
SEND-TO-PROP-OBJECT
The connection to the administration entity
specified by /SEND-TO-PROP-OBJECT is cleared.
Port signals an error when sending over administration entity
connection.

## POP0A1E

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A1E Not all specified administration entities are defined. Processing continues

### Meaning

WAIT-FOR-PROP-EVENTS, START-PROP-EVENT-MONITORING
Some of the administration entities specified for the
administration process are not defined.
Message POP9A07 is output for each administration entity.
Message POP9A06 is output for each defined administration
entity to which the connection is not active.
STOP-PROP-OBJECT-MONITORING
Some of the specified administration entities are not
defined for the administration process.
Message POP9A07 is output for each administration entity.
SEND-TO-PROP-OBJECT
The specified administration entity is not defined for the
administration process.

## POP0A1F

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A1F Not all specified events are defined. Processing continues

### Meaning

The list of specified events includes some which are,
not defined.
Message POP9A04 is output for each such event.

## POP0A10

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A10 Syntax error in command

### Meaning

GENERAL
The syntax of the command received could not be analyzed
by PROP-XT (SDF command analysis).
SIMULATE-PROP-EVENT
The syntax of the command to be simulated is incorrect.

## POP0A11

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A11 Command allowed again only after END-PROP-PROCESS

### Meaning

A second BEGIN-PROP-PROCESS command is only permitted in
an administration task after an END-PROP-PROCESS command.

## POP0A13

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A13 Arriving events can no longer be buffered for the administration process

### Meaning

The memory space required exceeds the value permitted by
the administration command MODIFY-PROP-PARAMETERS.

## POP0A14

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A14 Termination requested

### Meaning

Via the administration command SEND-TO-PROP-PROCESS
the administration process was requested to terminate.
WAIT-FOR-PROP-EVENT
Via the Administration command SEND-TO-PROP-PROCESS the
administration process was requested to terminate. Any wait
time started can thus be terminated.

## POP0A15

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A15 Data inconsistency when processing system command

### Response

- Create fault documentation
- notify system service

## POP0A16

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A16 Error in accessing administration entity management data

### Meaning

GENERAL
Error in accessing the administration entity management data.
SEND-TO-PROP-OBJECT
Error in the administration entity management when sending data
to the administration entity.

## POP0A17

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A17 Error in accessing event management data

### Meaning

GENERAL
Error in accessing event management data.
START-PROP-EVENT-MONITORING
No acknowledgment was received within 600 sec when signing
on a command. A negative acknowledgment was received from
UCON when signing on a command as an event.
SEND-TO-PROP-OBJECT
No job could be generated for sending data to the
administrator.

## POP0A18

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A18 Error in accessing administration process management data

## POP0A19

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A19 Event could not be simulated for some administration entities. Processing continues

## POP0A20

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A20 Subsystem PROP-XT stopped

## POP0A21

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0A21 The specification of a user-id requires also the specification of a password

## POP0A22

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A22 Variable SYSPOP or <RESULT-VAR> could not be assigned. Processing continues

### Meaning

The variable SYSPOP or the specified result variable could not be
assigned because of missing or invalid declaration.

### Response

Insert a correct declaration of the variable into the PROP-XT
procedure.

## POP0A30

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0A30 Illegal Value for OWN-APPLICATION

### Meaning

The name may not start with "*" or "$".

### Response

Correct and try again.

## POP0B0A

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B0A Unknown REFERENCE-NAME

### Meaning

The user has specified a REFERENCE-NAME that does
not identify an order in this administration process.
The order may already have been terminated.

### Response

Check the REFERENCE-NAME.

## POP0B0B

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B0B Although order elements are expected, no REFERENCE-NAME was given

### Response

Specify REFERENCE-NAME.

## POP0B0C

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B0C Event name already used

## POP0B0D

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B0D Event name already used as group name

## POP0B0E

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B0E Group name already used as event name

## POP0B00

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B00 Illegal event type

## POP0B01

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B01 Illegal data type

## POP0B08

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B08 Specified REFERENCE-NAME already exists. Command ignored.

### Meaning

The specified REFERENCE-NAME already exists. The command was ignored.
or was not unambiguous in the specified length.
When sending queries and commands, the REFERENCE-NAME
must be unambiguous in the first 3 characters.

### Response

Choose another REFERENCE-NAME.

## POP0B09

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B09 Resource bottleneck with internal PROP-XT reference name

### Meaning

Too many commands and inquiries for which PROP-XT
has assigned an internal reference name (max.: >1300!)
have not been terminated.

### Response

Check the administration procedures for endless loops.

## POP0B1B

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B1B Not all specified elements of list defined.

### Meaning

In case of wait or check event: No events occurred

## POP0B1C

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0B1C Command server no longer connected

### Meaning

The command event is no longer defined in the server
administration process.

## POP0B1D

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0B1D Command could not be transferred to server administration process

### Meaning

- Buffer overflow owing to problems with server
administration process.

## POP0B1F

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B1F PROP-XT does not support jobs for this entity type. Processing continues

### Meaning

An operand was specified that is only relevant for job processing
(e.g. REFERENCE-NAME, IMPLICIT-EVENT).
However, PROP-XT does not support any jobs with this administration
type (DCAM/UTM).

## POP0B10

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B10 Permitted number of servers for operator special commands reached

## POP0B11

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B11 Connection error in signing on operator special command

## POP0B12

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B12 Message type currently not allowed

### Meaning

The order identified by the specified REFERENCE-NAME
is in a status in which the specified message type is not
allowed.

### Response

Check the REFERENCE-NAME, message type and status of the order.

## POP0B13

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B13 Time specified for time event already elapsed

## POP0B14

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B14 Illegal time specification

## POP0B18

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B18 No events occurred for selection criterion

### Meaning

WAIT-FOR-PROP-EVENT
No more events have occurred for the specified events since
those that have already been fetched/transferred, and the
wait time for the WAIT command (TIME-LIMIT=) has elapsed.
If OPERATIONAL-MODE=SIMULATION applies for the administration,
process, an event generated by the SIMULATE-PROP-EVENT command
(TIME-LIMIT-REACHED) aborts the WAIT command.
CHECK-PROP-EVENT-OCCURRENCE
No more events have occurred for the specified events since
those that have already been fetched/transferred.

## POP0B19

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B19 The events specified in the command were not defined beforehand

## POP0B20

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B20 Message type not supported. Processing continues

### Meaning

For entities of type DCAM or UTM no message types are supported.
The TYPE Specification is ignored.

## POP0B22

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B22 Internal error in ONEVT call

### Meaning

Failed to enable CJC monitoring for job variable(s).

### Response

Take user dump for further diagnosis.

## POP0B23

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0B23 Internal error in DONEVT call

### Meaning

Failed to disable CJC monitoring for job variable(s).

### Response

Take user dump for further diagnosis.

## POP0C00

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0C00 Administration entity description not in database

### Meaning

No administration entity description is contained in the database
for the administration entity.

### Response

The attributes of the administration entity must be
supplied with START-PROP-OBJECT-MONITORING or the
administration entity must be defined in the database
by the PROP-XT administrator.

## POP0C01

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0C01 No authorization to use the administration entity description from the database

### Meaning

The user is not authorized to use this administration entity
description from the database.

### Response

The PROP-XT administrator must authorize this user (user ID)
to use this administration entity description from the
database.

## POP0E0C

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E0C Connection already exists

### Meaning

A connection already exists between OWN-APPLICATION
and APPLICATION

### Response

Select a different name for OWN-APPLICATION and try again

## POP0E0E

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E0E OWN-APPLICATION cannot be opened.

### Meaning

The auxiliary application specified under OWN-APPLICATION
could not be opened.
Possible reasons:
- Application is pregenerated and protected by a user password
- BCAM problems such as
- shortage of memory space
- threshold values exceeded
- name reserves or AP ID exhausted
- BCAM shutdown announced

### Response

Retry command later.

## POP0E0F

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E0F Application specified in OWN-APPLICATION already open

### Meaning

The connection to the application entity could not be set up
because the auxiliary application OWN-APPLICATION has already
been opened exclusively or with password protection by another task.

### Response

Specify a different name for OWN-APPLICATION.

## POP0E05

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E05 No data specified.

### Meaning

The user attempted to send an empty string to an
entity of the type DCAM or UTM. Empty strings may
only be sent to entities of the type Operating.

## POP0E06

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E06 Letter length error reported by BCAM

### Meaning

The message or connection letter could not be
sent.
Possible reasons:
- BCAM threshold values exceeded

### Response

Check BCAM threshold values and/or take
system dump of PROP-XT holder task for
further diagnosis.

## POP0E10

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E10 Connection rejected by partner.

### Meaning

The partner or his transport system rejected
the connection request. BCAM issues
Station Information YDB_STCONREJ.
Possible reason: incorrect password

## POP0E11

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E11 Partner Application not known

### Response

Correct and try again.

## POP0E12

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E12 Name of partner system not known

### Response

Correct and try again

## POP0E13

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E13 Maximum number of connections per application exceeded.

### Meaning

BCAM limits the number of connections that an
application may open.
This number has been exceeded for the application specified
under OWN-APPLICATION.
Note: Other tasks can also open connections from this
application.
If an error occurs with START-PROP-OBJ-MON <name>, type=*OPERATING
too many connections within PROP have already been set up
to computers within the user's own MSCF network (of the type
CCS) without a user ID being specified.

### Response

With type = DCAM/UTM: select a different value
for APPLICATION.
With type = OPERATING: notify the system administrator.

## POP0E14

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E14 Computer not in common MSCF network

### Meaning

The user attempted to set up a connection to an entity of
the type Operating on a foreign system without specifying
the user ID. This works only if the partner system and the
local system are both in a common MSCF network of the type
CCS, the network is active and the BS2000 version used on
the partner system is >= V11.2.

### Response

Notify the system administrator or specify an operator
user ID.

## POP0E15

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E15 Illegal operator role

### Meaning

Operator role unknown or not permitted for this User-Id

### Response

Correct and try again.

## POP0E16

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0E16 Incorrect authorization information

### Meaning

Either the User ID or password specified in the
START-PROP-OBJECT-MONITORING command is incorrect

### Response

Correct and try again

## POP0001

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

POP0001 SUBSYSTEM '(&00)' VERSION '(&01)' STARTED

## POP010A

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP010A Connection to administration entity already exists

### Meaning

The administration entity defined in the command was
already defined and the connection is active.

## POP010B

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP010B SDF communication area could not be set up correctly

### Meaning

IMPLEMENTOR=TPR(ENTRY=DUMMY,CALL=NEW) must be
specified in the command definition.
A user command may not contain more than 20 operands.

### Response

Correct the command and recompile with SDF-A.

## POP010C

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP010C Syntax error in name

### Meaning

Possible cause: The REFERENCE-NAME specified
cannot be abbreviated so that it is a valid reference
name for UCON, or the name includes "$" or "-".

### Response

Correct the name and retry the command.

## POP0100

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0100 Administration entity already in database

### Meaning

The administration entity definition in the command
already exists.

### Response

Check the name specified for the administration entity,
definition and overwrite if required.

## POP0102

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0102 No administration entity definition

### Meaning

The administration entity definition in the command
does not exist.

### Response

Check the name specified for the administration entity,
definition and correct it.

## POP0107

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0107 Administration entity not of type UCON

### Meaning

Specified type is not supported in this PROP-XT version.

### Response

Change the administration entity type.

## POP0108

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0108 No more administration processes/entities allowed

### Meaning

The maximum number of administration processes/entities
currently permissible have already signed on.

## POP020F

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP020F Subsystem JV not available

## POP021D

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP021D Message code does not exist. Alternate message was generated

### Meaning

The message could not be found in the message files assigned.

### Response

Define the message and/or attach the message file

## POP0211

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0211 Syntax error - Command privilege "PROP-ADMINISTRATION" does not exist

### Meaning

The command originator (administrator) does not have
the "PROP-ADMINISTRATION" privilege.

### Response

Assign the administrator the "PROP-ADMINISTRATION" privilege

## POP0212

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0212 User-Id could not be found

### Meaning

There is no user-id to check syntax or authorisation
Wrong NBMHE-Header version.

### Response

Use at least OSD V2.0 or UCON-rep.

## POP0213

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0213 Specified system message could not be generated

### Meaning

SEND-TO-PROP-ADMINISTRATOR
The specified system message could not be generated (Message with
MSG-ID not in the message file or message file not assigned).
SIMULATE-PROP-EVENT
The message to be simulated could not be generated.
Error in accessing the message file. Check whether this file
actually contains the message with the specified MSG-ID.

## POP0214

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0214 Syntax error - Command ignored

### Meaning

The command syntax is incorrect. Detailed information
on the syntax error is supplied in the subsequent messages.

### Response

Correct and reenter the command.

## POP022A

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP022A New databasefile was created

## POP0223

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0223 Syntax error - SDF environment cannot be set up

### Meaning

An error occurred while setting up the environment
assigned to the command originator.

### Response

Check the command originator's user ID and set up correctly.

## POP0225

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0225 Access to job variable not possible

### Meaning

The job variable cannot be accessed (not defined,
not shareable).

## POP0229

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP0229 ENCRYPTION-PASSWORD (OLD-PASSWORD) specified for the required database file is incorrect

### Meaning

The passwords contained in the file were not all encrypted
with the specified password, or the file is not a PROP-XT
database file. The command was not executed.

## POP0235

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP0235 Version of database file incorrect

### Meaning

PROP-XT cannot work with the version specified in the database
file, or the file is not a PROP-XT database file. The command was
not executed.

## POP0240

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0240 Specified timestamp ambigious. Processing continues

### Meaning

The time specified is in the time overlap when switching from
daylight saving time to normal time. Depending on the SEASON operand,
an alternative time has been fixed.

## POP0241

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0241 Calculated time ambiguous. Processing continues

### Meaning

The time specified is in the time overlap when switching from
daylight saving time to normal time. Depending on the SEASON operand,
an alternative time has been fixed.

## POP0242

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP0242 Specified timestamp does not exist. Processing continues

### Meaning

Owing to the switch from normal to daylight saving time, the time
specified for the timestamp does not exist. Depending on the SEASON
operand, an alternative time has been fixed.

## POP0705

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0705 ENCRYPTION-PASSWORD (OLD-PASSWORD) password is different from the current one current one

### Meaning

The command was not executed. Changes to the database will only be
implemented after the current password has been entered.

### Response

Enter the correct password and try again.

## POP0707

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0707 Internal error when switching the database file

### Meaning

Errors occurred in PROP-XT (DVS error or resource bottleneck
Possible reasons:
- The open DB file cannot be closed.
- The DB file cannot be created, opened, read or written to.
- The password cannot be encrypted.

### Response

- Try again with a different database file.
- Notify the system administrator.

## POP0708

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0708 Internal error when accessing the database

### Meaning

Errors occurred in PROP-XT (resource bottleneck, data inconsistency).
The status of the database is undefined.

### Response

- Notify the system administrator.

## POP090B

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP090B Internal error. Command not executed fully

### Meaning

Errors occurred in PROP-XT (resource bottleneck, data inconsistency).
The command was not executed fully.

### Response

Retry.

## POP090C

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP090C No administration process specified in command exists

### Meaning

None of the administration processes specified in the
command is signed on to PROP-XT.

### Response

Correct names of administration processes.

## POP090D

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP090D Not all administration processes exist

### Meaning

Not all the administration processes specified in the
command are signed on to PROP-XT.

### Response

Correct names of administration processes.

## POP090E

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP090E No response administration entity definition

### Meaning

No administration entity definition exists for the
response administration entity specified in the command.

### Response

Create an administration entity definition for the
response administration entity.

## POP090F

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP090F No administration entity definition for STD-ACTION administration entity

### Meaning

No administration entity definition exists for
the STD-ACTION administration entity.

### Response

Create an administration entity definition for the
STD-ACTION administration entity.

## POP0900

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0900 No such command

### Meaning

PROP-XT does not recognize the command entered.

### Response

Correct the command if it is incorrect.
- Check whether PROP-XT can be administered. If it cannot,
subsystem PROP-XT must be started again.

## POP0901

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0901 STD-ACTION already exists. Command not executed.

### Meaning

The STD-ACTION specified in the command is already
signed on to PROP-XT.

### Response

Check the name specified for STD-ACTION, and if required
overwrite using the REPLACE-OLD-ACTION=YES operand.

## POP0902

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0902 Internal error. STD-ACTION could not be accepted

### Meaning

Errors occurred in PROP-XT (resource bottleneck, data inconsistency).

## POP0903

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0903 STD-ACTION does not exist

### Meaning

The STD-ACTION specified in the command is not known
to PROP-XT.

### Response

Check and correct the name specified for the STD-ACTION.

## POP0904

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0904 Internal error. STD-ACTION could not be deleted

### Meaning

Errors occurred in PROP-XT (resource bottleneck, data inconsistency).

## POP0906

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0906 None of specified STD-ACTIONs exists

### Meaning

Specified STD-ACTIONs are not signed on to PROP-XT.

### Response

Correct the names of the specified STD-ACTIONs.

## POP0907

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0907 Not all specified STD-ACTIONs exist

### Meaning

Not all specified STD-ACTIONs are signed on to PROP-XT.

### Response

Check the names of the STD-ACTIONs and retry command.

## POP0908

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0908 Internal error. Administration entity could not be accepted

### Meaning

Errors occurred in PROP-XT (resource bottleneck, data inconsistency).

## POP0909

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0909 Internal error. Administration entity could not be deleted

### Meaning

Errors occurred in PROP-XT (resource bottleneck, data inconsistency).

## POP0910

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0910 Specified type of STD-ACTION administration entity not supported

### Meaning

Specified type is not supported in this PROP-XT version.

### Response

Change the administration entity type.

## POP0911

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0911 No administration object specified in command exists

### Meaning

None of the administration objects specified in the
command is signed on to PROP-XT.

### Response

Correct names of administration objects.

## POP0912

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP0912 Not all administration objects exist

### Meaning

Not all the administration objects specified in the
command are signed on to PROP-XT.

### Response

Correct names of administration objects.

## POP0913

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP0913 No administration object defined

## POP9A01

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

POP9A01 PROP-XT Administration process '(&01)' started

### Meaning

Command BEGIN-PROP-PROCESS executed.

## POP9A02

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

POP9A02 PROP-XT Administration process '(&01)' terminated

### Meaning

Command END-PROP-PROCESS executed.

## POP9A04

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP9A04 Event '(&01)' not known

## POP9A06

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP9A06 Connection to administration entity '(&01)' not active

## POP9A07

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

POP9A07 Administration entity '(&01)' not defined for administration process

## POP9A11

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

POP9A11 START-PROP-OBJECT-MONITORING executed for '(&00)'; Partner: (&01)/(&02)

### Meaning

(&00) - Object name
(&01) - Name of partner application or *FROM-DB
(&02) - Processor name of partner application or
*LOCAL or *FROM-DB

## POP9A12

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

POP9A12 STOP-PROP-OBJECT-MONITORING executed for '(&00)'

### Meaning

(&00) - Object name or *ALL

## POP9A13

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

POP9A13 Connection to PROP administration object '(&00)' broken

### Meaning

(&00) - Object name

## POP9A14

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9A14 Task terminating due to MSCF request

### Meaning

MSCF is terminating abnormally because of serious
problems. The task locks a shared PVS that is to
be exported, and therefore must be terminated.

## POP9B01

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9B01 COMMAND SERVER NOT FOUND

### Meaning

The command server was not found in the PROP-XT
command list or the command server is not active
or the entered command is ambigous from SDF point
of view.

## POP9B02

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9B02 COMMAND COULD NOT BE TRANSMITTED TO SERVER

### Meaning

A bourse error occured during the transmittal of
the command to the server procedure.

## POP9B03

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9B03 COMMAND SERVER TERMINATED

### Meaning

The PROP-XT administration process that had been
the server of this command, has terminated.

## POP9F01

Destination: CONSOLE Routing code: R Weight: 50

Warranty : YES

POP9F01 Connection to administration entity '(&01)' could not be established

### Meaning

No connection could be established to the administration
entity specified in the STD-ACTION.

## POP9F02

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9F02 Loss of connection to administration entity '(&01)' of STD-ACTION

### Meaning

Loss of data must be anticipated. PROP-XT initiates
connection setup automatically when this is required.

## POP9500

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9500 PROP-XT cannot be administered

### Meaning

The administration connection to the local
application $CONSOLE could not be established
or is refused, or some error occured during the
command connection of the PROP-XT administration
commands.

### Response

Check if BCAM is ready and the PROP-XT
administration commands are not occupied by any
other appliction (command SHOW-CMD-ATTRIBUTES).

## POP990A

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP990A Error in command analysis for user '(&01)'

### Meaning

Check whether the command is contained in the relevant SDF syntax
file. As command analysis of PROP-XT user commands is performed
in both the command originator's environment and in the command-
processing administration procedure, you are notified here of
the environment in which errors occurred.

## POP990C

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP990C Administration object '(&01)' not known

### Meaning

Specified object is not signed on to PROP-XT.

### Response

Correct the object name in the command.

## POP9900

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9900 All PROP-XT administration commands available

### Meaning

PROP-XT can now be administered.

## POP9902

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9902 STD-ACTION '(&01)' not known

### Meaning

STD-ACTION is not signed on to PROP-XT.

### Response

Sign on STD-ACTION or correct name of STD-ACTION in command.

## POP9903

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9903 No administration process found

### Meaning

No administration process is signed on to PROP-XT.

## POP9904

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9904 Administration process '(&01)' not known

### Meaning

Specified process is not signed on to PROP-XT.

### Response

Correct the process name in the command.

## POP9905

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9905 No administration entity exists for administration process '(&01)'

### Meaning

The specified administration process is not
monitoring any administration entities.

## POP9906

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9906 No event exists for administration process '(&01)'

### Meaning

Specified administration process is not monitoring any events.

## POP9908

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9908 Administration process '(&01)' could not be notified

### Meaning

The specified administration process could not be notified
by setting a return code.

## POP9909

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

POP9909 Administration process '(&01)' could be notified

### Meaning

The specified administration process was notified by
setting a return code.

©2025 Fujitsu | BS2000 System Messages