## NPSCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPSCOPY Copyright (C) (&01) (&00). All rights reserved

## NPSLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPSLOAD Program '(&00)', Version '(&01)' of '(&02)' loaded from file '(&03)'

## NPSSTRT

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPSSTRT Procedure '(&00)', Version '(&01)' of '(&02)' started from file '(&03)'

## NPS0001

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0001 PRIVILEGE ERROR. STATEMENT REJECTED

### Meaning

Possible reasons:
- A user without privilege "Software Monitor Administration" tried to
enter a privileged SM2 statement.
- A user who is not the primary SM2 administrator tried to enter
a privileged SM2 statement, which is reserved to the primary
administrator.
- A privileged user, who is not SM2 administrator tried to enter a
SM2 statement, which is reserved to the administrators.

## NPS0002

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0002 NO MORE FILES PERMITTED FOR FILE MONITORING

### Meaning

SM2 is already monitoring 32 files.

## NPS0003

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0003 USER NOT AUTHORIZED TO MONITOR FILES. STATEMENT REJECTED

### Meaning

The SM2 administrator has not (yet) permitted file monitoring
for this user.

## NPS0005

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0005 SM2 SYSTEM CODE LOCKED. SM2 RUN ABORTED. TRY AGAIN LATER

### Meaning

A serialization lock in the SM2 system code was not released after
a certain time.

## NPS0006

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0006 MEASUREMENT DATA MAY BE INCONSISTENT. no data for output

### Meaning

The data collected during the last monitoring cycle may be inconsistent
because of bottlenecks.

## NPS0009

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0009 USER NOT AUTHORIZED TO SUBMIT OR WITHDRAW SPECIFIED FILE

## NPS0010

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0010 FILE NOT SUBMITTED

### Meaning

A user tried to withdraw a file from monitoring which had not been
submitted in the first place.

## NPS0011

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0011 SYNTAX ERROR. STATEMENT CONTAINS INVALID OPERAND(S)

### Meaning

The statement has been rejected.

## NPS0012

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0012 SYNTAX ERROR. OUTPUT CYCLE NOT IN PERMITTED RANGE

### Meaning

The specified output cycle is not in the permitted range from 10 to
3600 seconds.
The statement has been rejected.

## NPS0014

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0014 STATEMENT UNKNOWN

## NPS0015

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0015 SYNTAX ERROR. STATEMENT CONTAINS INVALID OPERAND(S) '(&00)'

### Meaning

The statement has been rejected.

## NPS0016

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0016 NO REPORTS SELECTED FOR OUTPUT

### Meaning

Report output cannot be started until the appropriate reports have been
selected.

## NPS0018

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0018 SYNTAX ERROR. OPERAND MISSING

### Meaning

A statement has been entered without an essential operand.
The statement has been rejected.

## NPS0020

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0020 SYNTAX ERROR. INVALID LIST FORMAT

### Meaning

A list was specified in a statement which does not have the expected
format (e.g. ')' missing).
The statement has been rejected.

## NPS0021

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0021 SYNTAX ERROR. PERMITTED NUMBER OF LIST ELEMENTS EXCEEDED FROM '(&00)' OPERAND VALUE ONWARDS

### Meaning

The statement has been rejected.

## NPS0022

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0022 SYNTAX ERROR IN '(&00)' OPERAND VALUE

### Meaning

The statement has been rejected.

## NPS0023

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0023 SYNTAX ERROR. '(&00)' OPERAND TOO LONG

### Meaning

The statement has been rejected.

## NPS0024

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0024 SYNTAX ERROR. TOO MANY LIST ELEMENTS

### Meaning

Too many list elements were specified in a statement.
The statement has been rejected.

## NPS0025

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0025 SYNTAX ERROR. '(&00)' OPERAND TERMINATED INCORRECTLY

### Meaning

An improperly terminated operand (e.g. comment) was entered in a
statement.
The statement has been rejected.

## NPS0026

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0026 SYNTAX ERROR. INVALID KEYWORD '(&00)'

### Meaning

The statement has been rejected.

## NPS0027

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0027 DUPLICATE OR INCOMPATIBLE KEYWORD(S) '(&00)'

### Meaning

Possible reasons:
- a keyword was entered several times in the same statement,
- mutually exclusive keywords were specified.
The statement has been rejected.

## NPS0028

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0028 MAXIMUM WAITTIME IS REACHED. TRY AGAIN LATER.

### Meaning

Because of bottlenecks some instructions couldn't be executed within
timelimit.

## NPS0029

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0029 KEYWORDS NOT ALLOWED IN LIST

### Meaning

The keyword is not allowed in list.

## NPS0031

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0031 SYNTAX ERROR. STATEMENT TOO LONG

### Meaning

A statement is not allowed to have more than 1536 characters
inclusive all continuation lines.
Strings of blanks are counted as one character.
The statement has been rejected.

## NPS0032

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0032 SYNTAX ERROR. INPUT LINE LONGER THAN 256 CHARACTERS

### Meaning

The statement has been rejected.

## NPS0033

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0033 UNEXPECTED END OF INPUT FILE

### Meaning

Possible reasons:
- An end-of-file condition was encountered in batch mode.
- In interactive mode with statement input from a file, an end-of-file
condition was encountered when attempting to read a continuation line.
If the end-of-file condition is encountered while reading the first
line of a statement, SYSDTA is set to (PRIMARY) without this message
being displayed.

## NPS0035

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0035 INVALID BS2000 COMMAND

### Meaning

An invalid BS2000 command has been issued as an SM2 statement in batch
mode.

## NPS0036

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0036 '(&00)' MACRO ERROR. RETURN CODE '(&01)'

### Meaning

An error has occurred during execution of the specified macro.
Depending on the error, SM2 either continues program execution, i.e.
requests a corrected statement via ENTER COMMAND, or terminates.
(&01): return code of the macro (cf. the 'Executive Macros' manual).

## NPS0037

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0037 SM2 TERMINATED NORMALLY

## NPS0038

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0038 SM2 TERMINATED ABNORMALLY

### Meaning

A serious program error has occurred, leading to immediate program
termination.

## NPS0039

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0039 FORMATTED OUTPUT ONLY POSSIBLE TO SYSLST

### Meaning

Terminal output is not possible because:
- SM2 is running in batch mode, or
- the terminal has less than 80 columns, or
- the terminal has less than 24 lines.
Screen and status diagrams are put out to SYSLST.

## NPS0040

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0040 SM2 STXIT: CLASS=(&00), CODE=(&01), LOCATION=(&02). PROGRAM RUN ABORTED

### Meaning

An error has occurred in the unprivileged program part of SM2.
CLASS : event class.
CODE : error weight.
LOCATION: program counter of the location at which the error occurred.
For further information on the STXIT routine see the 'Executive
Macros' manual.

## NPS0041

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0041 TOO MUCH USERS WANT TO MONITOR THE SAME FILE

### Meaning

Maximal 64 users can monitor the same file at the same time.

## NPS0042

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0042 Invalid Input! Only +,-,-- or end allowed !

## NPS0044

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0044 USER NOT AUTHORIZED TO MONITOR TASK. COMMAND REJECTED

### Meaning

The SM2 administrator has not permitted task monitoring. As a result,
monitoring of the user task either cannot be started or can no longer
be stopped by the user.
If the user himself started the monitoring of his task by means of a
/START-TASK-MEASUREMENT command, monitoring has already been terminated
by the SM2 administrator.

## NPS0045

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0045 TASK ALREADY BEING MONITORED BY SM2

### Meaning

Monitoring of the task has already been started either by the user via
the /START-TASK-MEASUREMENT command or by the SM2 administrator.

## NPS0046

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0046 TASK MONITORING NOT INITIATED BY '/START-TASK-MEASUREMENT'. COMMAND REJECTED

### Meaning

Task monitoring cannot be terminated, either because it was not
started by the /START-TASK-MEASUREMENT command or because it has
already been terminated in the meantime (e.g. due to withdrawal of
permission to monitor the task or to SM2 shutdown).

## NPS0047

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0047 SPECIFIED TASK DOES NOT EXIST

### Meaning

A TSN was specified for which no task exists.

## NPS0048

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0048 COMMAND EXECUTED. TASK MONITORING STARTED ON (&00)

### Meaning

(&00): time stamp for the start of monitoring, in the format
YYYY-MM-DD HH:MM:SS.
Note:
Precisely this time stamp will be put out in the task analysis conducted
by the SM2-PA analysis routine.

## NPS0049

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0049 COMMAND EXECUTED. TASK MONITORING TERMINATED ON (&00)

### Meaning

(&00): time stamp for the end of monitoring, in the format
YYYY-MM-DD HH:MM:SS.
Note:
Precisely this time stamp will be put out in the task analysis conducted
by the SM2R1 analysis routine.

## NPS0050

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0050 SYSTEM ERROR IN SM2 MODULES. COMMAND REJECTED

### Meaning

A system error has occurred in SM2 during program execution. As a
result, task monitoring cannot be started after the
/START-TASK-MEASUREMENT
command or no task record 27 can be written to the userspecific
SM2 logging file after the /STOP-TASK-MEASUREMENT command.

### Response

Contact the SM2 administrator. He can determine the detailed error
cause using the trace entries of the //SHOW-SM2-STATUS function.
In that case he is able to clear away the difficulties or he can
produce detailed diagnostic material.

## NPS0051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0051 SPECIFIED TASK MUST NOT BE MONITORED BY USER

### Meaning

The specified TSN belongs to a task under a foreign user id.
Start and termination of monitoring foreign tasks is only permitted
for users with privilege SW-MONITOR-ADMINISTRATION.

## NPS0052

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0052 TOO MANY OBJECTS SPECIFIED FOR MONITORING. STATEMENT REJECTED

### Meaning

An ADD statement with an object list has been specified. Together with the
preceding ADD statements of the same kind the total number of objects
is greater than the maximum number of objects that may be specified.

## NPS0053

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0053 TOO MANY POOLS SUBMITTED FOR ISAM POOL MONITORING. STATEMENT REJECTED

### Meaning

There can be defined only in each case up to 16 ISAM pools over the
pool names or the file names.

## NPS0054

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0054 ISAM POOL NOT SUBMITTED. STATEMENT REJECTED

### Meaning

A user tried to withdraw an ISAM POOL from monitoring which had not
been submitted before.

## NPS0055

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0055 USER NOT AUTHORIZED TO MONITOR ISAM BUFFERS. STATEMENT REJECTED

### Meaning

The SM2 administrator has not permitted ISAM buffer monitoring. As a
result, monitoring of the ISAM buffers either cannot be started or
can no longer be terminated by the user.

## NPS0056

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0056 SYNTAX ERROR. LIST CONTAINS DOUBLE ELEMENTS. STATEMENT REJECTED

### Response

Correct the statement and try again.

## NPS0057

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0057 SYNTAX ERROR. LIST ELEMENTS NOT DEFINED IN ASCENDING ORDER. STATEMENT REJECTED

### Response

Correct the statement and try again.

## NPS0058

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0058 SYNTAX ERROR. AT LEAST ONE OPERAND MUST BE SPECIFIED. STATEMENT REJECTED

### Response

Correct the statement and try again.

## NPS0059

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0059 ONLY '*' AT END OF EXPRESSION PERMITTED AS WILDCARD HERE. STATEMENT REJECTED

### Response

Correct the statement and try again.

## NPS0060

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0060 SYSTEM ERROR DURING PROCESSING OF SDF STATEMENTS. SDF RETURN CODE '(&00)'

## NPS0061

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0061 SDF SYNTAX FILE DEFECTIVE OR INCORRECTLY ACCESSED. CONTACT SYSTEM ADMINISTRATOR

### Meaning

Either no SDF syntax file has been assigned or the one assigned is
invalid or cannot be accessed.

## NPS0065

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0065 NO MORE TASKS CAN BE MONITORED

### Meaning

The maximum possible number of tasks which can be monitored by
SM2 has been exceeded.

### Response

Either withdraw other tasks from monitoring or wait until some have
terminated, and then try the command again.

## NPS0066

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0066 INVALID FILE ATTRIBUTES SPECIFIED FOR USERSPECIFIC SM2 LOGGING FILE

### Meaning

Invalid file attributes have been specified for the userspecific SM2
logging file regarding the block size, record format, FCB type
or open type.

## NPS0067

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0067 DMS CODE '(&00)' WITH MACRO CALL '(&01)' FOR USERSPECIFIC SM2 LOGGING FILE

### Meaning

The userspecific SM2 logging file assigned either by LINK=PALINK or by
default (SM2.TASKSTATISTIK.<tsn>) cannot be processed correctly.
For more detailed information about the DMS error code enter /HELP-MSG
or see the BS2000 manual 'System Messages'.

### Response

Check the SM2 logging file, and assign another one if necessary.

## NPS0400

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0400 WARNING: ERROR DURING RESTART OF MONITORING PROGRAMS '(&00)'

### Meaning

The monitoring programs '(&00)' couldn't be restarted after reopen of
measurement file.

### Response

Check monitoring program definitions and start monitoring programs with
//START-MEASUREMENT-PROGRAM statement.

## NPS0501

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0501 ERROR DURING PROCESSING OF SM2 LOGGING FILE: DMS CODE '(&00)'

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## NPS0502

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0502 SYSTEM ERROR ON CALLING SM2

### Meaning

A serious error has occured when calling SM2
Possible reasons:
- an unexpected return code was delivered when calling an internal
BS2000 system function.
- SM2 itself detected an inconsistency in its own logic.
The statement has been rejected.

### Response

Contact the SM2 administrator. He can determine the detailed error
cause using the trace entries of the //SHOW-SM2-STATUS function.
In that case he is able to clear away the difficulties or he can
produce detailed diagnostic material.

## NPS0504

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0504 SYSTEM ERROR DURING SM2 RUN: CODE=(&00), SUBCODE=(&01)

### Meaning

This message is only put out during test phase of SM2.

## NPS0507

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0507 SYNTAX ERROR. CYCLE NOT IN PERMITTED RANGE

### Meaning

Possible reasons:
- The specified monitoring cycle is not in the permitted range from 10
to 3600 seconds.
- The specified sampling cycle is not in the permitted range from 200
to 10000 milliseconds.
The statement has been rejected.

## NPS0514

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0514 SM2 LOGGING FILE SPECIFIED VIA LINK NAME AND NO CORRESPONDING /SET-FILE-LINK COMMAND ENTERED

### Meaning

The SM2 administrator has failed to define a /SET-FILE-LINK command for
the file attributes of the SM2 logging file.

### Response

Enter a /SET-FILE-LINK command with LINK-NAME=SMLINK and try again.

## NPS0515

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0515 SM2 SUBSYSTEM NOT AVAILABLE

### Meaning

A non-privileged user has tried to start SM2 before the system
administrator or a SM2 administrator had started the subsystem SM2 or
subsystem SM2 was terminated during connection of user.

## NPS0516

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0516 REQUIRED MODULES COULD NOT BE LOADED

### Meaning

Certain monitoring program modules could not be loaded.
The return code of the loader function can be obtained by the
SM2 administrator using the trace entries of the //SHOW-SM2-STATUS
statement.

## NPS0517

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0517 VERSION OF SM2 TU PART NOT SUPPORTED BY THE VERSION OF SM2 MODULE LIBRARY. SM2 TERMINATED ABNORMALLY.

### Meaning

It was tried to start a newer SM2 TU part with an older version of
SM2 module library, which doesn't support the version of SM2 TU part.

### Response

Check the version number, if necessary unload subsystem SM2 and start
it new.

## NPS0518

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0518 CONFIGURATION RECORD COULD NOT BE WRITTEN

### Meaning

This message is for diagnostic purposes only.
The configuration record could not be written either because certain
resources were missing or because of a system error.

## NPS0520

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0520 ONLY 'RECORD-FORMAT=VARIABLE' PERMITTED FOR SM2 LOGGING FILE. STATEMENT REJECTED

### Meaning

The value of the RECORD-FORMAT operand in the /SET-FILE-LINK command for a
non-standard SM2 logging file is invalid.

## NPS0521

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0521 ONLY 'BUFFER-LENGTH=*STD(SIZE=16)' PERMITTED FOR SM2 LOGGING FILE. STATEMENT REJECTED.

### Meaning

SM2 logging files are only permitted with 'BUFFER-LENGTH=*STD(16)'.
The value of the BUFFER-LENGTH operand in the /ADD-FILE-LINK command
for a non-standard SM2 logging file is invalid or the existing
non-standard SM2 logging file has wrong BUFFER-LENGTH.

### Response

Retry the /ADD-FILE-LIND command without the BUFFER-LENGTH operand
and then retry OPEN-LOG-FILE statement.
If you want to open extend a non-standard SM2 logging file of an older
SM2 version, you first have to convert the file with SM2U1.

## NPS0522

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0522 SM2 LOGGING FILE NOT OPENED. STATEMENT REJECTED

### Meaning

An attempt was made to start a monitoring program while the SM2
logging file was not opened.

## NPS0523

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0523 MONITORING PROGRAM '(&00)' NOT DEFINED. STATEMENT REJECTED

### Meaning

An attempt was made to start a non-defined monitoring program.

## NPS0524

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0524 MONITORING PROGRAM '(&00)' ALREADY ACTIVE. STATEMENT REJECTED

### Meaning

An attempt was made to start a monitoring program that has already
been started.

## NPS0526

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0526 TSN '(&00)' NOT IN SYSTEM. STATEMENT REJECTED

### Meaning

An attempt was made to start TASK measurement for a specific task,
but the corresponding task could not be found in the system at the time.

## NPS0527

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0527 SYNTAX ERROR. UNKNOWN MONITORING PROGRAM SPECIFIED

### Meaning

The statement has been rejected.

## NPS0528

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0528 INVALID DEVICE/PUBSET DEFINITION SPECIFIED FOR DEVICE/PUBSET '(&00)'. STATEMENT REJECTED.

### Meaning

When defining a monitoring program, an attempt was made to specify
a device/pubset that is not valid for this program.
Possible reasons:
- device is unknown
- device is not a disk or not attached
(only measurement program SERVICETIME)
- pubset is exported or unknown or a volume set

### Response

Check and correct monitoring program definition.

## NPS0529

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0529 INVALID CHANNEL DEFINITION SPECIFIED FOR CHANNEL NUMBER '(&00)'

### Meaning

When defining a monitoring program, an attempt was made to specify an
invalid channel number.
The statement has been rejected.

## NPS0530

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0530 MONITORING PROGRAM '(&00)' INVALID DEFINED. STATEMENT REJECTED.

### Meaning

It was attempted to start a monitoring program with
invalid devices/pubsets.
Possible reasons:
- device is not any more in the configuration
- device is not in the status 'attached'
(only for measurement program SERVICETIME)
- pubset is exported or unknown or volume set

### Response

Check and correct monitoring program definition.

## NPS0531

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0531 WARNING: MONITORING PROGRAM '(&00)' PARTLY INVALID DEFINED. INVALID DEVICES/PUBSETS IGNORED.

### Meaning

While starting a monitoring program, it was found that some invalid
devices/pubsets were selected. The monitoring program is only
started with the valid devices/pubsets; the invalid devices/pubsets
are not monitored.
Possible reasons:
- device is not any more in the configuration
- pubset is exported or unknown or volume set

## NPS0533

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0533 SYSTEM ERROR IN '/START-TASK-MEASUREMENT' OR '/STOP-TASK-MEASUREMENT' COMMAND: CODE=(&00)

### Meaning

This message is for diagnostic purposes only.

## NPS0534

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0534 MONITORING PROGRAM '(&00)' NOT COMPLETELY DEFINED. STATEMENT REJECTED.

### Meaning

An attempt was made to start a not completely defined monitoring program.

### Response

Define montoring program completely and repeat statement.

## NPS0535

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0535 '//SET-BCAM-CONNECTION-PARAMETERS' STATEMENT NOT SPECIFIED. STATEMENT REJECTED.

### Meaning

The //ADD-BCAM-CONNECTION-SET statement cannot be specified unless
//SET-BCAM-CONNECTION-PARAMETERS statement is specified first.

### Response

Enter the //SET-BCAM-CONNECTION-SET-PARAMETERS statement and repeat your
original entry.

## NPS0536

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0536 MORE THAN 32 CONNECTION SETS DEFINED. STATEMENT REJECTED.

### Meaning

Maximal 32 connection sets can be monitored by measurement program
BCAM-CONNECTION. Statement rejected.

### Response

Use the //REMOVE-BCAM-CONNECTION-SET statement to terminate monitoring
of superfluous connection sets and repeat your original entry.

## NPS0537

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0537 NAME OF CONNECTION SET INVALID. STATEMENT REJECTED.

### Meaning

Possible reasons:
- The specified name in the //ADD-BCAM-CONNECTION-SET statement is
already defined.
- The specified name in the //REMOVE-BCAM-CONNECTION-SET statement does
not exist.

## NPS0538

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0538 CONNECTION SET DEFINITION IS ALREADY EXISTING. STATEMENT REJECTED.

### Meaning

There is already a connection set defined that monitors the same
connections.

## NPS0539

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0539 WARNING: NO CONNECTION SET REMOVED

### Meaning

The specified connection set does not exist.

## NPS0540

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0540 VERSIONS OF SM2 AND VM2000 ARE INCOMPATIBLE. STATEMENT REJECTED

### Meaning

The measurement program VM cannot fetch any VM data.

## NPS0541

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0541 INVALID TASK DEFINITION SPECIFIED FOR TSN '(&00)'

### Meaning

When defining a monitoring program, an attempt was made to specify a
task that is not valid for this program.
The statement has been rejected.

## NPS0542

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0542 WRONG BUCKET VALUES. STATEMENT REJECTED.

### Meaning

Only 1-4 buckets values may be specified in a list.
The values must be in ascending order.
Permissible value range: 1 to 999999.
The statement has been rejected.

## NPS0543

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0543 SM2 MONITORING TASK NOT WORKING CORRECTLY

### Meaning

Possible reasons:
- The SM2 monitoring task failed to answer a user request within a
given time.
- The SM2 monitoring task has already been terminated due to an
unrecoverable internal error.

### Response

A non-privileged user can check the SM2 status using the SM2 STATUS
statement, and should then
contact the SM2 administrator if this is necessary.
The SM2 administrator can check the status of the SM2
using the //SHOW-SM2-STATUS statement, and can then terminate and restart
the subsystem if this is necessary.

## NPS0544

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0544 SM2 VERSION (&00) AND BS2000 VERSION (&01) ARE INCOMPATIBLE. SM2 CANNOT BE LOADED

### Meaning

The version number (&00) of modules in the SM2 module library and the
version number (&01) of the operating system do not match.

## NPS0545

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0545 VERSIONS OF SM2 TU PART (&00) AND SM2 MODULE LIBRARY (&01) ARE INCOMPATIBLE. SM2 TERMINATED ABNORMALLY

### Meaning

The version number (&00) of the TU part of SM2 and the version number
(&01) of modules in the SM2 module library do not match.

## NPS0546

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0546 WRONG BCAM-VERSION. STATEMENT REJECTED.

### Meaning

The measurement program BCAM-CONNECTION cannot fetch any data by this
BCAM-Version.

## NPS0547

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0547 MONITORING PROGRAM '(&00)' WAS NOT ACTIVE

### Meaning

The SM2 administrator has tried to deactivate or modify a monitoring
program that has not been activated.
The statement has been rejected.

## NPS0548

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0548 WARNING: MONITORING PROGRAM '(&00)' STARTED, BUT ACCORDING SUBSYSTEM NOT LOADED IN SYSTEM

### Meaning

SM2 gets not the measurement data from the specified subsystem. As far
as this is not available, SM2 cannot deliver any measurement data.

### Response

Contact the system administrator, so that he can start the required
subsystem, or stop the monitoring program to save resources.

## NPS0549

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0549 START OF SERVICETIME MEASUREMENT NOT POSSIBLE. TRY START AGAIN LATER

### Meaning

It is not possible to start SERVICETIME measurement at the moment
because the previous measurement run has not yet been completed.

### Response

The statement //START-MEASUREMENT-PROGRAM TYPE=SERVICETIME may be repeated
later.

## NPS0550

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0550 WARNING: TASK MEASUREMENT STARTED WITHOUT RECORDING OF BCAM MONITORED DATAS

### Meaning

Some monitored datas cannot be recorded for TASK measurement,
because the subsystem BCAM-SM2 could not be loaded or initiated.

## NPS0552

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS0552 '/HOLD-SUBSYSTEM' NOT SUPPORTED BY SM2. REASON FOR FOLLOWING DSSM MESSAGES

### Response

Instead of /HOLD-SUBSYSTEM command use /STOP-SUBSYSTEM command.

## NPS0553

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0553 START OF SM2 SUBSYSTEM NOT POSSIBLE

### Meaning

Possible reasons:
- SM2 has not been declared in the subsystem catalog.
- The installed SM2 version is not compatible with the BS2000 version.
- A required file (e.g. the SM2 module library) is missing.

## NPS0554

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS0554 FUNCTION NOT EXECUTED BECAUSE SUBSYSTEM SM2 IN STATE 'IN HOLD', 'IN DELETE' OR ALREADY DELETED

### Meaning

The system administrator has held or stopped the SM2 subsystem.
As a result, a number of SM2 functions can no longer be executed.

### Response

Repeat the function as soon as SM2 is available again.

## NPS0555

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS0555 VERSION OF SM2 SUBSYSTEM (TPR PART) IS (&00)

## NPS0558

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS0558 SM2 LOGGING FILE ALREADY OPEN. STATEMENT REJECTED

### Meaning

A non-standard SM2 logging file with the specified name has already
been opened.

## NPS0559

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0559 WARNING: MORE THAN THE MAXIMUM ALLOWED NUMBER DEVICES FOR A MEASUREMENT PROGRAM SELECTED AND INVALID DEVICES IN WILDCARD LIST. SURPLUS AND INVALID DEVICES IGNORED.

### Meaning

With a measurement program definition were devices with wildcards
and/or pubsets selected.
The maximum admissible number of devices for a measurement program
was exceeded.
The measurement program is started with the maximum admissible amount
of devices. The surplus devices are not monitored.
The criteria for selecting the devices are described in the
BS2000 manual 'SM2'.
Moreover there were invalid devices in the wildcard list.
Possible reasons:
- device is no disk
Invalid devices are not monitored.

## NPS0560

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0560 MONITORING PROGRAM RECORD COULD NOT BE WRITTEN. TRY AGAIN LATER

### Meaning

Collection of statistics has not been activated.

## NPS0561

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0561 WARNING: MORE THAN THE MAXIMUM ALLOWED NUMBER DEVICES FOR A MEASUREMENT PROGRAM SELECTED. SURPLUS DEVICES IGNORED.

### Meaning

With a measurement program definition were devices with wildcards
and/or pubsets selected.
The maximum admissible number of devices for a measurement program
was exceeded.
The measurement program is started with the maximum admissible amount
of devices. The surplus devices are not monitored.
The criteria for selecting the devices are described in the
BS2000 manual 'SM2'.

## NPS0562

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0562 OPERATING SYSTEM RUNNING IN NATIVE MODE. VM MEASUREMENT NOT AVAILABLE. STATEMENT REJECTED

### Meaning

VM measurement cannot be activated as no VM2000 system
is currently being used.

## NPS0564

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0564 WARNING: INVALID DEVICES IN WILDCARD LIST OR FOR PUBSETS FOUND. INVALID DEVICES IGNORED.

### Meaning

With a measurement program definition were devices with wildcards
and/or pubsets selected.
With the resolve of the wildcards and/or pubsets were invalid
devices found.
Possible reasons:
- device is no disk or not attached
(only mesurement program SERVICETIME)
The invalid devices are not monitored.

## NPS0565

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0565 SYNTAX ERROR. INVALID BUCKET VALUES

### Meaning

Only 1-5 bucket values may be specified in a list.
The values must be in ascending order.
Permissible value range: 1 to 99999.
The statement has been rejected.

## NPS0566

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0566 NAME OF CONNECTION SET INVALID

### Meaning

Possible reasons:
- The specified name has not been defined in the statement
//REMOVE-CONNECTION-SET.
- The specified name has already been defined in the statement
//ADD-CONNECTION-SET.
The statement has been rejected.

## NPS0567

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0567 '//SET-RESPONSETIME-PARAMETER' STATEMENT NOT SPECIFIED. STATEMENT REJECTED

### Meaning

The //MODIFY-RESPONSETIME-PARAMETER or //ADD-CONNECTION-SET
statement cannot be specified unless
//SET-RESPONSETIME-PARAMETER statement is specified first.
The statement has been rejected.

### Response

Enter the //SET-RESPONSETIME-PARAMETER statement and repeat
your original entry.

## NPS0568

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0568 MORE THAN 15 CONNECTION SETS DEFINED

### Meaning

The connection set '*GLOBAL=(*ALL, *ALL, *ALL)' is always
defined additionally.
The statement has been rejected.

### Response

Use the //REMOVE-CONNECTION-SET statement to terminate monitoring of
superfluous connection sets and repeat your original entry.

## NPS0569

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0569 MORE THAN 15 CONNECTION GROUPS DEFINED

### Meaning

'(*ALL, *ALL, *ALL)' is always defined additionally as a connection
group.
The statement has been rejected.

### Response

Use the //REMOVE-CONNECTION-SET statement to terminate monitoring of
superfluous connection groups and repeat your original entry.

## NPS0571

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0571 SYNTAX ERROR. INVALID SORT CRITERION IN '//SET-PERIODIC-TASK-PARAMETER STATEMENT'

### Meaning

The statement has been rejected.

## NPS0572

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS0572 WARNING: USER TASK MONITORING STARTED WITHOUT RECORDING OF BCAM MONITORING DATAS

### Meaning

Some monitored datas cannot be recorded for user task monitoring,
because the subsystem BCAM-SM2 could not be loaded or initiated.

## NPS0573

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0573 INCONSISTENT OPERAND VALUES FOR ISAM POOL DEFINITION

### Meaning

The statement has been rejected.

## NPS0574

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS0574 FILE ALREADY SUBMITTED FOR MONITORING

### Meaning

The statement has been rejected.

## NPS0575

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0575 Subsystem SM2 is terminated abnormally.

### Meaning

A systemdump is created.

### Response

Contact your systemadministrator.

## NPS0576

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS0576 ISAM POOL ALREADY BEING MONITORED. STATEMENT REJECTED

### Meaning

The ISAM pool submitted by the user for ISAM pool monitoring
is already being monitored.

## NPS0577

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0577 TOO MUCH USERS MONITOR THE SAME ISAM POOL

### Meaning

Maximal 64 users can monitor the same ISAM POOL at the same time.
Statement rejected.

## NPS0578

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS0578 INVALID CACHE-ID. PERMISSIBLE VALUE RANGE: 0 TO 62

### Meaning

The statement has been rejected.

## NPS0579

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0579 INVALID OBJECT SPECIFICATION IN '//SET-PERIODIC-TASK-PARAMETER' STATEMENT

### Meaning

The statement has been rejected.

## NPS0580

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0580 INVALID FILENAME

### Meaning

Possible reasons: The filename is invalid, because
- the specified USER ID doesn't exist,
- the filename is too long,
- the complete filename with CAT ID and USER ID is too long,
- the filename with relative FGG is not cataloged.

## NPS0581

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0581 USER ID(S) '(&00)' DO NOT EXIST. STATEMENT REJECTED

### Meaning

With a measurement program definition was an USER-ID defined,
that does not exit.

## NPS0582

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0582 SM2 WRITETASK IS TERMINATED ABNORMALLY.

### Meaning

The writetask SM2W does not react any longer and is therefore
terminated. Possibly before the message NPS0501 with a DMS error
code is output at the console.

## NPS0583

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0583 INSTANCE NOT SUBMITTED

### Meaning

A user tried to withdraw an instance from monitoring which had not been
submitted in the first place. The statement has been rejected.

## NPS0584

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0584 NO MORE INSTANCES PERMITTED FOR MONITORING

### Meaning

There can be defined only up to 16 instances. The statement has been
rejected.

## NPS0585

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0585 INSTANCE ALREADY SUBMITTED FOR MONITORING

### Meaning

The statement has been rejected.

## NPS0586

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0586 WARNING: MONITORING OF SPECIFIED INSTANCE NOT POSSIBLE

### Meaning

For the specified instance no monitoring values can be supplied.
Possible reasons:
- The specified instance does not exist
- The recording of the monitoring values is not activated in openFT
for the instance
- The available version of openFT does not support the monitoring of
instances
- The subsystem openFT has not been started

## NPS0590

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0590 MONITORING PROGRAM '(&00)' INVALID DEFINED. STATEMENT REJECTED

### Meaning

It was attempted to start a monitoring program with invalid channels.
Invalid channels are:
- Channels, which are not any more in the configuration

### Response

Check and correct monitoring program definition.

## NPS0591

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0591 WARNING: MONITORING PROGRAM '(&00)' PARTLY INVALIDLY DEFINED. INVALID CHANNELS IGNORED

### Meaning

While starting a monitoring program, it was found that some invalid
channels were selected. The monitoring program is only started with
the valid channels; the invalid channels are not monitored.
Invalid channels are:
- Channels, which are not any more in the configuration

## NPS0592

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0592 WARNING: TSN(S) '(&00)' NOT IN SYSTEM. MONITORING NOT STARTED FOR THIS TASK(S)

### Meaning

The specified TSN '(&00)' could not be found in the system at the time.
No monitoring started for this task.

## NPS0593

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0593 WARNING: MONITORING PROGRAM SERVICETIME STARTED WITHOUT RECORDING OF THE DETAILED SERVICE TIMES

### Meaning

The function 'channel subsystem monitoring facility' is
required in order to monitore detailed service times.
This firmware feature can only ever be assigned to one
guest system under VM2000.
Another guest system already proved the function.
Only the device queue and the remaining service time
are monitored.

## NPS0594

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0594 WARNING: MONITORING PROGRAM SERVICETIME IS STARTED WITHOUT RECORDING OF THE DETAILED SERVICE TIMES FOR THE DEVICES '(&00)'

### Meaning

For certain devices the detailed service times cannot be monitored
under VM2000.
The restriction applies only to devices, which are operated with
indirect IO mode.
The restriction applies also to devices, which are not attached.
Only the device queue and the remaining service time are monitored.

## NPS0596

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0596 DEFINITION OF PARTNER/PROCESSOR LEADS TO INCORRECT MEASURED VALUES. DEFINE CONNECTION GROUP(S) WITHOUT PARTNER/PROCESSOR

### Meaning

With the definition of the connection groups applications are only
supposed to be indicated.
The selection of PARTNER/PROCESSOR leads to incorrect values.

### Response

The monitoring program BCAM-CONNECTION supports the selection of the
local and the partner application as well as the partner computer.

## NPS0597

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0597 WARNING: RECORDING OF THE DETAILED SERVICE TIMES WITH THE MONITORING PROGRAM SERVICETIME ON SYSTEMS WITH X86 ARCHITECTURE NOT POSSIBLE

### Meaning

On systems with x86 architecture the function pending,
device disconnect and device connect time cannot be supplied.
Only the device queue and the remaining service time
are monitored.

## NPS0598

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0598 WARNING: MONITORING PROGRAM VM STARTED, BUT VM2000 VIRTUAL MACHINE SYSTEM AT PRESENT NOT AVAILABLE

### Meaning

At present SM2 gets no measurement data from VM2000.
As soon as VM2000 is again available, SM2 measuring data will supply.

## NPS0599

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0599 WARNING: SM2 LOGGING FILE ALREADY OPEN. STATEMENT IGNORED

### Meaning

A non-standard SM2 logging file with the specified name has already
been opened.

## NPS0600

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS0600 UNRECOVERABLE ERROR IN SM2 MODULES

### Meaning

With this message number a SERSLOG record is written.

## NPS0603

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS0603 UNKNOWN DATA PASSED THROUGH BOURSE

### Meaning

The contents of bourse parameter RDATA is unknown to the gatherer task.
A SERSLOG record is written.

## NPS0700

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0700 HOST: '(&00)'

### Meaning

This host sends the following SM2 message.

## NPS0701

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0701 SELECTED HOST NOT AVAILABLE. STATEMENT REJECTED

### Meaning

The selected host is not available.
Possible reasons are:
- host name syntactically incorrect
- host not connected
- subsystem MSCF not available
- no host information in MSCF configuration
- SM2 version of remote host does not match
- parameters of //SELECT-HOST compete with one another
- connection to remote host interrupted
- subsystem SM2 on remote host not available

## NPS0710

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS0710 '(&01)' MACRO ERROR: '(&00)'

### Meaning

(&01) macro returns (&00).

## NPS3003

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3003 TIME STAMP '(&00)' OF INPUT FILE '(&02)' IS EARLIER THAN LAST TIME STAMP '(&01)' OF OUTPUT FILE

### Meaning

The time stamps of a SM2 logging file must be in ascending order.
The statement has been rejected.

## NPS3004

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3004 INVALID INPUT FILE '(&00)'

### Meaning

The specified input file is not
- a SM2 logging file although SM2 logging files are assumed to be handled
- a user logging file although user logging files are assumed to be
handled.
The statement has been rejected.

## NPS3006

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3006 /SET-FILE-LINK COMMAND WITH 'LINK-NAME=SM2UI1' MISSING FOR INPUT FILE

## NPS3007

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS3007 'SM2U1' UTILITY ROUTINE TERMINATED NORMALLY

### Meaning

The SM2U1 utility routine has terminated without errors.

## NPS3008

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3008 'SM2U1' UTILITY ROUTINE TERMINATED ABNORMALLY

### Meaning

A previously reported error caused the SM2U1 utility routine to be
terminated abnormally (TERMJ).

## NPS3009

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS3009 WARNING: CLOSE RECORD ADDED TO FILE '(&00)'

### Meaning

The last record in the specified file is not a CLOSE record (record
22 with CLOSE indicator).
Possible reason:
system crash during creation of the SM2 logging file.
To ensure that the monitored data are consistent, the last (possibly
incomplete) monitoring cycle of the input file is not written to the
output file. Instead, a CLOSE record with the indicator 'system
crash' is written.

## NPS3010

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS3010 FILE '(&00)' ADDED

### Meaning

The file with the specified name (&00) has been added to the output file.

## NPS3011

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS3011 START TIME=(&00), END TIME=(&01)

## NPS3012

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS3012 NUMBER OF RECORDS WRITTEN = (&00)

### Meaning

The last input file has been processed. Before the program terminates,
the user is informed of how many records have been written to the
output file.

## NPS3013

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS3013 NUMBER OF MISSING RECORDS = (&00)

### Meaning

During processing of the input file, the total number of records which
SM2 could not put out is added up. This number is put out when
processing has been completed, unless it is zero.

## NPS3014

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS3014 NAME OF OUTPUT FILE: '(&00)'

## NPS3015

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3015 INTERNAL SYSTEM ERROR DURING PROCESSING OF BS2000 MACRO '(&00)', RETURN CODE '(&01)'

### Meaning

This message is for diagnostic purposes only.

## NPS3016

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3016 /SET-FILE-LINK COMMAND WITH 'LINK-NAME=SM2UO' MISSING FOR OUTPUT FILE

## NPS3017

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3017 OUTPUT FILE '(&00)' IS NOT SM2 LOGGING FILE

### Meaning

This message can occur only when an existing output file is to be extended
(OPEN-MODE=EXTEND).

## NPS3018

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3018 DMS ERROR IN OUTPUT FILE. DMS CODE '(&00)'. /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG
or see the BS2000 manual 'System Messages'.

## NPS3019

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3019 DMS ERROR IN INPUT FILE '(&01)'. DMS CODE '(&00)'. /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG
or see the BS2000 manual 'System Messages'.

## NPS3020

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS3020 INVALID RECORD IN INPUT FILE '(&00)'

### Meaning

The specified input file contains an incorrect record, e.g. a record with
record length 0.

## NPS3021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3021 SM2U1 HANDLES SM2 LOGGING FILES

## NPS3022

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS3022 FILE(S) '(&00)' TRANSFERED TO OUTPUT FILE

## NPS3023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3023 SM2U1 HANDLES USER LOGGING FILES

## NPS3024

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3024 SPECIFIED 'LAST-INDEX=(&00)' GREATER THAN HIGHEST FILE INDEX '(&01)'. OPERAND '*LAST' ASSUMED

### Meaning

The specified LAST-INDEX value in the //SEPARATE-FILES statement is
greater
than the highest file index (&01) in the input file. All the data up
to the end of the input file will be transferred to the output file.

## NPS3025

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3025 SPECIFIED 'FIRST-INDEX=(&00)' GREATER THAN HIGHEST FILE INDEX '(&01)' IN INPUT FILE

### Meaning

The specified FIRST-INDEX value in the //SEPARATE-FILES statement is
greater than the highest file index (&01) in the input file.
No files have been transferred to the output file.

## NPS3026

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3026 OUTPUT FILE '(&00)' IS NOT USER LOGGING FILE

### Meaning

This message can occur only when an existing output file is to be extended
(OPEN-MODE=EXTEND).

## NPS3027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3027 /SET-FILE-LINK COMMAND WITH 'LINK-NAME=(&00)' MISSING FOR OUTPUT FILE

## NPS3028

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3028 /SET-FILE-LINK COMMAND WITH 'LINK=(&00)' MISSING FOR INPUT FILE

## NPS3029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3029 VALUE FOR 'LAST-INDEX' SMALLER THAN VALUE FOR 'FIRST-INDEX'

## NPS3030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS3030 FILE INDEX VALUES OF BLOCKS ARE NOT IN ASCENDING ORDER

## NPS3031

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS3031 ONLY 'BUFFER-LENGTH=*STD(SIZE=16)' PERMITTED FOR OUTPUT FILE '(&00)'.

### Meaning

Output files are only permitted with 'BUFFER-LENGTH=*STD(SIZE=16)'.
The value of the BUFFER-LENGTH operand in the /ADD-FILE-LINK command
for the output file is invalid or the existing output file
(OPEN-MODE=EXTEND) has a wrong BUFFER-LENGTH.

### Response

Retry the /ADD-FILE-LINK command without operand BUFFER-LENGTH or
convert the existing output file with SM2U1.

## NPS4102

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4102 SPECIFIED TIMES IN DEFINITION OF ANALYSIS INTERVAL NOT IN ASCENDING ORDER

### Meaning

The start time output for the analysis interval is greater than the
corresponding end time.

## NPS4139

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4139 SPECIFIED TIMES IN DEFINITION OF TIME WINDOW NOT IN ASCENDING ORDER

### Meaning

The specified start time of a time window is greater than the
corresponding
end time.

## NPS4140

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4140 TIME WINDOWS OVERLAPPING OR NOT IN ASCENDING ORDER

## NPS4145

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4145 '24:00' NOT PERMITTED AS START TIME FOR TIME WINDOW

## NPS4146

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4146 ILLEGAL TIME SPECIFICATION (LATER THAN 24:00)

## NPS4147

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4147 INVALID YEAR SPECIFIED

### Meaning

Year-specifications are only allowed from 0-99 and 1960-2059.

## NPS4154

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4154 '*SUMMARY' ONLY PERMITTED AS FIRST ELEMENT IN LIST

### Meaning

Possible reasons:
- *SUMMARY was specified more than once for disk analysis.
- *SUMMARY was not specified as the first element in a list.

## NPS4161

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS4161 ANALYSIS OF HEAD MOVEMENTS NO LONGER POSSIBLE SINCE SM2 V15.0A

### Meaning

The analysis for HEAD MOVEMENTS is no longer possible, because the data
are no more gathered.

## NPS4162

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4162 INCONSISTENT VALUES WHEN SELECTING CYLINDER AREA

### Meaning

When selecting a cylinder area either the number selected for the
last cylinder is smaller than the number of the first cylinder, or
the subinterval specified by *BY is larger than the selected
cylinder area.

## NPS4163

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4163 NUMBER OF LINES GREATER THAN 32766. NO ANALYSIS IS POSSIBLE

### Meaning

The number of table lines requested implicitly via the *BY operand is
greater than 32766.

## NPS4200

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS4200 BLOCK SIZE OF TRANSFER FILE TOO SHORT. PROCESSING ABORTED.

### Meaning

The buffer length of the transfer file is too short for the DATA
record.

### Response

- create the transfer file without specifying a buffer length.
BUFFER-LENGTH=STD(SIZE=16) will be defined automatically.
- reduce the number of analysis subintervals.

## NPS4310

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4310 STATEMENT REJECTED

### Meaning

The statement is invalid and must be reentered corrected.

## NPS4311

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4311 ERROR DURING STATEMENT ENTRY. SM2R1 TERMINATED ABNORMALLY

### Meaning

Errors in statement input could not be recovered in procedure or in
batch mode.
No analysis is possible.

## NPS4312

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4312 'CONNECTION-SET (&00)' NOT DEFINED

### Meaning

The name of the connection set is invalid or has not been defined.

## NPS4313

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4313 'USERID-SET (&00)' NOT DEFINED

### Meaning

The name of the USER ID set is invalid or has not been defined.
USER ID sets must be defined by means of the //CREATE-USERID-SET
statement.

## NPS4314

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4314 'TSN-SET (&00)' NOT DEFINED

### Meaning

The name of the task set is invalid or has not been defined.
Task sets must be defined by means of the //CREATE-TSN-SET statement.

## NPS4315

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4315 'JOBNAME-SET (&00)' NOT DEFINED

### Meaning

The name of the job name set is invalid or has not been defined.
Job name sets must be defined by means of the //CREATE-JOBNAME-SET
statement.

## NPS4316

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4316 'JOBCLASS-SET (&00)' NOT DEFINED

### Meaning

The name of the job class set is invalid or has not been defined.
Job class sets must be defined by means of the //CREATE JOBCLASS-SET
statement.

## NPS4317

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4317 MORE THAN MAXIMUM PERMITTED NUMBER OF '(&00)' DEFINED

## NPS4318

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4318 SDF SYNTAX FILE DEFECTIVE OR INCORRECTLY ACCESSED. CONTACT THE SYSTEM ADMINISTRATOR

### Meaning

Either no SDF syntax file has been assigned or the one assigned is
invalid or cannot be accessed.

## NPS4319

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4319 SYSTEM ERROR WHEN PROCESSING SDF STATEMENTS. SDF RETURN CODE '(&00)'

### Response

Contact the system administrator.

## NPS4320

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4320 NUMBER OF ANALYSIS PART-INTERVALS TOO HIGH

### Meaning

The analysis interval is divided in too many part-intervals. The maximal
number of intervals is 8000.

### Response

Choose longer part-intervals.

## NPS4321

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4321 WRONG ITEM NUMBER (&01) FOR REPORT (&00)

### Meaning

An item number (&01) which does not exist for report (&00)
was given.

## NPS4322

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4322 SYNTAX ERROR. 'LOWER-LIMIT' GREATER THAN 'UPPER-LIMIT'. STATEMENT REJECTED

### Response

Correct the statement and try again.

## NPS4330

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4330 USER-ID-, TSN-, JOBNAME- OR JOBCLASS-SET NOT DEFINED.

### Meaning

The statement PRINT-TASK-STATISTICS was given with TSN=*BY-SET-NAME,
but without any USER-ID-, TSN-, JOBNAME- or JOBCLASS-SET.
At least one SET name must be specified.

## NPS4350

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS4350 SM2 LOGGING FILE INCORRECTLY. ANALYSIS NOT POSSIBLE.

### Meaning

Possible reasons:
- the assigned SM2 logging file is empty
- the assigned file is not a SM2 logging file
- the assigned file does not have SAM format
- the version of SM2 logging file is lower than V11.0A

### Response

A logging file in PAM format can be converted with SM2U1.

## NPS4351

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4351 SM2 LOGGING FILE CONTAINS NO VALID TIME STAMP RECORD. ANALYSIS NOT POSSIBLE

## NPS4354

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS4354 SM2 LOGGING FILE CONTAINS NO CLOSE RECORD. ANALYSIS NOT COMPLETELY

### Meaning

The SM2 logging file was not correctly closed.
Possible reasons are
- SM2 system task has abnormally terminated
- system crash
during creation of SM2 logging file.

### Response

The file can be repaired by issuing the command
//REPAIR-DISK-FILES FILE-STATUS=*ANY (FILE-NAME=dateiname).
Subsequently, a CLOSE record should be attached with SM2U1.

## NPS4451

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4451 TIME STAMP OF CURRENT RECORD '(&00)' EARLIER THAN LAST TIME STAMP '(&01)'

### Meaning

The time stamps in the SM2 logging file are not in ascending order.

## NPS4452

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4452 SPECIFIED END TIME OF ANALYSIS INTERVAL SMALLER THAN FIRST TIME STAMP OF SM2 LOGGING FILE '(&00)'

## NPS4453

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4453 SPECIFIED START TIME OF ANALYSIS INTERVAL GREATER THAN LAST TIME STAMP OF SM2 LOGGING FILE '(&00)'

## NPS4503

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4503 (&00) ACCESSES TO CYLINDER NUMBERS WITH UNKNOWN ADDRESS

### Meaning

(&00): Number of disk accesses for which SM2 could not determine
the cylinder number.

## NPS4504

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4504 (&00) ACCESSES TO BLOCK NUMBERS WITH UNKNOWN ADDRESS

### Meaning

(&00): Number of disk accesses for which SM2 could not determine the
block number.

## NPS4551

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4551 NO MEASUREMENTS FOUND FOR TASK ANALYSIS

### Meaning

Task analysis was requested but the SM2 logging file does not contain
any task records in the specified analysis interval.

## NPS4552

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4552 NO MEASUREMENTS FOUND FOR SPECIFIED 'TSN-SET (&00)'

### Meaning

The SM2 logging file contains no TSNs of the specified TSN set
in the given analysis period.

## NPS4553

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4553 NO MEASUREMENTS FOUND FOR SPECIFIED 'USERID-SET (&00)'

### Meaning

The SM2 logging file contains no USER IDs of the specified USER ID set
in the given analysis period.

## NPS4555

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4555 NO MEASUREMENTS FOUND FOR QUEUE TRANSITION

### Meaning

Task queue analysis was requested but the SM2 logging file does not
contain any queue records in the given analysis interval.

## NPS4556

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4556 NO DATAS FROM DISK MEASUREMENTS FOUND

### Meaning

Disk statistics were requested but the SM2 logging file contains no
records of DISK measurement in the given analysis interval.

## NPS4557

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS4557 NO MEASUREMENTS FOUND FOR SPECIFIED 'JOBNAME-SET (&00)'

### Meaning

The SM2 logging file contains no job names of the specified job name set
in the given analysis period.

## NPS4558

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS4558 NO MEASUREMENTS FOUND FOR SPECIFIED 'JOBCLASS-SET (&00)'

### Meaning

The SM2 logging file contains no job classes of the specified job class
set in the given analysis period.

## NPS4559

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS4559 NO DATAS FROM HSMS MEASUREMENTS FOUND

### Meaning

Hsms statistics were requested but the SM2 logging file contains no
records of HSMS measurement in the given analysis interval.

## NPS4601

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4601 INTERNAL EAM MACRO ERROR. CODE=(&00)

### Meaning

An EAM call returns the specified error information.

## NPS4651

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4651 NO MEASUREMENTS FOUND FOR DISTRIBUTION OF HEAD MOVEMENTS FOR '(&00)'

### Meaning

The disk (&00) for which analysis was requested was not active in the
analysis period or was not monitored.

## NPS4652

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4652 NO MEASUREMENTS FOUND FOR DISTRIBUTION OF SERVICE TIMES FOR '(&00)'

### Meaning

The disk (&00) for which analysis was requested was not active in the
analysis period or was not monitored.

## NPS4653

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4653 NO MEASUREMENTS FOUND FOR DISTRIBUTION OF I/O REQUESTS FOR '(&00)'

### Meaning

The disk (&00) for which analysis was requested was not active in the
analysis period or was not monitored.

## NPS4654

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4654 NO MEASUREMENTS FOUND FOR SUMMARY OF I/O REQUESTS

### Meaning

In the analysis period either no disk was monitored by SM2 or none
of the monitored disks was active.

## NPS4655

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4655 NO MEASUREMENTS FOUND FOR SUMMARY OF HEAD MOVEMENTS

### Meaning

In the analysis period either no disk was monitored by SM2 or none
of the monitored disks was active.

## NPS4656

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4656 NO MEASUREMENTS FOUND FOR SUMMARY OF SERVICE TIMES

### Meaning

In the analysis period either no disk was monitored by SM2 or none
of the monitored disks was active.

## NPS4657

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS4657 NO DATA FOUND FOR OUTPUT OF CONFIGURATION

### Meaning

The SM2 logging file contains no configuration data for the selected
analysis period.

## NPS4658

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4658 DATA FOR OUTPUT OF CONFIGURATION IS INCOMPLETE

### Meaning

The SM2 logging file does not contain all configuration data. No output of
configuration data.

## NPS4751

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

NPS4751 INPUT CONTROL FILE 'MTFILE' HAS VERSION (&00)

## NPS4801

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4801 INSUFFICIENT VIRTUAL ADRESS SPACE FOR ANALYSIS

### Meaning

The storage space requested by the program could not be made available.
The analysis run can be restarted using fewer reports.

## NPS4853

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPS4853 NO MEASUREMENTS FOUND DURING ANALYSIS INTERVAL FOR '(&00)'

### Meaning

SM2 did not monitor the variable (&00) in the specified analysis interval.

## NPS4854

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4854 (&00) SUPPRESSED DUE TO REPORT CONDITION

### Meaning

Report (&00) suppressed because measurements are in given range.

## NPS4901

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4901 VERSIONS OF 'SM2R1' AND 'MTFILE' INCOMPATIBLE

## NPS4951

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4951 NO PERFORMANCE DATA AVAILABLE FOR CPU TYPE '(&00)'. CONTACT SYSTEM ADMINISTRATOR

### Meaning

Automatic analysis is not possible without limit values for the
specified CPU type.

## NPS4953

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS4953 MONITORED DATA FOR '(&00)' REQUIRED TO COMPLETE AUTOMATIC ANALYSIS

### Meaning

Automatic analysis should be conducted using all the required data
(cf. the BS2000 manual 'SM2'), otherwise it is possible that bottlenecks
will remain undetected.

## NPS4954

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPS4954 MONITORED DATA FOR VM2000 REQUIRED TO COMPLETE AUTOMATIC ANALYSIS AND FOR RELATIVATION OF PERFORMANCE DATA

### Meaning

Automatic analysis should be conducted using all the required data
(cf. the BS2000 manual 'SM2'), otherwise it is possible that bottlenecks
will remain undetected.
Additionally automatic analysis needs the CPU QUOTA of VM2000 record
for relativation of performance data.

### Response

Start monitoring program VM.

## NPS4955

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPS4955 Automatic analysis not possible due to live migration at '(&00)'

### Meaning

The Automatic Analysis cannot be performed, because in the evaluation
period a live migration to a system with a different CPU type has been
executed.
(&00): time stamp for the live migration, in the format
YYYY-MM-DD HH:MM:SS.

### Response

Retry Automatic Analysis for a evaluation period without live migration

## NPS5000

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NPS5000 UNKNOWN ERROR CODE '(&00)' OR SUBCODE '(&01)' DELIVERED FROM SM2

### Meaning

SM2 delivered an error code (&00) or a subcode (&01) referring to
a non-existent message.

©2025 Fujitsu | BS2000 System Messages