## NJD0001

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0001 (&00) SCU (&01) ALERT MT=(&02) SER=(&03) REFCODE=(&04) (&05)

### Meaning

This message from the Device Error Recovery (D.E.R) shows the data
reported by a controller as a Service Information Message (SIM).
SCU : Storage Control Unit.
(&00): a list in the format 'X1X2X3'
X1: the mnemonic name of the channel (2/4 characters)
X2: the mnemonic name of the controller (2/4 characters)
X3: the mnemonic name of the device (2/4 characters)
(&01): type of error
SERVICE : No performance degradation is expected.
No system or application outage has occurred.
MODERATE: Performance degradation is possible in a heavily loaded
environment.
No system or application outage has occurred.
SERIOUS : A primary I/O subsystem resource is disabled.
A significant performance degradation is possible.
A system or application outage may have occurred.
ACUTE : A major I/O subsystem resource is disabled, or
the product may have been damaged.
The performance may be severely degraded.
A system and/or application outage may have occurred.
(&02): the controller designation
MT: machine type
(&03): the serial number of the controller (SER)
(&04): displays information the service technician requires to repair
the fault
REFCODE: reference code
(&05): REPEAT, if the SIM is a repeat of a previous SIM.
In emergency messages the inserts are displayed without key words.

### Response

Contact the service technician.

## NJD0002

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0002 (&00) CACHE (&01) ALERT MT=(&02) SER=(&03) REFCODE=(&04) (&05)

### Meaning

This message from the Device Error Recovery (D.E.R) outputs the data
reported by a controller as a Service Information Message (SIM).
The failure concerns the controller cache.
(&00): a list in the format 'X1X2X3'
X1: the mnemonic name of the channel (2/4 characters)
X2: the mnemonic name of the controller (2/4 characters)
X3: the mnemonic name of the device (2/4 characters)
(&01): type of error
SERVICE : No performance degradation is expected.
No system or application outage has occurred.
MODERATE: Performance degradation is possible in a heavily loaded
environment. No system or application outage has occurred.
SERIOUS : A primary I/O subsystem resource is disabled.
A significant performance degradation is possible.
A system or application outage may have occurred.
ACUTE : A major I/O subsystem resource is disabled, or
the product may have been damaged.
The performance may be severely degraded.
A system and/or application outage may have occurred.
(&02): the controller designation
MT: machine type
(&03): the serial number of the controller (SER)
(&04): displays information the service technician requires to repair
the fault
REFCODE: reference code
(&05): REPEAT, if the SIM is a repeat of a previous SIM.
In emergency messages the inserts are displayed without key words.

### Response

Contact the service technician.

## NJD0003

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0003 (&00) DASD (&01) ALERT MT=(&02) SER=(&03) REFCODE=(&04) VSN=(&05) ID=(&06) (&07)

### Meaning

This message from the Device Error Recovery (D.E.R) outputs the data
reported by a device as a Service Information Message (SIM).
DASD: Direct Access Storage Device
(&00): a list in the format 'X1X2X3'
X1: the mnemonic name of the channel (2/4 characters)
X2: the mnemonic name of the controller (2/4 characters)
X3: the mnemonic name of the device (2/4 characters)
(&01): type of error
SERVICE : No performance degradation is expected.
No system or application outage has occurred.
MODERATE: Performance degradation is possible in a heavily loaded
environment. No system or application outage has occurred.
SERIOUS : A primary I/O subsystem resource is disabled.
A significant performance degradation is possible.
A system or application outage may have occurred.
ACUTE : A major I/O subsystem resource is disabled, or
the product may have been damaged.
The performance may be severely degraded.
A system and/or application outage may have occurred.
(&02): the device designation
MT: machine type
(&03): the serial number of the device (SER)
(&04): Displays information the service technician requires to repair
the fault
(&05): Volume Serial Number (VSN)
(&06): Service Information Message identifier (SIM ID)
(&07): REPEAT, if the SIM is a repeat of a previous SIM.
In emergency messages the inserts are displayed without key words.

### Response

Contact the service technician.

## NJD0004

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0004 (&00) MEDIA (&01) ALERT MT=(&02) SER=(&03) REFCODE=(&04) VSN=(&05) ID=(&06) CCHH=(&07) (&08)

### Meaning

This message from the Device Error Recovery (D.E.R) outputs the data
reported by a device as a Service Information Message (SIM).
The disk surface of the device is concerned.
MEDIA: surface in the disk.
(&00): a list of the format 'X1X2X3'
X1: the mnemonic name of the channel (2/4 characters)
X2: the mnemonic name of the controller (2/4 characters)
X3: the mnemonic name of the device (2/4 characters)
(&01): type of error
SERVICE : No performance degradation is expected.
No system or application outage has occurred.
MODERATE: Performance degradation is possible in a heavily loaded
environment.
No system or application outage has occurred.
SERIOUS : A primary I/O subsystem resource is disabled.
A significant performance degradation is possible.
A system or application outage may have occurred.
ACUTE : A major I/O subsystem resource is disabled, or
the product may have been damaged.
The performance may be severely degraded.
A system and/or application outage may have occurred.
(&02): the device designation
MT: machine type
(&03): the serial number of the device (SER)
(&04): displays information the service technician requires to repair
the fault
REFCODE: reference code
(&05): Volume Serial Number (VSN)
(&06): Service Information Message Identifier (SIM ID)
(&07): cylinder (CC) and head (HH) address of the faulty track
(&08): REPEAT, if the SIM is a repeat of a previous SIM.
In emergency messages the inserts are displayed without key words.

### Response

Contact the service technician.

## NJD0005

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0005 (&00)

### Meaning

This message is a shortened form of the standard device error recovery
message for disks EXC0857. Its only purpose is to inform the Support
Center via teleservice about an acute hardware problem with FBA-disks.
List of elements within the insert (refer to EXC0857 for details):
channel, controller, device mnemonic
error mnemonic
identifier of D.E.R-request
CSB, --, USB, sense bytes 0-2, EFB, Op-Code
sense bytes 3-7 sense bytes 30,31

### Response

None.

## NJD0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NJD0010 -AUTOCALL FAILED- (&00) MT=(&02) SER=(&03) REFCODE=(&04) (&05) - (&06)

### Meaning

This message from the Device Error Recovery (D.E.R) outputs the data
reported by a disk controller as a service information message (SIM).
(&00): a list in the format 'X1X2X3'
X1: the mnemonic name of the channel (2/4 characters)
X2: the mnemonic name of the controller (2/4 characters)
X3: the mnemonic name of the device (2/4 characters)
(&02): the controller designation
MT: machine type
(&03): the serial number of the controller (SER)
(&04): displays information the service technician might require to fix
the situation
REFCODE: reference code; format is 'xyyy-vwww-zzzz'
x476 = 'SERVICE PROCESSOR NOT RESPONDING'
x477 = 'AUTOCALL (TO EMC CSC) FAILED'
(&05): REPEAT, if the SIM is a repeat of a previous SIM.
(&06): Text string
'SERVICE PROCESSOR NOT RESPONDING' or
'AUTOCALL (TO EMC CSC) FAILED':
The call to the support center of the vendor could not be
performed by the disk controller. The controller should
still be able to perform the normal recovery/logging action,
but the support center of the vendor will not know about the
event and cannot dispatch service personnel.
In emergency messages the inserts are displayed without key words.

### Response

Please contact the service technician.
The technician has to check whether a reaction to the error causing the
failed AutoCall is needed.
Please check PC/modem.
Acknowledge message with tsn-nnn. to remove it from the list of messages
requiring a response.

## NJD0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NJD0011 -ENVIRONMENTAL ALARM- (&00) MT=(&02) SER=(&03) REFCODE=(&04) (&05) - (&06)

### Meaning

This message from the Device Error Recovery (D.E.R) outputs the data
reported by a disk controller as a service information message (SIM).
The problem causing the message is reported to the support center
of the vendor.
(&00): a list in the format 'X1X2X3'
X1: the mnemonic name of the channel (2/4 characters)
X2: the mnemonic name of the controller (2/4 characters)
X3: the mnemonic name of the device (2/4 characters)
(&02): the controller designation
MT: machine type
(&03): the serial number of the controller (SER)
(&04): displays information the service technician might require to fix
the situation
REFCODE: reference code; format is 'xyyy-vwww-zzzz'
x467 = 'ERROR/EVENT POSTED BY SRDF PARTNER BOX'
x470 = 'OVER TEMPERATURE'
x471 = 'LOW BATTERY / HIGH CHARGE STATE'
x472 = 'POWER SUBSYSTEM ALARM'
x47A = 'AC LINE FAILURE/INTERRUPTION'
x47B = 'BATTERY/CLOCK/DIRECTOR WITHOUT POWER'
x478/x479/x47C = 'UNSPECIFIED ENVIRONMENTAL PROBLEM'
(&05): REPEAT, if the SIM is a repeat of a previous SIM.
(&06): Text string
'ERROR/EVENT POSTED BY SRDF PARTNER BOX':
An error/event occured at the controller connected via SRDF.
'OVER TEMPERATURE':
Controller may be overheated; controller breakdown possible.
'LOW BATTERY / HIGH CHARGE STATE' or
'BATTERY/CLOCK/DIRECTOR WITHOUT POWER':
Problem with power supply.
'POWER SUBSYSTEM ALARM' or
'AC LINE FAILURE/INTERRUPTION':
Problem with power supply; controller breakdown possible.
'UNSPECIFIED ENVIRONMENTAL PROBLEM'
In emergency messages the inserts are displayed without key words.

### Response

Please contact the service technician immediately.
Acknowledge message with tsn-nnn. to remove it from the list of messages
requiring a response.

## NJD0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NJD0012 -REDUCED REDUNDANCY- (&00) MT=(&02) SER=(&03) REFCODE=(&04) (&05) - (&06)

### Meaning

This message from the Device Error Recovery (D.E.R) outputs the data
reported by a disk controller as a service information message (SIM).
The problem causing the message is reported to the support center
of the vendor.
(&00): a list in the format 'X1X2X3'
X1: the mnemonic name of the channel (2/4 characters)
X2: the mnemonic name of the controller (2/4 characters)
X3: the mnemonic name of the device (2/4 characters)
(&02): the controller designation
MT: machine type
(&03): the serial number of the controller (SER)
(&04): displays information the service technician might require to fix
the situation
REFCODE: reference code; format is 'xyyy-vwww-zzzz'
x460 = 'DYNAMIC SPARE INVOKED'
x463 = 'DISK ADAPTER FAILED'
x466 = 'DYNAMIC SPARE INVOKED FOR REMOTE DISK'
x46D = 'ALL REMOTE LINKS NOT OPERATIONAL'
x473 = 'LOCAL MIRRORED DEVICE NOT READY'
x474 = 'MIRRORED DEVICE WRITE-DISABLED'
x475 = 'REMOTE MIRRORED DEVICE NOT READY'
x47D = 'REMOTE LINK NOT OPERATIONAL'
(&05): REPEAT, if the SIM is a repeat of a previous SIM.
(&06): Text string
'DYNAMIC SPARE INVOKED' or
'DYNAMIC SPARE INVOKED FOR REMOTE DISK':
The redundancy is temporarily reduced but will be
automatically restored by the system.
'DISK ADAPTER FAILED':
Breakdown of a disk adapter; disks of defective adapter
taken over by partner adapter.
'ALL REMOTE LINKS NOT OPERATIONAL':
The disks connected via SRDF are no longer synchronized.
'LOCAL MIRRORED DEVICE NOT READY' or
'MIRRORED DEVICE WRITE-DISABLED' or
'REMOTE MIRRORED DEVICE NOT READY':
Breakdown of a redundant recorded device;
redundancy is reduced.
'REMOTE LINK NOT OPERATIONAL'
In emergency messages the inserts are displayed without key words.

### Response

Please contact the service technician.
Acknowledge message with tsn-nnn. to remove it from the list of messages
requiring a response.

## NJD0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NJD0013 -INFORMATION- (&00) MT=(&02) SER=(&03) REFCODE=(&04) (&05) - (&06)

### Meaning

This message from the Device Error Recovery (D.E.R) outputs the data
reported by a disk controller as a service information message (SIM).
(&00): a list in the format 'X1X2X3'
X1: the mnemonic name of the channel (2/4 characters)
X2: the mnemonic name of the controller (2/4 characters)
X3: the mnemonic name of the device (2/4 characters)
(&02): the controller designation
MT: machine type
(&03): the serial number of the controller (SER)
(&04): displays information the service technician might require to fix
the situation
REFCODE: reference code; format is 'xyyy-vwww-zzzz'
x461/x462 = 'RESYNCHRONIZATION COMPLETED'
x464 = 'DATA MIGRATION OF ALL VOLUMES COMPLETED'
x465 = 'RESYNCHRONIZATION STARTED'
x46E = 'ALL REMOTE LINKS OPERATIONAL AGAIN'
x47E = 'REMOTE LINK(S) OPERATIONAL AGAIN'
x47F = 'AUTOCALL (TO EMC CSC) COMPLETED'
(&05): REPEAT, if the SIM is a repeat of a previous SIM.
(&06): Text string
'RESYNCHRONIZATION COMPLETED':
The original redundancy is restored.
'DATA MIGRATION OF ALL VOLUMES COMPLETED'
'RESYNCHRONIZATION STARTED'
'ALL REMOTE LINKS OPERATIONAL AGAIN'
'REMOTE LINK(S) OPERATIONAL AGAIN'
'AUTOCALL (TO EMC CSC) COMPLETED'
In emergency messages the inserts are displayed without key words.

### Response

No response is necessary since this message reports the start or
completion of an operation.

## NJD0021

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0021 (&00) PERM DATA CHECK ON PRIMARY RECOVERED ON SECONDARY - MN=(&01) SSID=(&02) DPA=(&04)

### Meaning

A permanent data check occurred while reading from the primary disk of a
DualCopy pair. Data was read alternatively from the secondary disk.
(&00): VSN (if available)
(&01): Device MN
(&02): Subsystem Id
(&04): Device Path Address (device address including controller bits
for 3492: Physical Device Id)

### Response

You should repair the track concerned on the primary disk using the
program VOLIN. Refer to the track address in preceding messages or in
the Error Logging System (ELS).

## NJD0022

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0022 (&00) (&05) IS SUSPENDED DUPLEX - (&06) (&07) - MN=(&01) SSID=(&02) SP=(&03) DPA=(&04)

### Meaning

One disk of a DualCopy pair was set to state HOLD (SUSPENDED DUPLEX) due
to an error.
(&00): VSN (if available)
(&01): Device MN
(&02): Susbsystem Id
(&03): Storage Path Number (cluster 0/1, path 0/1)
(&04): Device Path Address (device address including controller bits
for 3492: Physical Device Id)
(&05): Suspended Device (PRIMARY or SECONDARY)
(&06): Failed Device (PRIMARY or SECONDARY)
(&07): Reason Code of error (clear text or code of sensebyte 8)

### Response

After repair you can switch to state DUAL again.
Acknowledge message with tsn-nnn. to remove it from list of messages
requiring response.

## NJD0023

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0023 (&00) DEVICE ERROR RECOVERY SUSPEND DUPLEX FOR PRIMARY REJECTED - MN=(&01) SSID=(&02) FRC=(&08)

### Meaning

Device Error Recovery tried to switch to state HOLD (SUSPENDED DUPLEX)
due to a write error on the primary disk of a DualCopy pair. This failed
because the initial state was not DUAL.
(&00): VSN (if available)
(&01): Device MN
(&02): Subsystem Id
(&08): Format/Message and Reason Code from sense bytes 7 and 8
or CSB and EFB if Unit Check was not the reason of rejection

### Response

None

## NJD0024

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0024 (&00) INTERVENTION REQUIRED - MN=(&01) SSID=(&02) DPA=(&04)

### Meaning

An error which requires the intervention of an operator occurred on a
disk device (disabled, CE-mode etc.).
(&00): VSN (if available)
(&01): Device MN
(&02): Subsytem Id
(&04): Device Path Address (device address including controller bits
for 3492: Physical Device Id)

### Response

Determine and correct the error.

## NJD0025

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0025 DASD FAST WRITE INHIBITED, NVS BATTERY DEAD - MN=(&09) SSID=(&02)

### Meaning

DASD Fast Write (cache supported writing) on the indicated controller is
no longer permitted, because the battery of the nonvolatile storage (NVS)
is dead.
(&02): Subsystem Id
(&09): Controller MN

### Response

Call maintenance to recharge battery.
Acknowledge message with tsn-nnn. to remove it from list of messages
requiring response.

## NJD0026

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0026 DEVICE CONTROLLER WRITE INHIBITED - MN=(&01) SSID=(&02) DPA=(&04)

### Meaning

Device Error Recovery inhibited writes for the erroneous path between
controller and disk device due to an error on the indicated device.
(&01): Device MN
(&02): Subsystem Id
(&04): Device Path Address (device address including controller bits
for 3492: Physical Device Id)

### Response

Call maintenance.

## NJD0027

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0027 CHANNEL PATH WRITE INHIBITED - SSID=(&02) CPID=(&10) SP=(&03)

### Meaning

Device Error Recovery inhibited writes for the indicated path between
channel and controller due to an I/O-error.
(&02): Subsystem Id
(&03): Storage Path Number (cluster 0/1, path 0/1)
(&10): Channel Path Id

### Response

Call maintenance.

## NJD0028

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0028 STORAGE PATH WRITE INHIBITED - SSID=(&02) SP=(&03)

### Meaning

Device Error Recovery inhibited writes for the indicated storage path due
to an I/O-error.
(&02): Subsystem Id
(&03): Storage Path Number (cluster 0/1, path 0/1)

### Response

Call maintenance.

## NJD0029

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0029 DEVICE NOT OPERATIONAL WITH STORAGE PATH - MN=(&01) SSID=(&02) SP=(&03) DPA=(&04)

### Meaning

The indicated path to the disk device was fenced by the firmware due to an
I/O-error.
(&01): Device MN
(&02): Subsystem Id
(&03): Storage Path Number (cluster 0/1, path 0/1)
(&04): Device Path Address (device address including controller bits
for 3492: Physical Device Id)

### Response

Call maintenance.
Acknowledge message with tsn-nnn. to remove it from list of messages
requiring response.

## NJD0030

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0030 DEVICE ADAPTOR NOT OPERATIONAL WITH STORAGE PATH - MN=(&01) SSID=(&02) SP=(&03) DPA=(&04)

### Meaning

The indicated path to the device adaptor was fenced by the firmware due to
an I/O-error.
(&01): Device MN
(&02): Subsystem Id
(&03): Storage Path Number (cluster 0/1, path 0/1)
(&04): Device Path Address (device address including controller bits
for 3492: Physical Device Id)

### Response

Call maintenance.
Acknowledge message with tsn-nnn. to remove it from list of messages
requiring response.

## NJD0031

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0031 DEVICE ERROR RECOVERY TERMINATED, RETRY IMPOSSIBLE - MN=(&01) LRC=(&11)

### Meaning

An I/O-error occurred on the indicated disk device. No more I/O-retries
by the Device Error Recovery are possible.
(&01): Device MN
(&11): Logical Return Code from Channel Control Block

### Response

None

## NJD0040

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0040 RAID1 INACTIVE TRANSITION FOR (&00) ON MN=(&01), DRIVE '(&12)' DPA=(&04) OUT OF USE

### Meaning

Due to a permanent error one drive of a RAID1 pair has gone out of use.
Recording will be continued with reduced availability (Mono).
(&00) VSN
(&01) Device MN
(&04) Device Path Address (physical device address incl. controller bits)
(&12) Drive identifier within the RAID1 pair (A or B)

### Response

Call maintenance.
Acknowledge message with tsn-nnn. to remove it from the list of messages
requiring a response.

## NJD0041

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0041 RAID1 ACTIVE TRANSITION FOR (&00) ON MN=(&01), DRIVE '(&12)' PDA=(&04) AVAILABLE

### Meaning

The specified second device of a RAID1 pair has become available (again).
Recording continues with high availability.
(&00) VSN
(&01) Device MN
(&04) Device Path Addr. (physical device address incl. controller bits)
(&12) Drive identifier within the RAID1 pair (A or B)

### Response

Acknowledge message with tsn-nnn. to remove it from the list of messages
requiring a response.

## NJD0042

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NJD0042 RAID1 FOR (&00) ON MN=(&01) TEMPORARILY INACTIVE, DRIVE '(&12)' PDA=(&04) OUT OF USE

### Meaning

Due to an error one drive of a RAID1 pair has gone out of use. A
suitable spare drive is available and all the data will be copied from
the lasting device intact onto the spare device. Until end of copy
recording will continue with reduced availability (Mono).
(&00) VSN
(&01) Device MN
(&04) Device Path Addr. (physical device address incl. controller bits)
(&12) Drive identifier within the RAID1 pair (A or B)

### Response

Call maintenance.
Acknowledge message with tsn-nnn. to remove it from the list of messages
requiring a response.

## NJD0101

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NJD0101 Creation of PAGDER bourse failed - call of $NBCREA shows inconsistencies

### Meaning

$NBCREA supplies one of the following return codes:
- inconsistent parameters
- wrong unit or function number
- wrong version number
System termination is initiated.

## NJD0102

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NJD0102 PAGDER bourse error - call of $NBRSIG shows inconsistencies

### Meaning

$NBRSIG supplies one of the following return codes:
- inconsistent parameters
- wrong unit or function number
- wrong version number
- rdata < sdata
System termination is initiated.

## NJD0103

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NJD0103 HARDWARE FAILURE ON PAGING/HOME PVS. SYSTEM TERMINATION IS INITIATED

### Meaning

A hardware failure occured on the paging PVS/home PVS.
System termination is initiated.

### Response

Contact the service-technician.

©2025 Fujitsu | BS2000 System Messages