## NKG0000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKG0000 NDM detects software problem

### Meaning

NDM (nucleus device management) has detected an inconsistency in NDM
oder I/O system tables or an error at an interface and has written an
entry in its error trace area. Extraordindary events are also indicated
in this manner.
If nessary an additional SERSLOG (software error logging) entry is
written.
The SERSLOG entry consists of an ID and the corresponding data.
Layout of the trace ID:
<fe> 1 character : A = NKA, D = NKD, G = NKG, S = NKS, R = NKR,
T = NKT, V = NKV, L = NKL (subsystem DRV)
NDM functional unit
<modul> 3 characters: short ID of an NDM module without prefix NK<fe>
<id> 4 characters: trace ID, in case of assembler moduls a label
###<id> exists
Example:
VDUTE1RE: FE=NKV, module=NKVDUTT, trace label=###E1RE
The contents of the trace data depends on the error case and in most
cases is described within the module at the corresponding NDMTRAC call.

### Response

To detect or analyse the problem, a NDMDAMP could be helpful. Not all
SERSLOG entries describe an actual error, some entries can be "normal".

## NKG0001

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKG0001 DEVICE '(&00)' CANNOT BE ASSIGNED TO LOCATION '(&01)'. MAXIMUM NUMBER OF DEVICES FOR THIS LOCATION ALREADY REACHED

## NKG0002

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKG0002 DEVICE '(&00)' CANNOT BE ASSIGNED TO LOCATION '(&01)'

## NKG0003

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKG0003 DEVICE '(&00)' IS NOT ASSIGNED TO LOCATION '(&01)'

## NKG0004

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKG0004 DEVICE '(&00)' IS NOT ASSIGNED TO ANY LOCATION

## NKG0005

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKG0005 LOCATION '(&00)' NOT DEFINED

## NKG0007

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

NKG0007 COMMAND NOT PERMITTED BECAUSE MAREN NOT IN SUBSYSTEM-CATALOG

## NKG0008

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

NKG0008 THE SUBSYSTEM MAREN IS NOT CREATED

### Meaning

Without the subsystem MAREN the command brings about that the specified
devices are permanently not available.

### Response

Please start MAREN !

## NKG0009

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NKG0009 /REMOVE-DEVICE-DEPOT UNIT=*ALL,LOCATION='(&00)' NOT PROCESSED. THERE ARE ALLOCATIONS IN THE SPECIFIED LOCATION

## NKG0010

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NKG0010 DEVICE-DEPOT-COMMAND FOR DEVICE '(&00)' NOT PROCESSED. THE DEVICE IS NOT AVAILABLE

### Meaning

If /SHOW-DEVICE shows FREE as ALLOC-STATE for the specified device, it is
nethertheless possible that the device is logically allocated by a type-
request.

### Response

The command will be processed for the device if it is DETACHED.

## NKG0011

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NKG0011 THE DEVICE '(&00)' IS ALREADY ASSIGNED TO LOCATION '(&01)'

## NKG0020

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NKG0020 NDM trace is stopped bacause of stop condition

©2025 Fujitsu | BS2000 System Messages