## BLS0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0002 DBL INTERNAL ERROR. PROCESSING ABORTED WITH DUMP

### Response

Contact the system administrator.

## BLS0003

Destination: CONSOLE Routing code: P Weight: 99

Warranty : NO

BLS0003 STARTUP ABORTED DUE TO INSUFFICIENT MEMORY OR SYSTEM ERROR

### Meaning

DBL cannot generate its global tables.

## BLS0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0004 DBL ERROR IN SYMBOLIC NAME PROCESSING. STARTUP ABORTED

### Meaning

A data element processed by DM (DBL data manager) is inconsistent.

## BLS0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0005 ERROR IN DBL CONTEXT VECTOR MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal inconsistency has been detected in the context
vector manager.

### Response

Contact the system administrator.

## BLS0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0006 INTERNAL ERROR IN DBL MEMORY MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the memory manager.

### Response

Contact the system administrator.

## BLS0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0007 ERROR DURING EXTERNAL CALL OF INTERFACE '(&00)'. RETURNED RC : X '(&01)'. PROCESSING ABORTED

### Meaning

Call of interface (&00) returned a bad return code. Possible error:
system error.

### Response

Contact the system administrator.

## BLS0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0008 INTERNAL ERROR IN DBL INTERFACE HANDLER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the interface handler.

### Response

Contact the system administrator.

## BLS0009

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0009 INTERNAL ERROR IN DBL DATA MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the data manager.

### Response

Contact the system administrator.

## BLS0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0010 INTERNAL ERROR '(&00)' IN DBL DATA STRUCTURE MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

Internal error '(&00)' has been detected in the data structure manager.

### Response

Contact the system administrator.

## BLS0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0011 INTERNAL ERROR IN DBL BASIC INPUT MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the basic input manager.

### Response

Contact the system administrator.

## BLS0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0012 INTERNAL ERROR IN DBL LINK-LOAD PROCESSOR. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected by the linking-loading processor.

### Response

Contact the system administrator.

## BLS0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0013 INTERNAL ERROR IN DBL ERROR HANDLER (ERROR-ID=(&00))

### Meaning

An internal error is detected by the DBL error handler:
the message corresponding to the given ERROR-ID (&00)
is not defined in the DBL message table.

### Response

Contact the system administrator.

## BLS0014

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0014 ERROR IN DBL SHARE PROCESSOR. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected by the SHARE processor.

### Response

Contact the system administrator.

## BLS0015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0015 LIBRARY ERROR DURING LDSLICE PROCESSING

### Meaning

A call to PLAM during LDSLICE processing has failed.

## BLS0016

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0016 ERROR IN DBL POSIX-PROGRAM STARTER. PROCESSING ABORTED

### Meaning

An internal error has been detected by the POSIX-program starter.

### Response

Contact the system administrator.

## BLS0017

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

BLS0017 ERROR '(&00)' DURING INITIALIZATION OF SUBSYSTEM '(&01)'

### Meaning

An internal error has been detected by the initialization routine
of subsystem (&00).
- '01' : DST not found
- '02' : SYSINF returns an invalid rc
- '03' : OS version not supported
- '04' : necessary reps are not installed in CP

### Response

Contact the system administrator.

## BLS0018

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0018 LOCK ON INTERNAL BLS VLN-SYMBOLTABLE HELD BY TASK WITH ID '(&00)'. PROCESSING ABORTED

### Meaning

Write or read accesses to the BLS symboltable for VLNs (Very Long Names)
cannot be performed, because the task with Id (&00) holds the
necessary lock.When (&00) = 0, no Id of task holding lock can be given.

### Response

Retry later the command; if the error persists, contact the system
administrator.

## BLS0020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0020 $GETMEM ERROR. TASK ABORTED WITH SYSTEM DUMP

### Meaning

The requested memory space could not be allocated.
Possible reason: system memory saturation at this moment.

### Response

Contact the system administrator or retry later.

## BLS0021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0021 $RETMEM ERROR. TASK ABORTED WITH SYSTEM DUMP

### Meaning

The requested memory space could not be released.
Possible reason : system error.

### Response

Contact the system administrator.

## BLS0023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0023 SYSTEM ERROR DURING CALL OF '(&00)' : RC '(&01)'. PROCESSING ABORTED

### Meaning

The call of interface (&00) returned a bad return code (&01).
Possible reason : system error.

### Response

Contact the system administrator.

## BLS0034

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0034 ERROR IN OBJECT MODULE '(&00)'. LOADING ABORTED WITH DUMP

### Meaning

An inconsistency in the input object module (&00) has been detected.
module name=C'?': no valid ESD-record in current module.

## BLS0035

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0035 ERROR '(&00)' IN DBL INTERNAL MEMORY MANAGEMENT. PROCESSING ABORTED

### Meaning

(&00): DBL memory management error code :
- '0B040188': invalid load address specified
- '0C080194': validation error, i.e. user has released or
changed
status of a class 6 memory page belonging to DBL.
- '0A0C0198': discrepancy error during allocation of vector
address space.
- '0B0C0198': saturation of vector address space.
- '0C0C0198': module too big or not enough space.
A dump is taken for diagnosis only in case of
error codes x'0B040188' and x'0C080194'.

### Response

Correct the program according to the return code
and try again.

## BLS0040

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0040 ERROR WHEN LOADING SYMBOLIC INFORMATION. LOADING ABORTED WITH DUMP

### Response

Correct object module.

## BLS0041

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0041 LSDA RECORD ERROR IN MODULE '(&00)'. LOADING ABORTED WITH DUMP

### Meaning

(&00): Module name.

### Response

Correct object module.

## BLS0053

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0053 ERROR IN CSECT '(&00)'. SYMBOLIC INFORMATION ABOUT CSECT IN MODULE '(&01)' NOT LOADED. DUMP TAKEN

### Meaning

(&00): CSECT name.
(&01): Module name.

### Response

Recreate object module.

## BLS0054

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0054 LOAD OF SYMBOLIC INFORMATION CONTINUES

### Meaning

Additional message to the preceding one.

## BLS0055

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0055 COMPILER OR LIBRARY ERROR. INVALID SYMBOLIC INFORMATION RECORD TYPE IN CSECT '(&00)' IN MODULE '(&01)'. DUMP TAKEN

### Meaning

(&00): CSECT name.
(&01): Module name.

### Response

Contact the system administrator.

## BLS0060

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0060 RESIDENCY OF (&00) '(&01)' INVALID IN THIS ENVIRONMENT. LOADING ABORTED

### Meaning

(&00): MODULE or COMMON.
(&01): name of the module or of the common.
Possible reasons for a MODULE:
1. The computed PSEUDO-RMODE of the module is 24 and the load unit
is loaded in the privileged memory.
2. The computed PSEUDO-RMODE of the module is 24 and the load unit
is loaded in a memory pool which is located above the 16 MB limit.
(How the PSEUDO-RMODE of a module is computed is explained in the
BS2000 "Dynamic Binder Loader / Starter" manual).
Possible reasons for a COMMON:
1. The COMMON is to be loaded below the 16 MB limit and the load unit
is loaded in a memory pool which is located above the 16 MB limit.
The COMMON is to be loaded below this limit because:
- its RMODE is 24 or
- the load unit PROGMODE is 24 or
- at least one MODULE of the load unit is loaded below the
16 MB limit.
2. The COMMON was already loaded in the same context (in a previous
load unit ) above the 16 MB limit and is to be loaded in the current
load unit below the 16 MB limit.
3. The COMMON is to be loaded below the 16 MB limit and the load
unit is to be loaded in the privileged memory.

### Response

Correct the program or module.

## BLS0061

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0061 AMODE OF SYMBOL '(&00)' INVALID IN THIS ENVIRONMENT. LOADING ABORTED

### Meaning

The load unit contains a symbol (CSECT, COMMON or ENTRY) (&00)
with AMODE=31. Either the system is not an XS one or
PROG-MOD=24 was specified or the loading concerns a privileged
sub-system.

### Response

Change the AMODE value (24 or ANY).

## BLS0100

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0100 NOT ENOUGH MEMORY CLASS '(&00)'. PROCESSING ABORTED

### Meaning

DBL receives the return code NOT ENOUGH MEMORY from the system
memory management. A memory class is saturated by the program
code or the areas requested by the user or by the system
metadata in the privileged memory.
The saturation is often due to an excessive amount of symbolic
information generated via the TEST-OPTIONS=AID or IDA parameter of the
/START-PROGRAM or /LOAD-PROGRAM or
/START-EXECUTABLE-PROGRAM or /LOAD-EXECUTABLE-PROGRAM commands
and the BIND macro.

### Response

Contact the system administrator for the saturation analysis (possibly
reduce the amount of symbolic information and try again).

## BLS0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0101 ERROR DURING VALIDATION OF CLASS 6 MEMORY BLOCK

### Meaning

The validation error occurs either
- if the user has released or changed status
of a class 6 memory block belonging to DBL or
- if the LLM to be loaded contains an empty slice or
- if the reference towards the server inside the user provided
indirection routine is only read accessible.

### Response

Correct the program and try again.

## BLS0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0102 SPECIFIED LOAD ADDRESS CAN NOT BE USED. PROCESSING ABORTED

### Meaning

1. The load address specified in the BIND call cannot be used.
The possible reasons are:
A. The address lies in a page previously requested and
OVERLAY=N is specified.
B. The address is not a class 6 address.
C. The address does not match the minimum alignment required by
the first module of the load unit (e.g. the address is not
page aligned and the first CSECT of the first module has the
attribute PAGE).
D. It is not allowed to load a LLM if a load address is specified
in the BIND call.
2. A not relocatable LLM cannot be loaded at the address specified
in the LLM, because the memory area in which the LLM should be
placed is not free.

### Response

Correct program and try again.

## BLS0104

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0104 ELEMENT '(&00)', VERSION '(&01)' FROM LIBRARY '(&02)' CANNOT BE LOADED. REASON '(&03)'. PROCESSING ABORTED

### Meaning

DBL cannot load LLM for reason (&03) :
- '01' : The LLM can only be loaded on a higher BS2000/OSD resp.
- BLSSERV version or it has an invalid LLM-Format or it contains
- invalid information.
- '02' : LLM sliced "BY-USER" cannot be loaded in POSIX environment.
- '03' : Only one LLM or PAM-LLM sliced "BY-USER" can be loaded
at any time in a given context but one already exists.
- '04' : LLM cannot be loaded in standard RUN MODE.
- '05' : LLM is not compatible with the "PRE-LOADING" feature.
- '06' : The LLM is not loadable, it can only be processed by BINDER
or LLMAM.
- '07' : A LLM with CSECT AMODE=31 cannot be loaded in a unit running in
AMODE 24.
- '08' : System options do not allow to load a LLM in standard RUN MODE.
- '09' : A LLM sliced "BY-USER" cannot be loaded in a "LIST-NAME-UNIT".

### Response

Correct the LLM.

## BLS0105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0105 CONNECTION TO MEMORY POOL '(&00)' WITH SCOPE '(&01)' IS NOT POSSIBLE. PROCESSING ABORTED

### Meaning

A memory pool which holds "user shared code" referenced by the
current load unit cannot be enabled by the task because the
memory block used by the memory pool is not free.

### Response

Ensure that memory block(s) occupied by memory pool(s) holding
"user shared code" are free.

## BLS0106

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0106 PAM-LLM '(&00)' CANNOT BE LOADED. REASON '(&01)'. PROCESSING ABORTED

### Meaning

DBL cannot load PAM-LLM for reason (&01) :
- '01' : The PAM-LLM can only be loaded on a higher BS2000/OSD resp.
- BLSSERV version or it has an invalid LLM-Format or it contains
- invalid information.
- '02' : Only one PAM-LLM or LLM sliced "BY-USER" can be loaded
at a time in a given context and there already exists one.
- '03' : The PAM-LLM is not loadable, it can only be processed
by BINDER.
- '04' : A PAM-LLM with CSECT AMODE=31 cannot be loaded in a unit
running in AMODE 24.
- '05' : A PAM-LLM, with "PUBLIC/PRIVATE" slices, cannot be loaded.

### Response

Correct the LLM.

## BLS0136

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLS0136 FUNCTION ALREADY PROCESSED

### Meaning

The desired function has already been realized earlier.

## BLS0139

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0139 (&00) '(&01)' IN (&02) '(&03)' IS DUPLICATE. PROCESSING ABORTED

### Meaning

A name collision is detected inside a context and the user has
specified NAME-COLLISION=ABORT.
(&00): 'ENTRY', 'COMMON' or 'CSECT'.
(&01): ENTRY, COMMON or CSECT name.
(&02): 'MODULE','LLM' or 'PAM-LLM'.
(&03): Module, LLM or PAM-LLM name.

### Response

Erase the name collision or make the symbol invisible in the specified
module or specify NAME-COLLISION=STD.

## BLS0140

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0140 WRONG '(&00)' RECORD TYPE IN MODULE '(&01)'. LOADING ABORTED WITH DUMP

### Meaning

(&00): Invalid record type.
(&01): Module name.

### Response

Compiler or library error.
Compile and try again.

## BLS0142

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0142 TYPE CODE '(&00)' IN ESD RECORD IN MODULE '(&01)' INCORRECT. LOADING ABORTED

### Meaning

(&00): Invalid type code.
(&01): Module name.
For the meaning of type code see the manual "System conventions".

### Response

Compile and try again.

## BLS0150

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0150 BLS-WARNING DURING LOADING

### Meaning

A warning has been issued by BLS during the loading.

## BLS0151

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0151 USER IS NOT AUTHORIZED TO ISSUE THIS COMMAND. COMMAND REJECTED

### Meaning

The command is rejected according to the task privileges.

## BLS0152

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0152 SYSTEM ERROR DURING LOADING. COMMAND NOT EXECUTED

### Meaning

A system error has been detected by BLS during loading.

## BLS0153

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0153 UNRECOVERABLE ERROR DURING LOADING. COMMAND NOT EXECUTED

### Meaning

An unrecoverable error has been detected by BLS during loading.

## BLS0160

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0160 COMMAND INPUT RESERVED FOR THE ADMINISTRATOR ONLY

### Meaning

Only the system administrator may enter an
/ADD-SHARED-PROGRAM command.

## BLS0162

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0162 PRODUCT NAME '(&00)' ALREADY IN SHARE TABLE. CMD NOT PROCESSED

### Meaning

The current product name (&00) already exists in the share table.
The command /ADD-SHARED-PROGRAM is rejected.

## BLS0163

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0163 INVALID OPERAND. CORRECT COMMAND

### Meaning

The format of the command /ADD-SHARED-PROGRAM is invalid
The command is not processed.

### Response

Correct rejected command and try again.

## BLS0165

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0165 INVALID FILENAME. COMMAND REJECTED

### Meaning

Invalid file name in the command /ADD-SHARED-PROGRAM.
The specified CATID is not local.

### Response

Repeat command with correct operand.

## BLS0166

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0166 ### SPECIFIED RESOLUTION SCOPE NOT PROCESSED BY DSSM

### Meaning

DBL receives a return code from "Select Subsystem Version"
function of DSSM.
The DSSM version is not correct (function not yet supported).

### Response

Retry with correct version of DSSM.

## BLS0167

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0167 ### PRODUCT '(&00)' NOT FOUND IN '(&01)' SCOPE TABLE. COMMAND NOT PROCESSED

### Meaning

The deletion of the product '&00' is not performed because
this product cannot be found in the given product table ('&01').
'&00': product name
'&01': table scope

## BLS0168

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0168 ### NO MEMORY AVAILABLE FOR PRODUCT TABLE. COMMAND NOT PROCESSED

### Meaning

The product entry cannot be created because no memory
can be requested for the product table.

## BLS0170

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0170 OPTION '(&00)' MAY NOT BE SPECIFIED IN COMBINATION WITH "OPTION-PRIORITY=FORCED". COMMAND NOT PROCESSED

### Meaning

An invalid option (&00) has been specified together with
OPTION-PRIORITY=FORCED.
(&00): LIBRARY
PROGRAM-VERSION
CONTEXT
CONTEXT-STATE

### Response

Correct rejected command and try again.

## BLS0171

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0171 INVALID CONTEXT NAME '(&00)' SPECIFIED. COMMAND NOT PROCESSED

### Meaning

The context name must begin with a letter.
(&00): Given context name

### Response

Correct the context name and try again.

## BLS0230

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0230 INVALID FORMAT IN STATEMENT '(&00)(&01)'. CONTINUE PROCESSING? REPLY (Y=YES; N=NO)

### Meaning

Message only for dialog process.
(&00): first part of REP or INCLUDE statement.
(&01): second part of REP or INCLUDE statement.

### Response

Enter appropriate reply.

## BLS0231

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0231 ### INVALID FORMAT IN STATEMENT '(&00)(&01)'. PROCESSING CONTINUES

### Meaning

Message only for batch process.
(&00): first part of REP or INCLUDE statement
(&01): second part of REP or INCLUDE statement.

## BLS0232

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0232 MODULE '(&00)' NOT IN THE LIBRARY. CONTINUE PROCESSING? REPLY (Y=YES; N=NO)

### Meaning

(&00): Module name.

### Response

Enter appropriate reply.

## BLS0233

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0233 ### MODULE '(&00)' NOT IN THE LIBRARY. PROCESSING CONTINUES

### Meaning

Message only for batch process.
(&00): module name.

## BLS0234

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLS0234 MODULE '(&00)' NOT IN CURRENT LOAD UNIT. REP STATEMENT IGNORED. CONTINUE PROCESSING? REPLY (Y=YES; N=NO)

### Meaning

(&00): module name.

### Response

Enter appropriate reply.

## BLS0235

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0235 ### MODULE '(&00)' NOT IN CURRENT LOAD UNIT. REP STATEMENT IGNORED. PROCESSING CONTINUES

### Meaning

Message only for batch process.
(&00): The module name which appears on the REP card.

## BLS0310

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0310 ERROR DURING MAP OUTPUT. SYSOUT MAP GENERATION ABORTED

### Meaning

The YTIEWOUT call returns an error. The map generation on SYSOUT
cannot be continued.

## BLS0311

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0311 WRLST ERROR DURING MAP OUTPUT. SYSLST MAP GENERATION ABORTED

### Meaning

The WRLST call returns an error. The SYSLST map generation cannot
be continued.

## BLS0330

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0330 ### INVALID RECORD '(&00)' IN MODULE '(&01)' IGNORED. PROCESSING CONTINUES

### Meaning

Error in object module.
(&00): Invalid record number.
(&01): Module name.

### Response

Compile and try again.

## BLS0331

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0331 ### CSECT '(&00)' ALREADY LOADED. CURRENT MODULE '(&01)' IGNORED

### Meaning

Duplicate CSECT names are not allowed in standard RUN MODE.
(&00): CSECT name.
(&01): Module name.

## BLS0332

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0332 ERROR DETECTED WHILE LOADING ELEMENT '(&00)', VERSION '(&01)' FROM LIBRARY '(&02)'. LOADING ABORTED

### Meaning

An error is detected while loading LLM (&00) with version (&01)
from library (&02). The private part of this BY-ATTRIBUTE
PRIVATE/PUBLIC LLM refers to a non-visible symbol of the public
part. The loading of the current load unit is aborted.

### Response

Make the related symbol visible or suppress the reference.

## BLS0333

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0333 RESOLUTION BETWEEN PRIVATE AND PUBLIC SLICES OF LLM '(&00)' FAILED. LOADING ABORTED

### Meaning

The resolution of the references from the PRIVATE to the PUBLIC slices
of the LLM (&00) has failed.
Possible reasons :
- A reference could not be solved because of programming mode
incompatibility.
- A reference could not be solved because no corresponding definition was
found.
- A reference could not be solved because of MMODE or HSI
incompatibility.

### Response

Please contact the responsible for loading the LLM PUBLIC slices
to adapt the programming mode(s), the MMODE(s) or the HSI(s)
or to correct the LLM.

## BLS0334

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0334 SYMBOL OR ELEMENT '(&00)' CANNOT BE FOUND. LOADING ABORTED

### Meaning

The symbol specified in the command
/START-EXECUTABLE-PROGRAM resp. /LOAD-EXECUTABLE-PROGRAM or
/START-PROGRAM resp. /LOAD-PROGRAM or
/EXEC resp. /LOAD or
in the macro-call ASHARE, BIND, LINK
resp. the element specified in the macro-call PBSSBDX
cannot be found in the assigned library(ies).

### Response

Correct the symbol resp. element name and try again.

## BLS0335

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0335 UNRESOLVED EXTERNAL REFERENCES '(&00)'

### Meaning

The specified EXTRN or VCON symbol(s) (&00) cannot be found in any
library. In batch process loading will be processed as far as possible.
In dialog process it can be decided in the following message (BLS0336)
whether loading should be continued or not.

## BLS0336

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0336 CONTINUE PROCESSING? REPLY (Y=YES; N=NO)

### Meaning

External references specified in the BLS0335 message cannot be
found in any library.

### Response

Enter appropriate reply.

## BLS0337

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0337 ### DUPLICATE SYMBOL '(&00)' SPECIFIED IN TABLE MACRO. PROCESSING CONTINUES

### Meaning

The user specifies a symbol (&00) which is already known in the
BLS tables. BLS accepts this duplicate symbol but some problems
could arise later.

## BLS0338

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0338 ### ATTRIBUTE (&00) OF CSECT '(&01)' IN MODULE '(&02)' IGNORED

### Meaning

Due to some internal consistency rules or to some system limitation
DBL cannot take account of the attribute (&00) of the CSECT (&01)
in module (&02). Nevertheless, this module is loaded.

## BLS0339

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0339 ### (&00) '(&01)' IN (&02) '(&03)' IS DUPLICATE

### Meaning

A name collision is detected in the context.
The processing continues.
(&00): ENTRY, COMMON or CSECT.
(&01): ENTRY, COMMON or CSECT name.
(&02): MODULE, LLM or PAM-LLM.
(&03): Module, LLM or PAM-LLM name.

## BLS0340

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0340 UNRESOLVED EXTERNAL REFERENCES

### Meaning

The list of the unresolved external references follows in the
message BLS0342.
In interactive mode the list is followed by the message BLS0350
which asks the user if he wants to continue the link-load
processing or not.
In batch mode the processing continues.
This message concerns the unresolved EXTRNs and V-CONs only
(the unresolved WXTRNs are not shown and the unresolved
XDSEC-References follow in the message BLS0341).

## BLS0341

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0341 UNRESOLVED XDSEC REFERENCES

### Meaning

The list of the unresolved XDSEC references follows in the message
BLS0342.
In interactive mode the list is followed by the message BLS0350
which asks the user if he wants to continue the link-load
processing or not.
In batch mode, the processing continues.

## BLS0342

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0342 ### '(&00)'

### Meaning

(&00) is a list of up to 7 unresolved symbol names.
The message BLS0342 follows the message BLS0340 or the
message BLS0341.

## BLS0343

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLS0343 RELOCATION TRUNCATED. PROCESSING CONTINUES

### Meaning

At least one address resulting from the computation of a relocation
has been truncated.

## BLS0344

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0344 ADDRESS IN A MIPS INSTRUCTION OUTSIDE THE CURRENT SEGMENT. PROCESSING ABORTED

### Meaning

The resulting address of a relocation computation, for a "JUMP" or
"JUMP and LINK" instruction, is outside the current segment :
this is forbidden for such instructions.

### Response

- Instead of "direct JUMP" instructions, use the corresponding "register"
instructions, or
- load the symbol referenced by the "JUMP" instruction in the same segment
as the instruction itself.

## BLS0345

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0345 SYMBOL '(&00)' ALREADY IN LINK CONTEXT. LOADING ABORTED

### Meaning

As the specified symbol is already loaded in the link context, a new
loading of this symbol is rejected, in order to avoid duplicate symbols
in a same context.

## BLS0346

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLS0346 INCOMPATIBILITY BETWEEN SERVER HSI CODE AND ILE HSI CODE

### Meaning

In the current load unit, a symbol usable as server of ILE has an HSI
code which doesn't match the HSI code of the corresponding ILE

## BLS0347

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

BLS0347 EOLDTAB IS FULL. PROCESSING CONTINUES

### Meaning

No additional CSECT or ENTRY can be added in EOLDTAB.

## BLS0348

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

BLS0348 SYMBOL '(&00)' NOT YET INITIALIZED IN "SHARED CODE" FOR THE CURRENT TASK

### Meaning

Symbol (&00) belongs to a subsystem not yet initialized for the current
task.

### Response

Make /LOGOFF followed by /SET-LOGON-PARAMETERS in order to initialize
the subsystem for a new task and retry in this task.

## BLS0349

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLS0349 THE COMMAND MODIFY-DBL-OPTIONS IS ONLY SUPPORTED UP TO VERSION V12.0Q AND V12.1P

### Meaning

The command is replaced by the MODIFY-DBL-PARAMETERS one.

## BLS0350

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

BLS0350 CONTINUE LINK-LOAD PROCESSING ? REPLY (Y=YES; N=NO)

### Meaning

This message is issued in interactive mode and asks the user if he
wants to continue the link-load processing after DBL has detected
an event explained in the previous message.
If the reply is Y, the processing continues.
If the reply is N, the processing is aborted, i.e. nothing is loaded.

## BLS0351

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

BLS0351 INVALID DBL-PARAMETER VALUE FOR OPERAND '(&00)'

### Meaning

An inconsistency has been detected between the operand (&00)
and the current value of the corresponding DBL-Parameter.

### Response

Correct the DBL-Parameter value and try the command again.

## BLS0352

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLS0352 INVALID VALUE SPECIFIED FOR WORKSPACE. SYSTEM MAXIMUM VALUE TAKEN

### Meaning

The value given to WORKSPACE is higher that the maximum value
allowed by CL2OP JTMAXMEM. Value of JTMAXMEM is used.

## BLS0353

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0353 PROCESSED ELEMENT : '(&00)' VERSION '(&01)' OF LIBRARY '(&02)'

### Meaning

Name, version and library name of the first module of the currently
processed load unit. The message BLS0353 is sent just before
the message BLS0340 or BLS0335.

## BLS0354

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0354 '(&00)' = '(&01)' OF '(&02)' SYMBOL '(&03)' INCOMPATIBLE WITH THE CURRENT LOAD UNIT ENVIRONMENT ONE (= '(&04)'). PROCESSING ABORTED

### Meaning

(&00) : 'MMODE' or 'HSI'
(&01) : MMODE or HSI value
(&02) : 'MAIN' or 'UNRESOLVED'
(&03) : incompatible Symbol Name
(&04) : MMODE or HSI value of the load unit environment
- When (&02) = MAIN :
An already loaded symbol with the name (&03) has been found,
which is incompatible with the MMODE or HSI of the current
load unit environment.
- When (&02) = UNRESOLVED :
A symbol has been found for the resolution of (&03), but
it is incompatible with the MMODE or HSI of the current
load unit environment.

### Response

Correct the MMODE or HSI.

## BLS0355

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0355 '(&00)' = '(&01)' OF '(&02)' SYMBOL '(&03)' INCOMPATIBLE WITH THE CURRENT LOAD UNIT ENVIRONMENT ONE (= '(&04)'). PROCESSING CONTINUES

### Meaning

(&00) : 'MMODE' or 'HSI'
(&01) : MMODE or HSI value
(&02) : 'MAIN' or 'UNRESOLVED'
(&03) : incompatible Symbol Name
(&04) : MMODE or HSI value of the load unit environment
- When (&02) = MAIN :
An already loaded symbol with the name (&03) has been found,
which is incompatible with the MMODE or HSI of the current
load unit environment.
- When (&02) = UNRESOLVED :
A symbol has been found for the resolution of (&03), but
it is incompatible with the MMODE or HSI of the current
load unit environment.

### Response

The current MMODE becomes the MMODE of the load unit.
If the optional REP A0480174 has been applied,
the processing continues with MMODE resp. HSI check.
If the optional REP A0480174 has not been applied,
the processing continues without MMODE resp. HSI check.

## BLS0356

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0356 ELEMENT '(&00)', VERSION '(&01)' FROM LIBRARY '(&02)' INCOMPATIBLE WITH THE CURRENT LOAD UNIT ENVIRONMENT. REASON '(&03)'. PROCESSING ABORTED

### Meaning

DBL cannot load LLM/OM for reason (&03) :
- '01' : The MMODE of the LLM/OM is incompatible
- with the current MMODE of the load unit.
- '02' : The HSI of the LLM/OM is incompatible
with the current HSI of the load unit.

### Response

Correct the LLM or the OM.

## BLS0357

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0357 ELEMENT '(&00)', VERSION '(&01)' FROM LIBRARY '(&02)' INCOMPATIBLE WITH THE CURRENT LOAD UNIT ENVIRONMENT. REASON '(&03)'. PROCESSING CONTINUES

### Meaning

DBL cannot load LLM/OMe for reason (&03) :
- '01' : The MMODE of the LLM/OM is incompatible
- with the current MMODE of the load unit.
- '02' : The HSI of the LLM/OM is incompatible
with the current HSI of the load unit.

### Response

The current MMODE becomes the MMODE of the load unit.
If the optional REP A0480174 has been applied,
the processing continues with MMODE resp. HSI check.
If the optional REP A0480174 has not been applied,
the processing continues without MMODE resp. HSI check.

## BLS0358

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0358 RESOLUTION BETWEEN PRIVATE AND PUBLIC SLICES OF LLM '(&00)' FAILED. PROCESSING CONTINUES

### Meaning

The resolution of the references from the PRIVATE to the PUBLIC slices
of the LLM (&00) has failed : a reference could not be solved
because of MMODE or HSI incompatibility.

### Response

The current MMODE becomes the MMODE of the load unit.
If the optional REP A0480174 has been applied,
the processing continues with MMODE resp. HSI check.
If the optional REP A0480174 has not been applied,
the processing continues without MMODE resp. HSI check.

## BLS0359

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0359 PROCESSED FILE : '(&00)'

### Meaning

Identification of the currently processed PAM-LLM.
The message BLS0359 is sent just before the message BLS0340.

## BLS0405

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0405 UNRECOVERABLE ERROR DURING MESSAGE OUTPUT BY MSG7-MACRO. PROCESSING CONTINUES

## BLS0420

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0420 ERROR WHEN OPENING EAM FILE (*- OR OMF FILE). LOADING ABORTED

## BLS0421

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0421 EAM FILE (*- OR OMF FILE) DOES NOT EXIST. LOADING ABORTED

## BLS0422

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0422 NON-PRIVILEGED PROGRAM NOT ALLOWED TO ACCESS PRIVILEGED EAM FILE (*- OR OMF-FILE). LOADING ABORTED

## BLS0424

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0424 I/O-ERROR WHEN READING EAM FILE (*- OR OMF-FILE). LOADING ABORTED

## BLS0425

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0425 ERROR WHEN CLOSING EAM FILE (*- OR OMF-FILE). PROCESSING CONTINUES

### Response

Contact the system administrator.

## BLS0450

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0450 ERROR WHEN ACCESSING FILE '(&00)'

### Meaning

(&00): Filename.
Error description in the next message.

## BLS0451

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0451 I/O ERROR WHEN ACCESSING OBJECT MODULE LIBRARY. DMS ERROR '(&00)'. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

For more detailed information about DMS error code enter
/HELP-MSG in system mode or see the DMS manual.

## BLS0452

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0452 FILE IS NOT A VALID LIBRARY

### Meaning

The specified file is neither a program library (PL) nor
an object module library (OML).

### Response

Specify an object module library or a program library.

## BLS0453

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0453 SIZE FIELD ERROR IN OML DIRECTORY

### Response

Send an error message to diagnosis.

## BLS0454

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0454 READ ERROR ON LIBRARY '(&00)'. PROCESSING ABORTED

### Meaning

A read error has occurred on the specified library (&00).
The current linking-loading processing cannot be
continued.

## BLS0455

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0455 SYSTEM TASKLIB DESTROYED. PROCESSING ABORTED

### Meaning

The System Tasklib has been destroyed between the begin and the end
of the loading.

### Response

Recreate System Tasklib and try again.

## BLS0456

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0456 ERROR WHILE ACCESSING FILE '(&00)'. DMS ERROR CODE '(&01)'. USE /HELP-MSG DMS(&01)

### Meaning

(&00): Filename.
(&01): DMS error code.
For more detailed information about the DMS error code enter
/HELP-MSG DMS(&01) in system mode or see the DMS manual.

## BLS0457

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0457 EXTERNAL REFERENCE '(&00)' CANNOT BE RESOLVED. MODULE NAME IN LIBRARY '(&01)' TOO LONG

### Meaning

(&00): ENTRY name.
(&01): Filename.
A module containing the ENTRY (&00) has a name longer than
8 characters.

### Response

Use module names shorter or equal to 8 characters.

## BLS0460

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

BLS0460 LOCK ERROR ON ELEMENT '(&00)' OF LIBRARY '(&01)'. PLAM ERROR CODE '(&02)'. IN SYSTEM MODE /HELP-MSG PLA(&02)

### Meaning

The element '(&00)' of the program library '(&01)'
can not be processed because it is currently locked
(PLAM return code '(&02)').
For more detailed information about PLAM return code
enter /HELP-MSG PLA(&02) in system mode.

### Response

Retry later.

## BLS0461

Destination: USER-TASK Routing code: Weight: 98

Warranty : YES

BLS0461 FILE '(&00)' IS LOCKED. DO YOU WANT TO RETRY ? REPLY (Y=YES, N=NO)

### Meaning

The specified file is currently locked (the DMS error code '0D99' is
received).
Reply = Y : DBL retries to open the file.
If the retry is not successful, the message is sent again
with a maximum of 10 attempts. If the last attempt fails,
the processing is aborted with a further error message.
Reply = N : no retry is performed. The processing is aborted with a
further error message.

### Response

Unlock the file, if it is possible, before the reply "Y".

## BLS0462

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0462 FILE '(&00)' IS LOCKED. RETRY IN PROGRESS

### Meaning

The specified file is currently locked (the DMS error code '0D99' is
received).
The message is sent only in batch mode. DBL retries to open the file;
up to 10 attempts are performed with a waiting time of 20 seconds.
If the last attempt fails, the processing is aborted with a further
error message.

## BLS0464

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0464 PLAM IS NOT AVAILABLE. LOADING ABORTED

### Meaning

PLAM is not linked to the operating system.

### Response

Contact the system administrator.

## BLS0465

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0465 FILE '(&00)' IS NOT A PLAM LIBRARY

### Meaning

The file '(&00)' is not a PLAM library. (For the chosen
function a PLAM library is expected).

### Response

Specify a PLAM library

## BLS0467

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0467 ERROR WHEN ACCESSING FILE '(&00)'. PLAM AMCB ERROR CODE '(&01)'. IN SYSTEM MODE /HELP-MSG PLA(&01)

### Meaning

(&00): Filename.
(&01): PLAM return code.
For more detailed information about PLAM return code
enter /HELP-MSG PLA(&01) in system mode.

### Response

Retry later.

## BLS0468

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0468 SYSTEM SERVICE ERROR CODE '(&00)'

### Meaning

(&00): System service error code (PLAM output).
(Continuation of message BLS0467).

## BLS0469

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0469 LINK NAME '(&00)' NOT FOUND. PROCESSING ABORTED

### Meaning

The specified link name '(&00)' does not exist.

### Response

Correct the link name or assign another one and try again.

## BLS0470

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0470 CATID OF FILE '(&00)' IS NOT LOCAL. PROCESSING ABORTED

### Meaning

The cat ID of the specified file is not local. The linking-
loading is rejected by DBL.

## BLS0500

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLS0500 PROGRAM '(&00)', VERSION '(&01)' OF '(&02)' LOADED

### Meaning

The program with name (&00), version (&01) and
creation date (&02) is loaded.
This message is always sent to the terminal (exception: the task
switch 4 is set) and, additionally, to the operator console if the
CPG-option EACTETYP is set to '2' or '3'.

## BLS0501

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0501 OPERAND ERROR IN MONJV (MONITORING JOB VARIABLE). COMMAND REJECTED

### Response

See previous MONJV message.

## BLS0502

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0502 ERROR WHEN READING PROGRAM FILE. LOADING ABORTED

## BLS0503

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0503 ERROR WHEN CLOSING FILE '(&01)'. DMS ERROR '(&00)'. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

For more detailed information about DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

## BLS0505

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0505 AT THE MOMENT INSUFFICIENT MEMORY TO EXECUTE PROGRAM

### Meaning

- Parameter "RESIDENT-PAGES" in /START-PROGRAM command or
- in /START-EXECUTABLE-PROGRAM command is in conflict
with the attributes of the current task, or
- Total number of pages (resident + pageable) for the program execution
is in conflict with the attributes of the current task, or
- Paging saturation.

## BLS0506

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0506 INVALID CONTEXT INFORMATION. PROGRAM NOT LOADABLE

### Meaning

Context information has been wrongly generated by PBELDE or
error occurred during BLS data structure initialization.

### Response

Contact the system administrator.

## BLS0507

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0507 LOADER FOUND INVALID TEXT MODIFIER RECORD. PROGRAM NOT LOADABLE

### Response

Correct the OML (object module library) and retry loading.

## BLS0508

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0508 NAME OF TEXT MODIFIER RECORD DOES NOT CORRESPOND TO PROGRAM NAME. PROGRAM NOT LOADABLE

### Response

Correct the OML (object module library) and retry loading.

## BLS0509

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0509 ERROR WHEN LOADING PROGRAM. COMMAND NOT PROCESSED

## BLS0510

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0510 FOR STATIC LOADER NO MEMORY AVAILABLE FOR LOADING PROGRAM

### Meaning

Either not enough space is available in the system or the load
point is not in the user address space.

## BLS0511

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0511 I/O ERROR WHEN READING PAM FILE '(&01))'. DMS ERROR '(&00)'.IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

An error corresponding to the specified DMS error code (&00) occurred
when loading the program by the static or dynamic loader.
For more detailed information about DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

### Response

Contact the system administrator.

## BLS0512

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0512 INVALID FILE OR MODULE NAME. COMMAND REJECTED

### Meaning

File or module name is invalid in the command /LOAD-PROGRAM resp.
/START-PROGRAM or in the command /LOAD-EXECUTABLE-PROGRAM resp.
/START-EXECUTABLE-PROGRAM or the filename references
a non imported pubset.

### Response

Correct the command and try again.

## BLS0513

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0513 PROGRAM ERROR FLAG SET. ALL COMMANDS WILL BE IGNORED UNTIL /SET-JOB-STEP OR /LOGOFF INTERCEPTED

### Meaning

User program has detected an error flag.

## BLS0514

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0514 ERROR WHEN OPENING FILE '(&01)'. DMS ERROR '(&00)'. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

For more detailed information about DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

## BLS0515

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0515 INVALID OPERAND IN COMMAND FOR LOADING PROGRAM. CORRECT COMMAND

### Meaning

User attempted to issue a /START-PROGRAM or
/LOAD-PROGRAM or /START-EXECUTABLE-PROGRAM or
/LOAD-EXECUTABLE-PROGRAM command with an invalid format.

### Response

Correct rejected command and try again.

## BLS0516

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0516 AUDIT MODE SWITCHED ON. PROCESSING CONTINUES

### Meaning

The TU-AUDIT is switched on. The loading time will be increased.

### Response

Switch off TU-AUDIT to decrease the loading time.

## BLS0517

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLS0517 MODULE '(&00)' LOADED

### Meaning

The dynamic bind and load is done.
(&00): First module name (if the first module is an object module). This
message is always sent to the terminal (exception: the switch 4 is
set) and, additionally, to the operator console when the CPG option
EACTETYP is set to '2' or '3'.

## BLS0518

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0518 INVALID FORMAT OF LOAD MODULE. COMMAND REJECTED

### Response

Generate the load module again.

## BLS0519

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : NO

BLS0519 PROGRAM '(&00)' LOADED

### Meaning

When the CPG-option EACTETYP is set to '1' or '2', the name of the
loaded program (&00) is sent to the operator console.

## BLS0520

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0520 ACCESS ERROR ON PROGRAM LIBRARY. PLAM AMCB ERROR CODE '(&00)' AND SYSTEM ERROR CODE '(&01)'. IN SYSTEM MODE /HELP-MSG PLA(&00)

### Meaning

An error has been detected by PLAM.
(&00) : PLAM AMCB error code (see manual LMS).
(&01) : System service error code.
For more detailed information about the PLAM AMCB error code
enter /HELP-MSG PLA(&00) in system mode.

### Response

If necessary take DUMP.

## BLS0521

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0521 LOADING OF CLASS-1 PROGRAM NOT PERMITTED. COMMAND REJECTED

## BLS0522

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0522 INPUT FILE NOT PAM FILE

### Meaning

The user tried to load a file which is not a PAM file.

## BLS0523

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

BLS0523 ELEMENT '(&00)', VERSION '(&01)', TYPE '(&03)' FROM LIBRARY '(&02)' IN PROCESS

### Meaning

External identification of
- a LLM, if the first loaded object is a LLM.
The type L element with the name (&00) and the version (&01)
from the library (&02) is processed by DBL.
- an Object Module or a GrossModule, if the first loaded object
is an Object Module or a GrossModule.
The type R element with the name (&00) and the version (&01)
from the library (&02) is processed by DBL.
- a Phase, if the loaded object is a Phase.
The type C element with the name (&00) and the version (&01)
from the library (&02) is processed by ELDE.

## BLS0524

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

BLS0524 (&03) '(&00)', VERSION '(&01)' OF '(&02)' LOADED

### Meaning

(&03) : 'LLM' or 'PAM-LLM'
Internal identification of a LLM (Link and Load Module), resp. PAM-LLM
(PAM Link and Load Module) if the first loaded module is a LLM, resp.
a PAM-LLM: LLM, resp. PAM-LLM, with internal name(&00), internal
version (&01) and creation date and time (&02) was loaded.
This message is always sent to terminal (exception : the task switch 4
is set) and, additionally, to the operator console if the CPG-option
EACTETYP is set to '2' or '3'.

## BLS0525

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0525 WARNING : ELEMENT OF TYPE C IGNORED

### Meaning

The value C can not be given when *std is given for
operand NAME-SCOPE.

### Response

The value C will be ignored by BLS during processing.

## BLS0526

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

BLS0526 PROGRAM FILE '(&00)' IN PROCESS

### Meaning

External identification of a program Phase.
The file with the name (&00) is processed by ELDE.

## BLS0527

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0527 VALUE C FOR OPERAND TYPE IS INCOMPATIBLE WITH NAME-SCOPE VALUE

### Meaning

The value C can not be given when *std or *symbol is given for
the operand NAME-SCOPE.

### Response

Correct operand "TYPE" and reenter the command.

## BLS0528

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

BLS0528 ERROR '(&00)' DURING PROCESSING OF PROGRAM PARAMETERS. COMMAND NOT PROCESSED.

### Meaning

During processing of program parameters, SDF or SDF-P returned the
error code (&00). The loading process is aborted.

## BLS0529

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0529 ERROR IN BLS STARTER. PROCESSING ABORTED

### Meaning

An internal error has been detected by the starter ECEXECUT:
the parameter list of $CPROG is incorrect.

### Response

Contact the system administrator.

## BLS0530

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0530 I/O ERROR WHEN READING PROGRAM LIBRARY : PLAM AMCB ERROR CODE '(&00)' AND SYSTEM ERROR CODE '(&01)'. IN SYSTEM MODE /HELP-MSG PLA(&00)

### Meaning

(&00): PLAM-AMCB error code.
(&01): System error code.
The error occurred during static loading.
For more detailed information about PLAM-AMCB error
code enter /HELP-MSG PLA(&00) in system mode.

### Response

Retry later.

## BLS0531

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0531 DUPLICATE VALUE SPECIFIED FOR OPERAND TYPE.PROCESSING ABORTED

### Meaning

A duplicate value has been found for operand TYPE

### Response

Correct the operand value and reenter the command.

## BLS0532

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0532 ERROR WHEN LOADING PROGRAM

### Meaning

Further information about the error is generally specified in a preceding
BLS message.
If there is no preceding message, an inconsistency has been detected
by the dynamic loader between the load unit to be processed and the
/START-PROGRAM or /LOAD-PROGRAM
/START-EXECUTABLE-PROGRAM or /LOAD-EXECUTABLE-PROGRAM command
of DBL.
Example : a subsystem is loaded above 16 MB and a command /START-PROGRAM
or /LOAD-PROGRAM or /START-EXECUTABLE-PROGRAM or LOAD-EXECUTABLE-PROGRAM
is specified with the same entry point name and without
PROG-MOD=ANY on an XS machine.

### Response

See the preceding BLS message if there is any.

## BLS0533

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0533 SYSTEM ERROR

### Meaning

Error code for $TERM after system error.

### Response

Contact the system administrator.

## BLS0534

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0534 NO MEMORY SPACE AVAILABLE. PROGRAM NOT LOADED

### Meaning

Class 5 memory saturation. There is not enough space to satisfy the
system request.

### Response

Contact the system administrator.

## BLS0535

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0535 DUPLICATE VALUE SPECIFIED FOR OPERAND ALTERNATE-LIBRARIES. PROCESSING ABORTED

### Meaning

A duplicate value has been found for operand ALTERNATE-LIBRARIES

### Response

Correct the operand value and reenter the command.

## BLS0536

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0536 INTERNAL ERROR IN STATIC LOADER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error has been detected while reading the program phase.

### Response

Contact the system administrator.

## BLS0537

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0537 INVALID SYMBOL NAME SPECIFIED IN OPERAND ELEMENT-OR-SYMBOL. COMMAND NOT PROCESSED

### Meaning

As the name specified in operand ELEMENT-OR-SYMBOL must be
considered as a symbol name (NAME-SCOPE=*SYMBOL), its size
is restricted to maximum 32 characters.

### Response

Correct the symbol name and try again.

## BLS0538

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0538 INVALID PHASE NAME SPECIFIED IN OPERAND ELEMENT-OR-SYMBOL. COMMAND NOT PROCESSED

### Meaning

As the name specified in operand ELEMENT-OR-SYMBOL must be
considered as a phase name (TYPE=C), its size
is restricted to maximum 41 characters.

### Response

Correct the symbol name and try again.

## BLS0539

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

BLS0539 PROGRAM FILE '(&00)' IN PROCESS

### Meaning

External identification of a PAM-LLM.
The file with the name (&00) is processed by DBL.

## BLS0540

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0540 DATA SECURITY CHECK FAILURE. LOADING ABORTED

### Meaning

Error during library or element check. Possible reasons :
the relocation items (RLD) or the OML directory (1 or 2) or the
input (LLM or OM) is corrupted.

### Response

Correct input and try again.

## BLS0541

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLS0541 THE SYMBOLIC INFORMATION (LSD) IS ONLY PARTIALLY LOADED

### Meaning

A discrepancy between the real LSD size and the corresponding information
in the LSDA records has been detected.

## BLS0550

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0550 DISCREPANCY BETWEEN LAST PAGE NUMBER IN CATALOG ENTRY OF PROGRAM FILE AND PROGRAM HEADER

### Meaning

The number of the last page in catalog entry of the program file is
not equal to the page number written by TSOSLNK.

## BLS0551

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLS0551 Copyright (C) (&01) (&00). All rights reserved

### Meaning

(&00): copyright text.
(&01): copyright year, if specified.
This message is issued when the copyright is available. This message is
always sent to the terminal (exception: the task switch 4 is set) and,
additionally, to the operator console if the CPG-option EACTETYP is
set to '2' or '3'.

## BLS0552

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLS0552 Copyright (C) (&00) Fujitsu Technology Solutions GmbH. All rights reserved

### Meaning

(&00): copyright year, if specified.
This message is always sent to the terminal (exception: the task switch 4
is set), and, additionally, to the operator console if the CPG-option is
set to '2' or '3'.

## BLS0553

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0553 IN THIS PROCEDURE IT IS NOT PERMITTED TO UNLOAD AN ALREADY LOADED PROGRAM. COMMAND REJECTED

### Meaning

The operand UNLOAD=NO was given in the command /CALL-PROCEDURE.
So it is not permitted to unload a program which has already been
loaded at this moment.
This case is an error, SPINOFF is activated.

## BLS0554

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

BLS0554 NO PROGRAM TO UNLOAD

### Meaning

A command /CANCEL-PROGRAM was issued when no program had been loaded.

## BLS0555

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0555 PROGRAM FILE NOT COMPLETE. LOADING ABORTED

### Meaning

The number of the last page in the catalog entry of the program file
written by TSOSLNK does not correspond to the number in the program
header. Part of the program file has been destroyed.

## BLS0560

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLS0560 INVALID 'CFID' DETECTED DURING PROGRAM LOADING

### Meaning

The 'CFID' of the page does not match the 'CFID' in the catalog
entry.Either this page has not been written by TSOSLNK during the
program generation or it has been overwritten before the
/START-PROGRAM or /LOAD-PROGRAM or /START-EXECUTABLE-PROGRAM or
/LOAD-EXECUTABLE-PROGRAM command.

## BLS0565

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLS0565 ### INCOMPATIBLE OPERAND VALUES. OPERAND IGNORED. PROCESSING CONTINUES

### Meaning

There is an incompatibility between operand values of the
/START-PROGRAM or /LOAD-PROGRAM or /START-EXECUTABLE-PROGRAM or
/LOAD-EXECUTABLE-PROGRAM command.
Possible reasons:
- ALTERNATE-LIBRARIES=NO and AUTOLINK=ALTERNATE-LIBRARIES: AUTOLINK=NO
assumed.

## BLS0566

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0566 Module '(&00)' can only be loaded without LSD information. Continue processing? Reply (Y=Yes; N=No)

### Meaning

Message only for dialog task.
The LSD information of the load module (&00) exceeds 256MB.
The load module can therefore only be loaded without
the LSD information.

### Response

Load module without LSD information and specify library containing LSD
information using AID command %SYMLIB.

## BLS0567

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0567 The module '(&00)' is loaded without LSD information.

### Meaning

Message only for batch process.
The LSD information of the loading module (&00) exceeds 256MB.
The load module is loaded without the LSD information.

## BLS0570

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0570 TEST AND DIAGNOSTIC INFORMATION NOT LOADED

### Meaning

A 'CFID' error has been detected when loading the test and diagnostic
information.

## BLS0977

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0977 ### REPFILE '(&00)' DOES NOT EXIST. REP PROCESSING ABORTED

### Meaning

The specified repfile (&00) does not exist. The module is loaded
without REP correction.

### Response

Retry with the correct repfile name.

## BLS0978

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

BLS0978 PROBLEM DURING REPLOG TASK INITIALIZATION. NO REP LOGGING ON THIS SESSION

### Meaning

A problem occurs during REPLOG task initialization, no REP
logging will be active on current session.

### Response

Contact the system administrator.

## BLS0979

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0979 ### NO ACTIVE REP LOGGING FILE ON THIS SESSION. NO READ MARK SET

### Meaning

On this session, no REP logging file is currently open.
The /SET-REPLOG-READ-MARK command is thus aimless.

## BLS0980

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLS0980 REP COMMENT: '(&00)'

### Meaning

The REP comment (&00) from the REP file is displayed.

## BLS0981

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLS0981 LOCK FOR REP LOGGING HELD BY TASK WITH ID '(&00)'. PROCESSING CONTINUES WITHOUT REP LOGGING

### Meaning

Accesses to the REP logging information in memory cannot be performed,
because the task with Id (&00) holds the necessary lock.

### Response

Contact the system administrator.

## BLS0989

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLS0989 DMS ERROR '(&00)' WHEN OPENING FILE '(&01)'. IN SYSTEM MODE /HELP-MSG DMS(&00).

### Meaning

The REP file cannot be opened.
For more detailed information about DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.
The program remains loaded but without REP correction(s).

## BLS0990

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLS0990 PROCESSING OF REP FILE '(&00)' STARTED

### Meaning

(&00): REP file name.

## BLS0991

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLS0991 $GETMEM ERROR. PROCESSING OF REP FILE '(&00)' NOT EXECUTED

### Meaning

The REP loader routine cannot obtain memory space.

## BLS0992

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLS0992 DMS ERROR CODE '(&00)'. PROCESSING OF REP FILE '(&01)' ABORTED. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

(&00): DMS error code
(&01): REP file name
The REPs read before the DMS error are applied.
For more detailed information about the DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

### Response

Correct the file before the next loading.

## BLS0993

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLS0993 REP '(&00)'-ERROR. REPFILE '(&02)'. REP PROCESSING CONTINUES. (&01)

### Meaning

An error of the type (&00) has been detected when processing the REP
record (&01) that has last been read from the file (&02).
This REP is not applied.
(&00) = FORMAT : format error
= PARITY : parity error
= CHECK : data check error
= NAME : invalid module name or module not found
= LENGTH : address not in module
= VERSION : invalid version number.
= RELOC : - relocation truncated (type H or L) or
- relocation range error (type I)
(&01): invalid REP record.

### Response

Correct the invalid REP before the next loading.

## BLS0994

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLS0994 ERROR WHILE SETTING READ MARK ON CURRENT REP LOGGING FILE. COMMAND NOT PROCESSED

### Meaning

The CLTF CLOSE function (called with type = PSEUDO) has reported
an error to BLS. The command is not processed.

## BLS0995

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLS0995 NOREF FILE IS '(&00)'

### Meaning

(&00) NOREF file name.

## BLS0996

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLS0996 DMS ERROR CODE '(&00)'. PROCESSING OF NOREF FILE '(&01)' ABORTED. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

(&00): DMS error code.
(&01): NOREF file name.
For more detailed information about the DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

### Response

Correct the file before the next loading of the concerned program.

## BLS0997

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLS0997 $GETMEM ERROR. PROCESSING FOR NOREF FILE '(&00)' ABORTED

### Meaning

The REP loader routine cannot obtain a
work area. The NOREF file (&00) cannot be used.

## BLS0998

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

BLS0998 DMS ERROR '(&00)' WHEN OPENING FILE '(&01)'. RETRY ? REPLY (Y=YES; N=NO). IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

The REP file cannot be opened.

### Response

Correct the error and retry (answer: Y),
or abort the REP processing (answer: N).
Only one retry is allowed and if it is not successful
the REP processing is aborted with message BLS0992.
When the REP processing is aborted the program remains
loaded but without REP correction(s).

## BLS0999

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

BLS0999 ERROR IN REPLOG TASK. REP LOGGING SUPPRESSED. DUMP TAKEN, PROCESSING CONTINUES

### Meaning

An external call has reported to DBL an error in the REPLOG task.
The possible external calls are :
- $RETMEM
- CLTF(Common-Log-Task-Facility) call
- $TSKID
- $SYSINF.
System dump taken and REP logging suppressed, but the normal REP
processing continues.

### Response

Contact the system administrator.

©2025 Fujitsu | BS2000 System Messages