## JDS0301

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0301 DESTINATION PROCESSOR '(&00)' NOT CONNECTED TO MSCF NETWORK. COMMAND REJECTED

### Meaning

The specified destination processor is known to the MSCF network but
the communication link to this processor was severed when the
command was issued.
(&00): BCAM name of the destination processor specified in the command as
a BCAM name or a catalog ID (CAT-ID) or via a job variable.
MSCF: Multi System Control Facility.

### Response

Request the operator to restore the connection to this processor
and repeat the command after this has been done.

## JDS0302

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0302 DESTINATION PROCESSOR '(&00)' NOT KNOWN IN MSCF NETWORK. COMMAND REJECTED

### Meaning

(&00): BCAM name of the destination processor specified in the
command as a BCAM name or a catalog ID (CAT-ID) or via
a job variable.
MSCF: Multi System Control Facility.

### Response

Correct the BCAM processor name, catalog ID or job variable and then
repeat the command.

## JDS0303

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0303 CONNECTION TO DESTINATION PROCESSOR '(&00)' SEVERED. COMMAND PROCESSING ABORTED

### Meaning

While transmitting a job to the specified destination processor the
communication link to this processor was interrupted. The result of
command processing is undefined.
Exception: in the case of ENTER processing and if message JDS0311 was
displayed on the operator console of the destination processor,
ENTER processing was error-free; without message JDS0311, it was
aborted without any result.
(&00): BCAM name of the destination processor.

### Response

Ask the operator of the destination processor for information on the
processor or job status.

## JDS0304

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0304 JOB VARIABLE '(&00)' NOT ACCESSIBLE. REASON: '(&01)'. COMMAND REJECTED

### Meaning

The job variable containing the name of the processor or catalog is not
accessible. The /ENTER-JOB command was not processed.
(&00): name of the job variable specified in the HOST operand instead of
the BCAM name or the catalog ID.
(&01): return code (same meaning as message JVS(&01)).

### Response

Perform the action suggested for the error identified in the
appropriate JVS message and repeat the /ENTER-JOB command.

## JDS0305

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JDS0305 JOB DISTRIBUTION NOT AVAILABLE. COMMAND REJECTED

### Meaning

When the /ENTER-JOB command was issued, the job distribution
facility (MSCF) was not available.
MSCF: Multi System Control Facility.

### Response

Ask the operator to set up the MSCF environment and repeat the
/ENTER-JOB command once this has been done.

## JDS0307

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

JDS0307 JOB DISTRIBUTION READY

## JDS0308

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0308 JOB DISTRIBUTION CURRENTLY INACTIVE ON DESTINATION PROCESSOR '(&00)'. COMMAND NOT PROCESSED

### Meaning

The job distribution facility on the destination processor is available,
but currently not ready for use. The /ENTER-JOB command was not processed.
(&00): BCAM name of the destination processor.

### Response

Request the system administrator of the destination processor to
ready the job distribution facility, and repeat the /ENTER-JOB command
once this has been done.

## JDS0309

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0309 CATALOG '(&00)' NOT KNOWN IN MSCF NETWORK. COMMAND REJECTED

### Meaning

The catalog identified in the HOST operand is not known in the
MSCF network.
MSCF: Multi System Control Facility.

### Response

Correct the catalog name and repeat the /ENTER-JOB command.
If there was no error in the catalog name, contact the system
administrator.

## JDS0310

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0310 CATALOG '(&00)' KNOWN IN MSCF NETWORK BUT NOT ACCESSIBLE. COMMAND REJECTED

### Meaning

The catalog specified in the HOST operand is known in the MSCF
network, but is not accessible.
MSCF: Multi System Control Facility.

### Response

Ask the system administrator to make the catalog accessible
and repeat the /ENTER-JOB command once this has been done.

## JDS0311

Destination: CONSOLE Routing code: J Weight: 70

Warranty : NO

JDS0311 USER ID '(&03)' RECEIVED JOB FROM REMOTE PROCESSOR '(&00)', USER ID '(&02)'. TSN: (&01)

### Meaning

This message is purely informative and explains that the local
processor has accepted a valid job from the specified remote processor.
(&01): TSN of the job.
(&02): user ID which issued the /ENTER-JOB or /ENTER-PROCEDURE command.
(&03): user ID under which the job is to run.

## JDS0313

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JDS0313 Command not supported on destination processor. Command rejected

### Meaning

The destination processor uses a different BS2000 Version that does not
support the sending or receiving of the given command.

## JDS0314

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0314 OPERAND '(&00)' NOT SUPPORTED ON DESTINATION PROCESSOR. PROCESSING CONTINUES

### Meaning

Operand (&00) is not known in BS2000 version of the destination
processor.
Command processing is continued in such a way, as if the parameter
was not specified.
(&00): Operand of the actual command.

## JDS0316

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JDS0316 SYSCMD FILE NOT CATALOGED ON REMOTE HOST

### Meaning

The requested SYSCMD file has not been cataloged on the pubset
of the remote host.
Command processing is aborted.

## JDS0317

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JDS0317 SYSCMD FILE IS MIGRATED ON REMOTE HOST. COMMAND REQUEST WITHDRAWN BY CALLER

## JDS0320

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JDS0320 JOB DISTRIBUTION NOT POSSIBLE. COMMAND REJECTED

### Meaning

It is not possible to accept the job on any of the hosts of the
XCS cluster with the given operands or defaults.

### Response

Try it again with new operand values.

## JDS0321

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JDS0321 SUBSYSTEM 'JPPOPT' NOT LOADED: COMMAND NOT PROCESSED

### Meaning

The corresponding subsystem is not loaded in the present BS2000
configuration.

### Response

Try the command again after having loaded the subsystem.

## JDS0322

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JDS0322 PROCESSOR '(&00)': JOB NOT ACCEPTED: '(&01)'

### Meaning

Job cannot be accepted on processor (&00) of XCS cluster.
Possible reasons (&01):
- Connection to the destination processor is severed
- System error / SHUTDOWN in process / memory saturation
- Command file / MONJV / calendar data not accessible
- Invalid access authorization
- Job class IN DELETE / not accessible / not defined
- Job class limits inhibit value of operand

### Response

NONE

## JDS0349

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

JDS0349 JOB DISTRIBUTION TASK TERMINATED ABNORMALLY

### Meaning

A system error has occurred in the job distribution task, causing
task termination and making job distribution impossible.

### Response

Request the system administrator to restart MSCF communication
by means of the /MRSSTART command.

©2025 Fujitsu | BS2000 System Messages