# HAL

## HAL0001

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0001 MDEBUG ACTIVE

### Meaning

The master debugger mdebug has been started.

## HAL0002

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0002 MDEBUG INACTIVE

### Meaning

The master debugger mdebug has been stopped.

## HAL0111

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0111 ADMIN RESET GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP

### Meaning

VM2000 has stopped and reset the processor concerned due to a VM2000 command.

## HAL0112

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0112 ADMIN STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP

### Meaning

VM2000 has stopped the processor concerned due to a VM2000 command.

## HAL0140

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0140 HAL ABORT GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP

### Meaning

The HAL on this processor has detected an inconsistency and has terminated the
processing of BS2000 instructions on all processors.

### Response

In the SEM execute the action “Generate new diagnostic data" under Hardware -> Server -> - Service - Diagnostics and save the data by downloading it to your administration PC.
Please notify the Customer Support.

## HAL0141

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0141 HAL ABORT GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP OTHER GP

### Meaning

The HAL on another processor has detected an inconsistency and has terminated the
processing of BS2000 instructions on all processors.
This message is a continuation message of HAL0140.

## HAL0211

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0211 MDEBUG STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP

### Meaning

The master debugging interface has been used by either mdebug or RMAassist to halt the
processing of BS2000 instructions. This may happen as a normal part of IPL processing or
if mdebug is being used to examine the system.

## HAL0212

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0212 MDEBUG STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP BREAK-POINT

### Meaning

A break point set by mdebug has been executed by the given processor. The processing of
BS2000 instructions has been halted.

## HAL0213

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0213 MDEBUG STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP DATA TRAP

### Meaning

The given processor has executed an instruction that has modified a virtual memory
address that is being monitored for modification via mdebug. The processing of BS2000
instructions has been halted.

## HAL0214

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0214 MDEBUG STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP SAVE-STATE

### Meaning

The master debugging interface has been used by either mdebug or RMAassist to halt the
processing of BS2000 instructions in preparation for a new IPL. This always happens as a
normal part of IPL processing.

## HAL0215

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0215 MDEBUG SPIN GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP FW-STOP

### Meaning

The relevant processor has interrupted the execution of BS2000 instructions due to a breakpoint in HAL set by mdebug.

## HAL0221

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0221 MDEBUG START GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP

### Meaning

The master debugging interface has been used by either mdebug or RMAassist to start the
processing of BS2000 instructions. This is not a normal part of IPL processing but the result
of administrator intervention with mdebug or RMAssist.

## HAL0231

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0231 MDEBUG RESET DATABP GPXX

### Meaning

The monitoring for modification of a virtual memory address has been stopped on the
processor concerned.

## HAL0241

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0241 MDEBUG SET DATABP GPXX VVVVVVVVVVVVVVVV

### Meaning

The monitoring for modification of the given virtual memory address has been started on
the processor concerned.

## HAL0311

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0311 BS2000 STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP DISABLED-WAIT

### Meaning

A new PSW has been loaded by the given processor in which the wait bit is set and no
interrupts are enabled. As a result, the processing of BS2000 instructions has been halted.
This may occur as part of a normal system shutdown or may be due to a system crash -
SETS.

### Response

If the BS2000 system is no longer running and was not terminated intentionally, please perform a SLED to back up the diagnostic data.

## HAL0312

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0312 BS2000 STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP SIGP

### Meaning

BS2000 stopped the processor concerned using an SIGP instruction. This is a normal
during BS2000 system shutdown or when a CPU is detached, but also occurs in
conjunction with a system crash or SETS.

### Response

If the BS2000 system is no longer running and was not terminated intentionally, please
perform a SLED to back up the diagnostic data.

## HAL0313

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0313 BS2000 STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP SIGP RESET

### Meaning

BS2000 has reset the processor concerned using an SIGP instruction.

## HAL0314

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0314 BS2000 STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP SIGP STORE-STATUS

### Meaning

BS2000 used an SIGP instruction to request that diagnostic data about the current state of
the processor concerned be saved.

## HAL0315

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0315 BS2000 STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP START DUMP

### Meaning

The processor concerned has been stopped because a dump IPL has been started by
BS2000 (Crash Restart).

## HAL0316

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0316 BS2000 STOP GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP START IPL

### Meaning

The processor concerned has been stopped because an IPL has been started by BS2000
(Shutdown Restart).

## HAL0321

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0321 BS2000 START GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP SIGP

### Meaning

BS2000 has started the processor concerned with an SIGP instruction.

## HAL0322

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0322 BS2000 START GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP IPL-RESTART

### Meaning

The master debugging interface has been used by either mdebug or RMAassist to start the
processing of BS2000 instructions directly after a new IPL boot block has been loaded. This
is the last step in normal IPL processing.

## HAL0440

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

HAL0440 IOD ABORT GPXX SSSSSSSSSSSSSSSS PPPPPPPPPPPPPPPP IOD-ABEND

### Meaning

An error has been recognized by the input/output driver and processing has been
terminated. In the case of a BS2000 restart and a DIPL into the running system, this
message is normal and can be ignored.

### Response

Examine the proceeding messages on the BS2000 console for information as to the cause
of the problem.

©2025 Fujitsu | BS2000 System Messages