## VMSCOPY

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMSCOPY Copyright (C) (&01) (&00). All rights reserved

## VMS0000

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0000 MONITOR SYSTEM TERMINATED. VM2000 TERMINATION

### Meaning

Because of a non-interruptible IDLE in the monitor system, the hypervisor
stops all activities.

## VMS0004

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0004 HYPERVISOR INCONSISTENCY. TAKE SLED

### Meaning

Termination of VM2000.

## VMS0007

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0007 ILLEGAL GLOBAL INTERRUPT. TAKE SLED

### Meaning

Termination of VM2000.

## VMS0008

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0008 PE IN HYPERVISOR AT ADDRESS: (&00); EC: (&01). TAKE SLED

### Meaning

Program error (PE) in the hypervisor.
(&00): Address in the hypervisor
(&01): Program interruption code (EC).

### Response

Send the dump to the diagnosis department.

## VMS0009

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0009 TEST HPVC PROCESSED. VM2000 TERMINATION

### Meaning

VM2000 was stopped with the help of a "test" hypervisor call for
diagnostic reasons.

## VMS0012

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0012 MACHINE CHECK INTERRUPT: SYSTEM DAMAGE

### Meaning

Termination of VM2000.

## VMS0013

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0013 MACHINE CHECK INTERRUPT: CHANNEL SUBSYSTEM DAMAGE

### Meaning

Termination of VM2000.

## VMS0014

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0014 MACHINE CHECK INTERRUPT: PROCESSOR DAMAGE

### Meaning

An equipment malfunction, HW or FW, occured.

### Response

Contact the system administrator.

## VMS0016

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0016 HYPERVISOR STACK ERROR. TAKE SLED

### Meaning

Hypervisor program stack overflow or underflow.

## VMS0017

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0017 CPU (&00) detached by system

### Meaning

The real CPU has been detached by system because of a hardware failure.
(&00): Number of the real CPU

### Response

Contact the service technician.

## VMS0018

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0018 MONITOR SYSTEM TERMINATED. VM2000 ADMINISTRATION NO LONGER POSSIBLE

### Meaning

Crash in the monitor system without a restart option or a restart
failure. At least one guest system is still running.

### Response

Perform SHUTDOWN of all guest systems if possible or try to restart the
monitor system via SVP (if the model supports this function).

## VMS0019

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0019 MAIN MEMORY NOT CONTIGUOUS. VM2000 TERMINATION

### Meaning

Possible reasons:
- The logical storage segments do not have contiguous absolute addresses.
- The main memory information is inconsistent.

### Response

Contact the service technician.

## VMS0020

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0020 System device '(&00)' cannot be assigned (CC (&01)). Startup aborted

### Meaning

Error during assignment of a public disc or console to the Monitor VM.
(&00): Mnemonic device name
(&01): Condition Code

## VMS0021

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0021 CPU (&00) detached by system. Reply (EOT)

### Meaning

The real CPU has been detached by system because of a hardware failure.
To guarantee that the message will not be ignored an acknowledge is
requested.
(&00): Number of the real CPU

### Response

Contact the service technician.

## VMS0022

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0022 SPECIFIED HYPERVISOR SIZE TOO SMALL. STARTUP ABORTED

### Response

Modify the HYPERVISOR-SIZE parameter and start the system anew.

## VMS0023

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0023 CPU (&00) attached by system

### Meaning

Due to a CPU failure a spare CPU has been attached by system.
(&00): Number of the real CPU

## VMS0024

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS0024 CPU (&00) attached by system. Reply (EOT)

### Meaning

Due to a CPU failure a spare CPU has been attached by system.
To guarantee that the message will not be ignored, an
acknowledge is requested.
(&00): Number of the real CPU

### Response

Where appropriate contact the service technician.

## VMS0025

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS0025 CPU '(&00)' SWITCHED BY SYSTEM FROM CPU POOL '(&01)' TO CPU POOL '(&02)'

### Meaning

Due to a CPU failure VM2000 changes the CPU pool assignment
of the specified CPU.
(&00): CPU identification
(&01): Identification of the source CPU pool
(&02): Identification of the target CPU pool

## VMS0026

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS0026 CPU POOL ASSIGNMENT OF VIRTUAL MACHINE ((&00),(&01)) CHANGED BY SYSTEM FROM CPU POOL '(&02)' TO CPU POOL '(&03)'

### Meaning

Due to a CPU failure VM2000 changes the CPU pool assignment
of the specified virtual machine.
(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Identification of the source CPU pool
(&03): Identification of the target CPU pool

## VMS0027

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS0027 CPU POOL ASSIGNMENT OF VM GROUP '(&00)' CHANGED BY SYSTEM FROM CPU POOL '(&01)' TO CPU POOL '(&02)'

### Meaning

Due to a CPU failure VM2000 changes the CPU pool assignment
of all virtual machines assigned to the specified VM group.
(&00): Name of the VM group
(&01): Identification of the source CPU pool
(&02): Identification of the target CPU pool

## VMS1000

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1000 YOU HAVE ALREADY OPENED AN ADMINISTRATION DIALOG TO VIRTUAL MACHINE ((&00), (&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

### Response

If necessary, issue /END-VM-DIALOG.

## VMS1001

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1001 FOR THE VIRTUAL MACHINE ((&00),(&01)) AN ADMINISTRATION DIALOG VIA $VMCONS IS ALREADY OPENED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS1002

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1002 VM2000 COMMAND NOT PERMITTED FOR THE MONITOR VM. /(&00) REJECTED

## VMS1003

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1003 NO AUTHORIZATION EXISTS TO ADMINISTER OTHER VIRTUAL MACHINES. /(&00) REJECTED

### Meaning

The VM administrator may administer only the VM connected to his own
terminal.

## VMS1004

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1004 NO AUTHORIZATION EXISTS TO ISSUE VM2000 ADMINISTRATOR COMMANDS. /(&00) REJECTED

### Meaning

This command may only be used by the VM2000 administrator.

## VMS1009

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1009 VM2000 COMMAND NOT PERMITTED FROM A VM2000 CONSOLE. /(&00) REJECTED

## VMS1010

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1010 YOU ARE NOT CONNECTED WITH A VIRTUAL MACHINE. /(&00) REJECTED

### Response

Establish a logical link between the terminal and the VM by means of a
/BEGIN-VM-DIALOG command.

## VMS1012

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1012 PARTNER HAS TERMINATED AN ADMINISTRATION DIALOG WITH VIRTUAL MACHINE ((&00),(&01)). ADMINISTRATION-ID USED: (&02)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Authorization-Name given by UCON or TSN of user task

## VMS1013

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1013 PARTNER '(&00)' HAS STARTED AN ADMINISTRATION DIALOG WITH VIRTUAL MACHINE ((&01),(&02)). ADMINISTRATION-ID USED: (&03)

### Meaning

(&00): Identification of the partner
(&01): Index of the virtual machine
(&02): Name of the virtual machine
(&03): Authorization-Name given by UCON or TSN of the user task

## VMS1015

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1015 THERE IS NO VM ADMINISTRATOR FOR THE VIRTUAL MACHINE ((&00),(&01)). /(&02) REJECTED

### Meaning

The command can be processed only if there is a VM administrator
connected to the virtual machine.
(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS1016

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1016 PARTNER '(&00)' TRIES TO ESTABLISH CONNECTION TO VIRTUAL MACHINE ((&01), (&02)) WITHOUT SUCCESS

### Meaning

(&00): Identification of the partner
(&01): Index of the virtual machine
(&02): Name of the virtual machine

### Response

If this message recurs with an identical partner identification, the
user's authorization should be checked for security reasons.

## VMS1024

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1024 INVALID PASSWORD FOR DIALOG-AUTHORIZATION WITH VM ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Reenter command with correct password.

## VMS1030

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1030 BCAM APPLICATION '$VMCONS' READY

## VMS1032

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1032 PARTNER HAS TERMINATED A VC DIALOG WITH VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS1033

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1033 PARTNER '(&00)' HAS STARTED A VC DIALOG WITH VIRTUAL MACHINE ((&01),(&02))

### Meaning

(&00): Identification of the partner
(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS1034

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1034 YOU HAVE ALREADY OPENED A VC DIALOG WITH VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS1035

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1035 MAXIMUM NUMBER OF ADMINISTRATION/VC DIALOGS FOR THE VIRTUAL MACHINE ((&00), (&01)) ALREADY REACHED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS1036

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1036 VC dialogs with the Monitor VM are not permitted

## VMS1037

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1037 NO CORRESPONDING DIALOG HAS BEEN STARTED FOR THE VIRTUAL MACHINE ((&00), (&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS1038

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS1038 VC dialogs are not permitted for user tasks

### Meaning

A VC dialog is only possible via a $VMCONS connection.

## VMS1039

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1039 THE SPECIFIED DIALOG TYPE IS NOT ALLOWED

## VMS1040

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1040 BCAM APPLICATION '$VMCONS' NO LONGER AVAILABLE

## VMS1050

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS1050 VC DIALOG WITH KVP '(&02)' OF VIRTUAL MACHINE ((&00),(&01)) COULD NOT BE ESTABLISHED

### Meaning

(&00): Index of virtual machine
(&01): Name of virtual machine
(&02): Mnemonic device name of KVP output path

### Response

Check the corresponding KVP user id (password) and
retry the command later.

## VMS1051

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS1051 VC DIALOG WITH KVP '(&02)' OF VIRTUAL MACHINE ((&00),(&01)) TERMINATED ABNORMALLY

### Meaning

(&00): Index of virtual machine
(&01): Name of virtual machine
(&02): Mnemonic device name of KVP output path

### Response

Try to establish the VC dialog again by command
/BEGIN-VM-DIALOG TYPE=*VC.

## VMS1502

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1502 LOG ON TIMEOUT. NO DIALOG WITH '$VMCONS' INITIATED

### Meaning

/BEGIN-VM-DIALOG not issued within the time limit.

## VMS1505

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1505 PROCEDURE MODE ALREADY ACTIVE FOR THE REQUESTED VIRTUAL MACHINE

### Meaning

Only one procedure can be active at a time for a virtual machine.

### Response

Try again later.

## VMS1506

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1506 PROCEDURE FILE '(&00)' NOT OF TYPE 'SAM' OR 'ISAM'

### Meaning

(&00): Name of the procedure file.

## VMS1507

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1507 INVALID PARAMETER(S) IN CONTINUATION LINE. '/(&00)' REJECTED

## VMS1508

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1508 COMMAND '/(&00)' IN PROCEDURE TOO LONG

## VMS1509

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1509 COMMAND IN PROCEDURE IS NOT PREFIXED WITH '/'. INPUT REJECTED

## VMS1520

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1520 VM/GS PREFIX NOT YET GENERATED. INPUT REJECTED

## VMS1521

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1521 PARTNER CANNOT BE REACHED. DCAM RETURN INFORMATION: '(&00)'

### Meaning

(&00): DCAM return information.

## VMS1522

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1522 MAXIMUM NUMBER OF ADMINISTRATION/VC DIALOGS ALREADY REACHED. INPUT REJECTED

## VMS1523

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1523 Connecting to $CONSOLE failed. Dialog via $VMCONS not possible

### Meaning

The reason has been usually output in a preceding message NBR0717.

### Response

Please check, if the use of $VMCONS has been prepared correctly.

## VMS1524

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1524 MAXIMUM NUMBER OF APPLICATIONS CONNECTED TO $CONSOLE ALREDY REACHED. NEW DIALOG VIA $VMCONS IMPOSSIBLE

## VMS1531

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1531 CONNECTION TO PARTNER ((&00),(&01)) SEVERED BY '$VMCONS'. ADMINISTRATION-ID USED: (&02)

### Meaning

The messages addressed to partner ((&00),(&01)) have not been picked up,
despite of repeated prompts to do so, or the network connection has been
interrupted. /END-VM-DIALOG was initiated due '$VMCONS'.
(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Authorization-Name given by UCON.

## VMS1540

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1540 (&00)

### Meaning

(&00): VM2000 command output text

## VMS1561

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1561 PROCEDURE FILE '(&00)' NOT CATALOGED

### Meaning

(&00): Name of the Procedure File

## VMS1562

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1562 ERROR 'DMS(&01)' DURING OPENING OF THE PROCEDURE FILE '(&00)'

### Meaning

(&00): Name of the Procedure File
(&01): DMS return code

### Response

The cause of the DMS error message can be detected with
/HELP-MSG-INFORMATION DMS(&01).

## VMS1563

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1563 ERROR 'DMS(&01)' DURING ACCESSING THE PROCEDURE FILE '(&00)'

### Meaning

(&00): Name of the Procedure File
(&01): DMS return code

### Response

The cause of the DMS error message can be detected with
/HELP-MSG-INFORMATION DMS(&01). After the correction of
the error the procedure can be recalled.

## VMS1564

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1564 ERROR 'DMS(&01)' DURING CLOSING THE PROCEDURE FILE '(&00)'

### Meaning

(&00): Name of the Procedure File
(&01): DMS return code

### Response

The cause of the DMS error message can be detected with
/HELP-MSG-INFORMATION DMS(&01).

## VMS1600

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1600 INPUT FROM VC DIALOG IGNORED. REASON: '(&00)'

### Meaning

An input from a VC dialog could not be processed correctly.
(&00): '01', the virtual machine is not initialized
'02', either a virtual console is not defined for the virtual
machine or has not been attached to the guest system,
'03', input is longer than 256 characters
'04', the last input has not yet been completely processed
'05', the virtual machine is inoperable

## VMS1601

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1601 USER ERROR '(&02)' AT VC DIALOG WITH VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): '01', the virtual machine is not initialized
'02', a virtual console is no longer specified for the
virtual machine
'03', a command input medium is not assigned to the
virtual machine

### Response

If '01': Create VM again by means of /CREATE-VM
'02': Specify the virtual console by means of /ADD-VM-DEVICES
'03': Assign a command input medium with /BEGIN-VM-DIALOG
and restart the virtual machine with /START-VM.

## VMS1602

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS1602 SOME OUTPUT MESSAGES TO VC DIALOG WITH THE VIRTUAL MACHINE ((&00),(&01)) MAY HAVE BEEN LOST

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

If necessary look for missing messages in the KVP logging or
the BS2000 console logging.

## VMS2000

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2000 VIRTUAL MACHINE ((&00),(&01)) ALREADY IN WAIT STATE

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS2001

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2001 VIRTUAL MACHINE ((&00),(&01)) NOT IN WAIT STATE

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS2002

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2002 NO ADDRESS STOP SET AT LOCATION ('(&00)',(&01)) FOR VIRTUAL MACHINE ((&02), (&03)). /(&04) REJECTED

### Meaning

The address stop at the specified location does not exist or has been
overwritten.
(&00): Address where the stop was expected
(&01): Address mode (virtual/real)
(&02): Index of the virtual machine
(&03): Name of the virtual machine.

## VMS2003

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2003 ADDRESS STOP AT LOCATION ('(&00)',(&01)) FOR VIRTUAL MACHINE ((&02),(&03)) NOT ACCESSIBLE

### Meaning

The address stop could not be processed, because the page concerned is
currently not available in main memory.
(&00): Address where the stop was expected
(&01): Address mode (virtual/real)
(&02): Index of the virtual machine
(&03): Name of the virtual machine.

## VMS2004

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2004 MAXIMUM NUMBER OF ADDRESS STOPS ((&00)) HAS ALREADY BEEN REACHED FOR VIRTUAL MACHINE ((&01),(&02)). /(&03) REJECTED

### Meaning

(&00): Maximum number of the address stops for one VM
(&01): Index of the virtual machine
(&02): Name of the virtual machine.

## VMS2005

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2005 VIRTUAL MACHINE ((&00),(&01)) STOPPED AT LOCATION ('(&02)',(&03)), CPU (&04)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Location at which the virtual machine was stopped
(&03): Address mode (virtual/real)
(&04): Number of the virtual CPU

## VMS2006

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2006 EXPECTED-CONTENTS=X'(&00)' DOES NOT MATCH MEMORY CONTENTS OF VIRTUAL MACHINE ((&01),(&02)). /(&03) REJECTED

### Meaning

(&00): Contents of the EXPECTED-CONTENTS operand
(&01): Index of the virtual machine
(&02): Name of the virtual machine.

### Response

Correct the value of the EXPECTED-CONTENTS operand in the
/MODIFY-VM-MEMORY(-CONTEXT) command and reissue the command.

## VMS2007

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2007 LOCATION '(&00)' ((&01)) DOES NOT EXIST FOR VIRTUAL MACHINE ((&02),(&03)) /(&04) REJECTED

### Meaning

If the address is real in the VM domain then it lies outside the domain
of the virtual machine.
If the address is virtual, then in the corresponding guest system of the
virtual machine it could not be translated.
(&00): Location lying outside the specified domain
(&01): Address mode (virtual/real)
(&02): Index of the virtual machine
(&03): Name of the virtual machine.

## VMS2008

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2008 AREA IS NOT ADDRESSABLE FOR VIRTUAL MACHINE ((&03),(&04)) (START ADDRESS '(&00)' ((&01)), LENGTH '(&02)'). /(&05) REJECTED

### Meaning

If the address is real, then part of the specified area lies outside
the domain of the virtual machine.
If the address is virtual, then an address within the domain could not
be translated in the guest system of the virtual machine.
(&00): Start address of the specified area
(&01): Address mode (virtual/real/ESA)
(&02): Length of the specified domain in bytes
(&03): Index of the virtual machine
(&04): Name of the virtual machine

## VMS2009

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2009 VIRTUAL ADDRESS '(&00)' OF VIRTUAL MACHINE ((&01),(&02)) NOT ACCESSIBLE. /(&03) REJECTED

### Meaning

The virtual address could not be processed because the page concerned
is currently not available in main memory or the address stop code
has been changed.
(&00): Virtual address which could not be found because the page
concerned is not currently available in main memory
(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS2010

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2010 ALL THE ADDRESS STOPS OF VIRTUAL MACHINE ((&00),(&01)) COULD NOT BE REMOVED

### Meaning

The address stops could not all be removed, because the pages concerned
are not currently available in main memory or the address stop code has
been changed.
(&00): Index of the virtual machine
(&01): Name of the virtual machine.

### Response

Request a list of the address stops with the help of the
/SHOW-VM-ATTRIBUTES command.

## VMS2011

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2011 CPU (&00) OF VIRTUAL MACHINE ((&01),(&02)) STOPPED

### Meaning

(&00): Number of the virtual CPU.
(&01): Index of the virtual machine.
(&02): Name of the virtual machine.

## VMS2012

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2012 VIRTUAL MACHINE ((&00),(&01)) PLACED IN WAIT STATE BY THE VM2000 ADMINISTRATOR

### Meaning

This wait state can be cancelled only by the VM2000 administrator.
(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS2014

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2014 VM2000 PROGRAM ERROR. MODULE '(&00)', LABEL '###(&01)', ERROR CODE '(&02)'

### Meaning

The monitoring task
continues command processing at a consistent label, VM2000 can be
continued.
(&00): Name of the VM2000 module in which the error occurred
(&01): Label in the VM2000 module (&00)
(&02): Further error information.

### Response

In case one of the above errors occurred the VM2000 developers'
department should be informed about errors not yet known and diagnostic
documents should be sent (see VM2000 manual, chapt. "Error handling
in VM2000").

## VMS2016

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2016 VIRTUAL MACHINE ((&00),(&01)) RESUMED BY THE VM2000 ADMINISTRATOR

### Meaning

The VM2000 administrator has issued a /START-VM or /RESUME-VM command.
(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS2019

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2019 AREA OF VIRTUAL MACHINE ((&03),(&04)) IS NOT ACCESSIBLE (START ADDRESS '(&00)' ((&01)), LENGTH '(&02)'). /(&05) REJECTED

### Meaning

The specified area lies in a page which has been outpaged.
(&00): Start address of the specified area
(&01): Address mode (virtual/real/ESA)
(&02): Length of the specified area in bytes
(&03): Index of the virtual machine
(&04): Name of the virtual machine.

## VMS2020

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2020 VIRTUAL MACHINE ((&00),(&01)) REMAINS IN WAIT STATE. FOR FURTHER INFORMATION ISSUE /SHOW-VM-ATTRIBUTES

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS2021

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2021 VIRTUAL MACHINE ((&00),(&01)) TERMINATED BY THE VM2000 ADMINISTRATOR

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS2022

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2022 ADDRESS STOP AT LOCATION ('(&00)',(&01)) ALREADY SET FOR VIRTUAL MACHINE ((&02),(&03)). /(&04) REJECTED

### Meaning

(&00): Address where the stop point is to be set
(&01): Address mode (virtual/real)
(&02): Index of the virtual machine
(&03): Name of the virtual machine.

## VMS2023

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2023 CPU (&00) OF VIRTUAL MACHINE ((&01),(&02)) STARTED

### Meaning

(&00): Number of the virtual CPU.
(&01): Index of the virtual machine.
(&02): Name of the virtual machine.

## VMS2024

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2024 ADDRESS STOP AT LOCATION ('(&00)',(&01)) FOR VIRTUAL MACHINE ((&02),(&03)) OVERWRITTEN. /(&04) REJECTED

### Meaning

(&00): Address where the stop was expected
(&01): Address mode (virtual/real)
(&02): Index of the virtual machine
(&03): Name of the virtual machine.

## VMS2028

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2028 ADDRESS STOP AT LOCATION ('(&00)',(&01)) FOR VIRTUAL MACHINE ((&02),(&03)) WAS SET BY THE VM2000 ADMINISTRATOR

### Meaning

The address stop could not be removed because the VM administrator may
only remove stops set by himself.
(&00): Address where the stop was expected
(&01): Address mode (virtual/real)
(&02): Index of the virtual machine
(&03): Name of the virtual machine

## VMS2029

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2029 ADDRESS STOP AT LOCATION ('(&00)',(&01)) FOR THE VIRTUAL MACHINE ((&02), (&03)) REMOVED

### Meaning

(&00): Address where the stop was before
(&01): Address mode (virtual/real)
(&02): Index of the virtual machine
(&03): Name of the virtual machine.

## VMS2033

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2033 '(&00)' FROM VM ((&01),(&02)) VIA SVP

### Meaning

(&00): Text of the SVP message.
(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS2035

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2035 MEASURING FACILITIES CURRENTLY BEING USED BY VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS2036

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2036 MESSAGE FROM VIRTUAL MACHINE ((&00),(&01)): '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Message text.

## VMS2037

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2037 NON-INTERRUPTIBLE WAIT STATE FOR VIRTUAL MACHINE ((&00),(&01)), CODE (&02), CPU (&03)

### Meaning

Possible reasons:
- The guest system reached a non-interruptible wait state.
- In the virtual machine a sequence of program interruptions
has occurred.
(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): WAIT STATE code in hexadecimal format
(&03): Number of the virtual CPU

## VMS2038

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2038 VIRTUAL MACHINE ((&00),(&01)) CURRENTLY IN TRACE-MODE

### Meaning

The command can be only be processed after completion of the preceding
trace-order.
(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Retry later.

## VMS2039

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2039 CPU(s) of virtual machine ((&00),(&01)) not assigned or inoperable

### Meaning

(&00) Index of the virtual machine
(&01) Name of the virtual machine

## VMS2050

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2050 GUEST SYSTEM ON VM ((&00),(&01)) READY

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS2051

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2051 GUEST SYSTEM ON VM ((&00),(&01)) DOWN; REASON: (&02)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Reason for state of guest system:
- SHUTDOWN
- CRASH:
The guest system failed due to a system error.
- ADMINISTRATOR COMMAND:
The guest system was terminated by a system administrator
via IPL or "Abort VM".
- VM-ADMINISTRATOR COMMAND:
a) /START-VM has been issued for a guest system which is
already operable.
b) The guest system was terminated via the command /RESET-VM.

## VMS2052

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2052 GUEST SYSTEM ON VM ((&00),(&01)) NOT READY. RESTART HAS BEEN INITIATED

### Meaning

Possible reasons:
- An automatic RESTART has been initiated after a system error
in the guest system
- SHUTDOWN with RESTART initiated in the guest system
(&00): Index of virtual machine
(&01): Name of virtual machine

## VMS2054

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2054 SHUTDOWN OF GUEST SYSTEM ON VM ((&00),(&01)) INITIATED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS2055

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2055 SHUTDOWN NOT RECEIPTED BY GUEST SYSTEM ON VM ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

It has to be checked by means of the command /SHOW-VM-ATTRIBUTES that
the virtual machine will reach the state DOWN. If a VM2000 shutdown
with unlimited waiting time is in progress, someone has to see to the
termination of the guest system so that the VM2000 shutdown can be
finished.

## VMS2056

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2056 SHUTDOWN OF GUEST SYSTEM ON VM ((&00),(&01)) ALREADY IN PROGRESS

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS2057

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2057 APPLIED SHUTDOWN INTERFACE NOT SUPPORTED BY GUEST SYSTEM ON VM ((&00), (&01))

### Meaning

Either the guest system is still in the startup phase or
the applied function is not supported by the guest system.
(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

After SYSTEM READY the guest system can be terminated by
the command /SHUTDOWN from its BS2000 console. Furthermore
the shutdown of the guest system can be initiated by the
VM administrator with /SHUTDOWN-VM.

## VMS2058

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2058 SHUTDOWN REJECTED OR PROCESSED WITH WARNINGS BY GUEST SYSTEM ON VM ((&00), (&01)). REASON: (&02)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Message number (error cause in guest system)

## VMS2059

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2059 SHUTDOWN OF GUEST SYSTEM ON VM ((&00),(&01)) ABORTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

If a VM2000 shutdown with unlimited waiting is in progress, it has to
be seen to the completion of the shutdown of the guest system, so that
the shutdown of VM2000 can also be completed.

## VMS2070

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2070 VM ((&00),(&01)) IN WAIT STATE

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS2100

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2100 VM2000 SHUTDOWN INITIATED

## VMS2101

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

VMS2101 VM2000 SHUTDOWN IN PROGRESS. /(&00) REJECTED

### Meaning

(&00): Command

## VMS2102

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

VMS2102 VM2000 SHUTDOWN REJECTED BECAUSE NO APPROPRIATE MONITOR SYSTEM IS RUNNING

## VMS2103

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

VMS2103 UNLIMITED WAITING FOR SHUTDOWN OF GUEST SYSTEM NOT PERMITTED

### Meaning

A virtual machine is in state IN HOLD (WAIT) or the guest system
running on the virtual machine does not support the called function.

### Response

Please repeat /SHUTDOWN-VM after the wait state of the virtual machine
has been suspended by /RESUME-VM or the operator has terminated the
guest system.

## VMS2104

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2104 VM2000 SHUTDOWN INITIATED ALTHOUGH A VIRTUAL MACHINE IS IN WAIT STATE

### Meaning

Virtual machines which are in state IN HOLD (WAIT) will be terminated
independently of their state by force after the waiting time in the
monitor system has expired.

## VMS2105

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

VMS2105 /ENTER-JOB CANNOT BE PROCESSED IN A GUEST SYSTEM. VM2000 SHUTDOWN REJECTED

### Meaning

/SHUTDOWN-VM with ACTION=*SHUTDOWN(...) has already been called
for a virtual machine.

## VMS2300

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2300 Definition of VM '(&00)' does not exist

### Meaning

(&00): Name of the virtual machine

## VMS2301

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2301 Definition of VM '(&00)' created

### Meaning

(&00): Name of the virtual machine

## VMS2302

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2302 Definition of VM '(&00)' deleted

### Meaning

(&00): Name of the virtual machine

## VMS2303

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2303 Definition of VM '(&00)' not accessible

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- The data communication system in BS2000 (BCAM) is not ready.
- No Management Unit is ready.
- There is a definition of a persistent virtual machine in the
storage for VM definitions that has the same name as an already
initialized (not persistent) virtual machine.
(&00): Name of the virtual machine

### Response

A name conflict is reported by the message VMS2360 (requiring a
response) on the console of the monitor system. The conflict may
be resolved
- by deleting the definition of the persistent virtual machine
and replacing it by the definition of the already initialized
virtual machine or
- by terminating and deleting the already initialized virtual machine.
The first alternative solution will be processed automatically if the
message VMS2360 is answered with "Y". The second one has to be processed
manually by the VM or VM2000 administrator before the message VMS2360
is answered with "N".
After resolving a name conflict, there may occur further conflicts,
which have to be resolved in the same way.

## VMS2305

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2305 Definition of VM '(&00)' could not be created. /(&01) rejected

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- No Management Unit is ready.
- The connection to a Management Unit via the BS2000 data communication
system (BCAM) has been disturbed.
(&00): Name of the virtual machine
(&01): Command

### Response

Try to remove the error cause and repeat the command, please.

## VMS2306

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2306 Definition of VM '(&00)' could not be updated

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- No Management Unit is ready.
- The connection to a Management Unit via the BS2000 data communication
system (BCAM) has been disturbed.
VM2000 attempts periodically to subsequently update the VM definition.
(&00): Name of the virtual machine

## VMS2307

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2307 Definition of VM '(&00)' could not be modified. /(&01) rejected

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- No Management Unit is ready.
- The connection to a Management Unit via the BS2000 data communication
system (BCAM) has been disturbed.
(&00): Name of the virtual machine
(&01): Command

### Response

Try to remove the error cause and repeat the command, please.

## VMS2308

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2308 Definition of VM '(&00)' could not be deleted

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- No Management Unit is ready.
- The connection to a Management Unit via the BS2000 data communication
system (BCAM) has been disturbed.
VM2000 attempts periodically to subsequently delete the VM definition.
(&00): Name of the virtual machine

## VMS2309

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2309 Definition of VM '(&00)' could not be deleted. /(&01) rejected

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- No Management Unit is ready.
- The connection to a Management Unit via the BS2000 data communication
system (BCAM) has been disturbed.
(&00): Name of the virtual machine
(&01): Command

### Response

Try to remove the error cause and repeat the command, please.

## VMS2310

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2310 Processing of /(&00) for VM definition '(&01)' not acknowledged in time

### Meaning

Problem in the communication with an external administration
component of the VM2000 system. It is uncertain whether the command
has been processed.
(&00): Command
(&01): Name of the VM definition

### Response

Please check the VM definition with /SHOW-VM-DEFINITION. You have
possibly to repeat the command. If even a repetition does not work,
please contact the service.

## VMS2311

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2311 MAXIMUM NUMBER ((&00)) OF VM DEFINITIONS ALLOWED ALREADY REACHED. /(&01) REJECTED

### Response

If necessary, delete a VM definition.

## VMS2312

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2312 NO VM DEFINITION WITH MATCHING VM NAME FOUND

## VMS2313

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2313 Device '(&00)' specified with different usage type. /(&01) rejected

### Meaning

Maybe the device was specified by a device range or a
wildcard specification.
(&00): Mnemonic device name
(&01): Command

## VMS2314

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2314 Device usage conflict between pubset device '(&00)' and its pubres device '(&02)' during assignment to VM '(&01)'

### Meaning

Pubset devices are specified in a VM definition by the respective
pubres device. Additionally, one of these pubset devices is specified
explicitly by its mnemonic device name but with a different device
usage than the pubres device.
(&00): Mnemonic device name of pubset device
(&01): Name of the virtual machine
(&02): Mnemonic device name of pubres device

## VMS2315

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2315 Device '(&00)' already inserted with another type of usage in the definition of VM '(&01)'

### Meaning

(&00): Mnemonic device name
(&01): Name of the virtual machine

## VMS2316

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2316 VM index (&00) in VM definition '(&01)' greater than current maximum number ((&02)) of virtual machines. /(&03) rejected

### Meaning

(&00): VM index
(&01): Name of the VM definition
(&02): Current maximum number of VMs
(&03): Command

### Response

If the VM name is not a standard VM name, the VM index can be modified
with MODIFY-VM-DEFINITION.

## VMS2317

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2317 Memory values not suitable with already inserted values in the definition of VM '(&00)'

### Meaning

(&00): Name of the virtual machine

## VMS2318

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2318 VM index (&00) in VM definition '(&01)' already used by an initialized virtual machine. /(&02) rejected

### Meaning

(&00): VM index
(&01): Name of the VM definition
(&02): Command

### Response

The VM index can be modified with MODIFY-VM-DEFINITION.

## VMS2320

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2320 Definition of VM '(&00)' migrated to target SU '(&01)'

### Meaning

(&00): Name of the virtual machine
(&01): Name of the Server Unit to which the definition of the
virtual machine has been migrated (target SU)

## VMS2321

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2321 Definition of VM '(&00)' successfully created on target SU '(&01)', but error at the deletion of the local definition

### Meaning

(&00): Name of the virtual machine
(&01): Name of the Server Unit to which the definition of the
virtual machine has been migrated (target SU)

### Response

Please check with the help of /SHOW-VM-DEFINITION if
the VM definition does still exist locally. In this case
delete the VM definition with /DELETE-VM-DEFINITION, please.
If this command fails too, please contact the service.

## VMS2323

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2323 Definition of VM '(&00)' could not be migrated to target SU '(&01)'. /(&02) rejected

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- No Management Unit is ready.
- The inquiry of the cluster configuration has failed.
- The DNS entry of the target SU is inconsistent.
- The target SU (&01) has delivered an unexpected
HTTP status code.
(&00): Name of the virtual machine
(&01): Name of the Server Unit to which the definition of the
virtual machine should have been migrated (target SU)
(&02): Command

## VMS2324

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2324 Migration of the definition of VM '(&00)' rejected by target SU '(&01)'. Reason: (&02)

### Meaning

The reason for the rejection on the target SU (&01) can be
determined by /HELP-MSG for the message number which is issued
in the last insert of the message.
(&00): Name of the virtual machine
(&01): Name of the Server Unit to which the definition of the
virtual machine should have been migrated (target SU)
(&02): String which is composed of a VM2000 message number and
corresponding message inserts

## VMS2325

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2325 Migration of the definition of VM '(&00)' not acknowledged in time by target SU '(&01)'

### Meaning

Problem in the communication with an external administration
component of the VM2000 system.
The VM definition has not been deleted locally. Possibly, the
VM definiton has been already created on the target SU (&01).
(&00): Name of the virtual machine
(&01): Name of the Server Unit to which the definition of the
virtual machine should have been migrated (target SU).

### Response

Please check if the VM definition has been already created on
the target SU. In this case delete the local VM definition with
/DELETE-VM-DEFINITION, please. Otherwise repeat the command. If
even a repetition does not cause the creation of the VM definition
on the target SU, please contact the service.

## VMS2330

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2330 Storage for VM definitions accessible

## VMS2331

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2331 Storage for VM definitions not accessible

## VMS2332

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2332 Storage for VM definitions not accessible. /(&00) rejected

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- The data communication system in BS2000 (BCAM) is not ready.
- No Management Unit is ready.
- There is a definition of a persistent virtual machine in the
storage for VM definitions that has the same name as an already
initialized (not persistent) virtual machine.
(&00): Command

### Response

A name conflict is reported by the message VMS2360 (requiring a
response) on the console of the monitor system. The conflict may
be resolved
- by deleting the definition of the persistent virtual machine
and replacing it by the definition of the already initialized
virtual machine or
- by terminating and deleting the already initialized virtual machine.
The first alternative solution will be processed automatically if the
message VMS2360 is answered with "Y". The second one has to be processed
manually by the VM or VM2000 administrator before the message VMS2360
is answered with "N".
After resolving a name conflict, there may occur further conflicts,
which have to be resolved in the same way.

## VMS2340

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2340 Definition of VM '(&00)' recovered from remote SU '(&01)'

### Meaning

(&00): Name of the virtual machine
(&01): Name of the remote Server Unit

## VMS2341

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2341 No unique remote SU found

### Meaning

There is not exactly one remote Server Unit in the cluster
in which the local Server Unit can be found.

## VMS2342

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2342 Specified remote SU '(&00)' is equal to local SU

### Meaning

(&00): Name of the remote Server Unit

## VMS2343

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2343 Specified remote SU '(&00)' not in SU cluster with local SU

### Meaning

(&00): Name of the remote Server Unit

## VMS2344

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2344 Remote SU '(&00)' must not be running. /(&01) rejected

### Meaning

(&00): Name of the remote Server Unit
(&01): Command

## VMS2345

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2345 Definition of VM '(&00)' could not be recovered from remote SU '(&01)'

### Meaning

Possible reason:
- The subsystem REWAS is not available.
- The subsystem REWAS has reported an internal error.
- The data communication system in BS2000 (BCAM) is not ready.
- The inquiry of the cluster configuration has failed.
- The DNS entry of the remote Server Unit is inconsistent.
- The Management Unit (MU) of the remote Server Unit has
delivered an unexpected HTTP status code.
(&00): Name of the virtual machine
(&01): Name of the remote Server Unit
SU: Server Unit

## VMS2346

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2346 Definition of VM '(&00)' becomes ambiguous in SU cluster

### Meaning

At the recovery of the VM definition from the remote Server Unit,
the deletion on the remote Server Unit failed at first and then
during the error recovery the deletion on the local Server Unit
failed.
(&00): Name of the virtual machine

### Response

Avoid to activate and start the VM definition on the local as well as
on the remote Server Unit, please. If the data communication system
in BS2000 (BCAM) is ready, try to delete the VM definition locally by
/DELETE-VM-DEFINITION and repeat the command.

## VMS2347

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2347 Local SU not found in any SU cluster. /(&00) rejected

### Meaning

(&00): Command
SU: Server Unit

## VMS2350

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2350 Definition of active VM ((&00),(&01)) not found. Recreation initiated

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS2360

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2360 Ambiguous VM name '(&00)'. Is persistent VM definition to be deleted and replaced by definition of already initialized VM? Reply (Y=Yes; N=No)

### Meaning

There is a definition of a persistent virtual machine in the
storage for VM definitions that has the same name as an already
initialized (not persistent) virtual machine.
(&00): Name of the virtual machine

### Response

If you want to keep the initialized virtual machine, answer 'Y',
please. In this case the persistent definition will be deleted and
replaced by the definition of the initialized virtual machine.
If you want to preserve the persistent definition, terminate
(/SHUTDOWN-VM) and delete (/DELETE-VM) the initialized virtual
machine and AFTERWARDS answer 'N', please.

## VMS2400

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2400 Unknown SU '(&00)'. /(&01) rejected

### Meaning

(&00): Name of Server Unit specified in the command
(&01): Command

## VMS2401

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2401 Live migration of a VM already in progress

### Meaning

If this message is issued directly, a live migration of
a VM from the own to another SU is currently in progress.
If the message key is issued as insert of the message
VMS2404, then another VM is taken over currently by the
target SU due to a live migration.
SU: Server Unit

## VMS2402

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2402 Target SU '(&00)' unavailable

### Meaning

Possible causes:
- The target SU (&00) does not comply with the requirements for a
successful migration.
- The connection to the target SU (&00) could not be established.
(&00): Name of the Server Unit which should be the target of the
migration (target SU)

### Response

If the cause is not clear on SU /390, please increase the trace level
of the Monitor VM with /MODIFY-VM-ATTRIBUTES VM-ID=1,TRACE-LEVEL=*STD,
repeat the command and take a VMDUMP. After resetting the trace level
contact the service, please.

## VMS2403

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2403 Connection to target SU '(&00)' disturbed

### Meaning

(&00): Name of the Server Unit which should be the target of the
migration (target SU)

## VMS2404

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2404 Live migration of VM ((&00),(&01)) rejected by target SU '(&02)'. Reason: (&03)

### Meaning

The reason for the rejection on the target SU (&02) can be
determined by /HELP-MSG-INFORMATION for the message number
which is output in the last insert of the message.
(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should be migrated (target SU)
(&03): String which is composed of a VM2000 message number and
corresponding message inserts

## VMS2405

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2405 Live migration of VM ((&00),(&01)) in current state not permitted

### Meaning

Possible causes:
- A migration of the VM is already in progress.
- A memory reconfiguration for the VM is in progress.
- Start or restart of the VM is in progress.
- Shutdown of the VM which has been initiated by /SHUTDOWN-VM
is in progress.
- The VM has been terminated abnormally.
- The VM has been stopped by command.
(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS2406

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2406 Live migration not supported by guest system of VM ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS2407

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2407 Start of live migration to target SU '(&02)' rejected by guest system of VM ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2408

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2408 Start of live migration to target SU '(&02)' not confirmed in time by guest system of VM ((&00),(&01)). /(&03) rejected

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)
(&03): Command

## VMS2409

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2409 Live migration of VM ((&00),(&01)) to target SU '(&02)' rejected by administration component of VM system

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should be migrated (target SU)

## VMS2410

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2410 Target SU '(&00)' not in active SU cluster with source SU

### Meaning

Possible reasons:
- The inquiry of the cluster configuration has failed.
- The DNS entry of the target SU is inconsistent.
- The source SU is not in an active SU cluster
(with function "LM").
- The target SU has been specified, but it is not in the
same cluster SU as the source SU.
(&00): Name of the Server Unit to which the virtual machine
should be migrated (target SU)
SU: Server Unit

### Response

Please, check and correct the target SU name if it has been
specified. If necessary, let the service set up and activate
or appropriately extend an SU cluster.

## VMS2411

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2411 Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted after restart of monitor system

### Meaning

The live migration was aborted, because the message VMS2444 was
answered with "N" at the console of the monitor system.
(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2412

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2412 Monitor memory shortage. Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

### Response

Check the state of the system, please. Possibly, the
live migration can be processed a little bit later.

## VMS2413

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2413 Connection to target SU '(&02)' disturbed. Live migration of VM ((&00), (&01)) aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2414

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2414 Continuation of the live migration of VM ((&00),(&01)) to target SU '(&02)' rejected by guest system

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2415

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2415 Continuation of the live migration of VM ((&00),(&01)) to target SU '(&02)' not confirmed in time by guest system. Processing aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2416

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2416 Detach of device '(&03)' rejected by guest system. Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)
(&03): Mnemonic device name

## VMS2417

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2417 Detach of device '(&03)' not confirmed in time by guest system. Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)
(&03): Mnemonic device name

## VMS2418

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2418 Device '(&03)' is busy. Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)
(&03): Mnemonic device name

## VMS2419

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2419 Internal error. Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2420

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2420 Live migration of VM ((&00),(&01)) to target SU '(&02)' processed, but VM could not be deleted locally

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
has been migrated (target SU)

## VMS2421

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS2421 Live migration of VM ((&00),(&01)) aborted by VM2000 on target SU '(&02)'. Reason: (&03)

### Meaning

The reason for the abort on the target SU (&02) can be determined
by /HELP-MSG-INFORMATION for the message number which is output
in the last insert of the message.
(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)
(&03): String which is composed of a VM2000 message number and
the corresponding message inserts

## VMS2422

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2422 Error recovery or reconfiguration in progress. Live migration of VM ((&00), (&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

### Response

If a retry of the migration leads to an abort with the same
message, please take a VMDUMP and contact the service.

## VMS2423

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2423 Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted by administration component of VM system

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2424

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2424 VM deleted regardless to its state. Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2425

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2425 Changing memory pages cannot be transferred in time. Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

### Response

If the trace level of the Monitor VM is set to the default value *OFF,
please increase it with /MODIFY-VM-ATTRIBUTES VM-ID=1,TRACE-LEVEL=*STD.
Then try again to migrate the virtual machine. If the migration is
aborted with the same message, please take a VMDUMP and contact the
service.
If the trace level has been already set to *STD or *MAX, you can take
the VMDUMP directly without a retry of the migration.
You can determine the current trace level with the VMDUMP command 'S'.
If you have increased the trace level, you should reset it again.

## VMS2426

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2426 Hypervisor memory exhausted. Live migration of VM ((&00),(&01)) to target SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

### Response

Please check the specification of the hypervisor main memory size
in the startup parameter file of BS2000.
If there is specified HYPERVISOR-SIZE=*BY-SYSTEM (default value),
please take a VMDUMP and contact the service.
If there is specified an explicit value for the hypervisor main
memory size, this value may be too small. Possibly you can free
some space for the hypervisor by deleting a VM (of less importance).

## VMS2430

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2430 Live migration of VM ((&00),(&01)) from source SU '(&02)' started

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit from which the virtual machine
is migrating (source SU)

## VMS2431

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2431 Live migration of VM ((&00),(&01)) from source SU '(&02)' completed

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit from which the virtual machine
has been migrated (source SU)

## VMS2432

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2432 VM ((&00),(&01)) resumed at live migration from source SU '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit from which the virtual machine
is migrating (source SU)

## VMS2433

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2433 Live migration of VM ((&00),(&01)) from source SU '(&02)' completed with warnings in the guest system

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit from which the virtual machine
has been migrated (source SU)

### Response

Please look for the warnings in the KVP logging or the BS2000
console logging of the migrated VM.

## VMS2434

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2434 Live migration of VM ((&00),(&01)) from source SU '(&02)' aborted

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit from which the virtual machine
should have been migrated (source SU)

### Response

If the cause for the abort of the live migration is not evident,
please take a VMDUMP on the source SU and contact the service.

## VMS2436

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2436 Configuration of device '(&00)' on target SU not compatible with that on the source SU

### Meaning

(&00): Mnemonic device name
SU: Server Unit

### Response

Please check the device type of the affected I/O device.
SU /390: Please check the channel path identifiers (a subset of CHPIDs
must be same on both SUs) and the channel path availability
on the target SU.
If a channel path of the affected device is offline on the
target SU, attach it in the monitor system on the target SU.
If the affected device is a disk device, please check also
the zoning and LUN masking and then execute command
/CHECK-VM-DISK-CONFIGURATION on the target SU.
SU x86: Check the device generation (host connector and unit id) of
the affected device.
If the cause of the incompatibility is evident, please try to resolve
it or remove the affected device from the VM to be migrated.
In all other cases take a VMDUMP on both SUs and contact the service.

## VMS2437

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2437 Device '(&00)' not assignable to virtual machine on target SU

### Meaning

The device is already assigned (exclusively) to another VM.
(&00): Mnemonic device name
SU: Server Unit

## VMS2438

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2438 VM name not available on target SU

### Meaning

On a Server Unit (SU), VM names have to be unique.

## VMS2439

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2439 Migrating VM could not be established on target SU within time limit

### Meaning

Setup of the migrating VM on the target SU (including assignment
of all its devices) was not completed in time.
SU: Server Unit

### Response

If the assignment of some particular devices took several seconds
(cp. time stamps of VMS4005 in CONSLOG), please check the hardware
configuration and operability of the affected devices. In all other
cases take VMDUMP on the target SU and contact the service!

## VMS2440

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2440 Live migration of VM ((&00),(&01)) could not be aborted on target SU '(&02)' due to a connection error

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2441

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2441 Live migration of VM ((&00),(&01)) could not be aborted on target SU '(&02)' due to a connection error. Retry in progress

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

## VMS2442

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2442 Connection error at live migration of VM ((&00),(&01)). VM already resumed on target SU '(&02)'? Reply (Y=Yes; N=No)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

### Response

If the VM has already been resumed on the target SU, answer 'Y',
please. In this case the VM will be deleted locally. Otherwise
answer 'N', please. The live migration will be aborted.

## VMS2443

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2443 Abort of live migration of VM ((&00),(&01)) rejected by target SU '(&02)'. VM already resumed on target SU? Reply (Y=Yes; N=No)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

### Response

If the VM has already been resumed on the target SU, answer 'Y',
please. In this case the VM will be deleted locally. Otherwise
answer 'N', please. The live migration will be aborted locally.

## VMS2444

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2444 Monitor restart at live migration of VM ((&00),(&01)). VM already resumed on target SU '(&02)'? Reply (Y=Yes; N=No)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)

### Response

If the VM has already been resumed on the target SU, answer 'Y',
please. In this case the VM will be deleted locally. Otherwise
answer 'N', please. The live migration will be aborted locally.

## VMS2450

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2450 Live migration of VM ((&00),(&01)) to target SU '(&02)' started

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
is migrating (target SU)

## VMS2451

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2451 Live migration of VM ((&00),(&01)) to target SU '(&02)' completed

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
has been migrated (target SU)

## VMS2452

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2452 VM ((&00),(&01)) suspended at live migration to target SU '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
is migrating (target SU)

## VMS2460

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS2460 Live migration of VM ((&00),(&01)) to target SU '(&02)' possible

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should be migrated (target SU)

## VMS2461

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

VMS2461 Live migration of VM ((&00),(&01)) to target SU '(&02)' not possible

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should be migrated (target SU)

## VMS2462

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS2462 Requirements for live migration of VM ((&00),(&01)) to target SU '(&02)' not fulfilled. /(&03) rejected

### Meaning

Possible reasons have been output in previous messages.
(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
should have been migrated (target SU)
(&03): Command

## VMS2470

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

VMS2470 Specified target SU '(&00)' is equal to local SU

### Meaning

(&00): Name of target SU specified in the command
SU: Server Unit

## VMS2471

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

VMS2471 Device '(&00)' will be detached by live migration

### Meaning

(&00): Mnemonic device name

## VMS2472

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

VMS2472 Device '(&00)' (physically) different on target SU '(&01)'

### Meaning

1) If the device is assigned to the migrating VM:
The physical entity of the specified device on the target
SU (&01) differs from that on the source SU or cannot be
determined.
2) If the device is not assigned to the migrating VM (SU x86):
The device generation (type, host connector or unit id) of the
specified device on the target SU differs from that on the
source SU.
(&00): Mnemonic device name
(&01): Name of the Server Unit to which the virtual machine
is migrating (target SU)
SU: Server Unit

### Response

1) If this warning was issued for command /CHECK-VM-MIGRATION on SU /390
and the physical entity of the device is to be the same, first
execute command /CHECK-VM-DISK-CONFIGURATION (on the target SU
as well as on the source SU) to update both disk configurations.
Then repeat command /CHECK-VM-MIGRATION, please. If the physical
entity is still different, check the zoning and LUN masking.
2) Please try to resolve the inconsistent device generation. Note
that the persisting inconsistence would prohibit an assignment of
this device to the migrated VM on the target SU later on.

## VMS2480

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

VMS2480 Live migration of VM ((&00),(&01)) to target SU '(&02)' started in spite of warnings

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the Server Unit to which the virtual machine
is migrating (target SU)

### Response

Pay attention to the warnings, please.

## VMS3000

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS3000 VM2000 COMMAND /(&00) FOR VIRTUAL MACHINE ((&01),(&02)) PROCESSED SUCCESSFULLY

### Meaning

(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS3001

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3001 VM2000 COMMAND FOR VIRTUAL MACHINE ((&01),(&02)) COULD NOT BE PROCESSED SUCCESSFULLY. /(&00) REJECTED

### Meaning

(&01): Index of the virtual machine
(&02): Name of the virtual machine

### Response

Identify the error with the aid of the preceding messages and correct it,
then try again.

## VMS3002

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3002 INVALID VALUE OF OPERAND '(&00)' IN VM2000 COMMAND. /(&01) REJECTED

## VMS3003

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3003 INVALID COMBINATION OF '(&00)' AND '(&01)'. /(&02) REJECTED

## VMS3004

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3004 VALUE LIST OF OPERAND '(&00)' IN COMMAND '/(&01)' CONTAINS MULTIPLE SPECIFIED ELEMENTS

## VMS3005

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3005 COMMAND NOT SUPPORTED

## VMS3006

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3006 TRACE END FOR VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS3007

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3007 VM PROCEDURE PROCESSED FOR VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS3008

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3008 VM PROCEDURE FOR VIRTUAL MACHINE ((&00),(&01)) TERMINATED WITH ERRORS

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Correct the procedure and retry.

## VMS3010

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3010 ILLEGAL COMMAND IN PROCEDURE FILE. /(&00) REJECTED

## VMS3011

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3011 COMMAND '/(&00)' NOT SUPPORTED FOR THIS HSI

## VMS3012

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3012 OPERAND '(&00)' NOT SUPPORTED FOR THIS HARDWARE. /(&01) REJECTED

## VMS3014

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3014 /(&00) REJECTED FOR VIRTUAL MACHINE ((&01),(&02)) BECAUSE 'ADMIN-PRIVILEGES=*MIN' IS SPECIFIED

### Meaning

The privileged options open to the VM2000 administrator have been
limited by means of ADMIN-PRIVILEGES=*MIN.
(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS3015

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3015 PERIODIC OUTPUT OF MONITORING DATA ALREADY STARTED BY (&00) '(&01)'. COMMAND REJECTED

### Meaning

When a periodic output of monitoring data has been initiated for
a virtual machine by an administrator, a different administrator
may not interrupt the processing by issuing a new command.
(&00): Keyword: CONSOLE or TASK or APPLICATION
(&01): Identification of VM2000-Administrator:
Console Mnemonic or TSN or
Authorization Name of Authorized User Program

### Response

Stop running periodic output of monitoring data where required
and reenter the command.

## VMS3016

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3016 PERIODIC OUTPUT OF MONITORING DATA STARTED

## VMS3017

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3017 PERIODIC OUTPUT OF MONITORING DATA IS NOT BEING PERFORMED NOW. /(&00) REJECTED

### Meaning

If the command is entered with the default value *NO for the
parameter PERIOD, only the periodic display of the measurement
data is stopped.

### Response

You have to specify a time interval in seconds for the parameter PERIOD
if you want to collect and display periodically measurement data.

## VMS3018

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3018 No measurement object specified

## VMS3019

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS3019 No virtual machine with matching VM name found. Command rejected

## VMS3025

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3025 No monitoring data for last interval

## VMS3026

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3026 No monitoring data for SHOW-VM-STATUS *RECENT available

## VMS3027

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3027 Monitoring data collection for SHOW-VM-STATUS *RECENT aborted

## VMS3029

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3029 PERIODIC OUTPUT OF MONITORING DATA TERMINATED

## VMS3030

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3030 Operand '(&00)' not supported for this HSI

### Meaning

HSI: hardware/software interface.

## VMS3031

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3031 OPERAND '(&00)' NOT ALLOWED FOR VIRTUAL MACHINE ((&01),(&02))

## VMS3032

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3032 VALUE OF OPERAND '(&00)' NOT SUPPORTED FOR THIS HSI. /(&01) REJECTED

### Meaning

(&00): Name of operand

## VMS3033

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3033 ADMIN-PRIVILEGES=*MAX not allowed for the Monitor VM. Command rejected

## VMS3034

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3034 ADMIN-PRIVILEGES=*MIN only allowed for the Monitor VM. Command rejected

## VMS3035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3035 IO-PRIORITY privilege cannot be set for VM ((&00),(&01)). Command rejected

### Meaning

The total number of virtual CPUs of all VMs with the IO-PRIORITY
privilege may not exceed the number of available real CPUs.
(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS3036

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3036 VM-NAME and VM-INDEX do not correspond. Command rejected

## VMS3037

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3037 No select operand specified. Command rejected

### Meaning

Because the output of detailed information for all the devices may be
very extensive, explicit selection operands must be specified.
This is to avoid an unintended (longtime) blocking of the console
or the $VMCONS-dialog.

### Response

To obtain detailed information for all the devices, specify UNITS=*ALL.

## VMS3038

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3038 PERSISTENT=*YES not allowed for the Monitor VM. Command rejected

## VMS3040

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3040 COMMAND NOT PROCESSED FOR THE VIRTUAL MACHINE ((&00),(&01)) BECAUSE OF THE STATE OF THE VM

### Meaning

The command with the option CHECK-VM-STATE=*YES is only allowed for a
VM in the state "INIT-ONLY" or "DOWN".

### Response

If justifiable, reenter the command with CHECK-VM-STATE=*NO.

## VMS3041

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

VMS3041 COMMAND NOT PROCESSED FOR MIGRATING VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Please repeat the command, after the migration of the VM has been
finished!

## VMS3042

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

VMS3042 VIRTUAL MACHINE ((&00),(&01)) IS MIGRATING. /(&02) REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Command

### Response

Please retry the command, after the migration of the VM has been
finished!

## VMS3050

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3050 VIRTUAL MACHINE ((&00),(&01)) CREATED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS3051

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS3051 Virtual machine ((&00),(&01)) reset

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4000

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4000 VIRTUAL MACHINE ((&00),(&01)) NOT YET INITIALIZED. /(&02) REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

If necessary, initialize the VM concerned.

## VMS4001

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4001 No virtual machine with matching VM name found

## VMS4002

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4002 VIRTUAL MACHINE ((&00),(&01)) COULD NOT BE TERMINATED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS4003

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4003 DEVICE '(&00)' IS BUSY. COMMAND REJECTED FOR VIRTUAL MACHINE ((&01),(&02))

### Meaning

A device can only be removed if it has terminated all its
I/O operations.
(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine

### Response

Retry the command after the device concerned has terminated
its I/O operations or remove the device with FORCE=*YES.

## VMS4004

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4004 DEVICE '(&00)' ALREADY ASSIGNED EXCLUSIVELY TO VM ((&01),(&02))

### Meaning

A device may be assigned exclusively to one VM only.
(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS4005

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4005 DEVICE '(&00)' ASSIGNED TO VIRTUAL MACHINE ((&01),(&02)) (&03) (&04)

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine
(&03): "(TYPE=SD)" or "(TYPE=VC)" if explicitly specified by command
(&04): Cause:
- Blank: VM2000 administrator command
- "(BY GUEST)": Implicit assign by guest system
- "(BY SYSADM)": Action of the system administration

## VMS4006

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4006 DEVICE '(&00)' NOT AVAILABLE

### Meaning

The device
- is not generated (correctly) on the local SU (Server Unit),
- is not generated in the guest system having been migrated (SU /390), or
- is generated differently (type, host connector or unit id) in the
guest system having been migrated (SU x86).
(&00): Mnemonic device name

## VMS4007

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : YES

VMS4007 DEVICE '(&00)' NOT ASSIGNED TO VIRTUAL MACHINE ((&01),(&02))

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine.

## VMS4008

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4008 DEVICE '(&00)' SWITCHED FROM VIRTUAL MACHINE ((&01),(&02)) TO VIRTUAL MACHINE ((&03),(&04)) (&05)

### Meaning

(&00): Mnemonic device name
(&01): Index of the source virtual machine (FROM-VM)
(&02): Name of the source virtual machine (FROM-VM)
(&03): Index of the target virtual machine (TO-VM)
(&04): Name of the target virtual machine (TO-VM).
(&05): Cause:
- Blank: VM2000 administrator command
- "(BY GUEST)": Implicit switch by guest system

## VMS4009

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4009 DEVICE '(&00)' REMOVED FROM VIRTUAL MACHINE ((&01),(&02)) (&03)

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine
(&03): Cause:
- Blank: VM2000 administrator command
- "(BY GUEST)": Implicit remove by guest system
- "(BY SYSADM)": Action of the system administration
- "(BY IPL)": Implicit remove by IPL of guest system
- "(BY RECONF)": Reconfiguration by system administrator

## VMS4010

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4010 MAXIMUM NUMBER ((&00)) OF VIRTUAL MACHINES ALLOWED ALREADY REACHED. /(&01) REJECTED

### Response

If necessary, terminate a virtual machine.

## VMS4011

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4011 REQUESTED MEMORY FOR VIRTUAL MACHINE ((&00),(&01)) IS NOT AVAILABLE. /(&02) REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Correct the operands MEMORY-SIZE and/or LOCATION and reenter the command.

## VMS4012

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4012 REQUESTED MEMORY FOR VIRTUAL MACHINE ((&00),(&01)) IS NOT SUFFICIENT. /(&02) REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Please reenter the command with sufficient memory size.

## VMS4013

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4013 VM name '(&00)' not available. Reason: (&01)

### Meaning

VM names have to be unique on a Server Unit and in an HA cluster.
(&00): VM name which is not available
(&01): Reason:
1 - The VM name is already used by a FOREIGN VM on
the local Server Unit.
2 - The VM name is already used by a FOREIGN VM on
a Server Unit which is in an HA cluster together with
the local Server Unit.
3 - The VM name is already used by a BS2000 VM on
the local Server Unit.
4 - The VM name is already used by a BS2000 VM on
a Server Unit which is in an HA cluster together with
the local Server Unit.
5 - The VM name is already used in the definition of a BS2000 VM
on the local Server Unit.
6 - The VM name is already used in the definition of a BS2000 VM
on a Server Unit which is in an HA cluster together with
the local Server Unit.
7 - The total number of BS2000 and FOREIGN VMs running or defined
on the local Server Unit has reached the allowed maximum.

## VMS4014

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4014 Virtual machine ((&00),(&01)) not created due to SVP error

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS4015

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4015 VIRTUAL MACHINE ((&00),(&01)) ALREADY INITIALIZED. /(&02) REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS4016

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : YES

VMS4016 DEVICE '(&00)' CANNOT BE USED AS VIRTUAL CONSOLE. /(&01) REJECTED FOR VIRTUAL MACHINE ((&02),(&03))

### Meaning

The device type code must be '02' or '03'
(&00): Mnemonic device name
(&02): Index of the virtual machine
(&03): Name of the virtual machine.

## VMS4017

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4017 IPL DEVICE TYPE ILLEGAL. /(&00) REJECTED FOR VIRTUAL MACHINE ((&01),(&02))

### Meaning

Only disks or tapes are allowed as IPL devices.
(&01): Index of the virtual machine
(&02): Name of the virtual machine.

## VMS4018

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4018 REQUESTED CPU NOT ASSIGNED TO VIRTUAL MACHINE ((&00),(&01)). /(&02) REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS4019

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4019 SPECIFIED VIRTUAL CPU UNSUITABLE FOR IPL. /(&00) REJECTED FOR VIRTUAL MACHINE ((&01),(&02))

### Meaning

The specified virtual CPU is blocked by VM2000 or
it is a spare CPU.
(&00): Command
(&01): Index of the virtual machine
(&02): Name of the virtual machine.

## VMS4020

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4020 DEVICE '(&00)' NOT ASSIGNED TO VIRTUAL MACHINE ((&01),(&02)). /(&03) REJECTED

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS4021

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4021 DEVICE '(&00)' IS LAST CONSOLE OR MAIN CONSOLE OF MONITOR SYSTEM. RECONFIGURATION NOT POSSIBLE

### Meaning

(&00): Mnemonic device name.

## VMS4022

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4022 DEVICE '(&00)' CURRENTLY IN USE AS PUBLIC DEVICE IN MONITOR VM. RECONFIGURATION NOT POSSIBLE

### Meaning

(&00): Mnemonic device name.

## VMS4023

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4023 THE REQUESTED IPL DEVICE IS NOT AVAILABLE. /(&00) REJECTED

## VMS4024

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4024 VIRTUAL MACHINE ((&00),(&01)) TERMINATED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4026

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4026 VIRTUAL CONSOLE ALREADY DEFINED FOR VIRTUAL MACHINE ((&00),(&01)). /(&02) REJECTED FOR DEVICE '(&03)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&03): Mnemonic device name

## VMS4027

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4027 NO CONSOLE DEFINED FOR VIRTUAL MACHINE ((&00),(&01)). /(&02) REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.

## VMS4030

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4030 A VIRTUAL CONSOLE CANNOT BE ASSIGNED TO THE MONITOR VM. /(&00) REJECTED

### Meaning

(&00): VM2000 command name.

## VMS4031

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4031 DEVICE '(&00)' IS INOP. COMMAND REJECTED FOR VIRTUAL MACHINE ((&01),(&02))

### Meaning

The device is inoperable or there are different LUNs connected via
individual channel paths of the disk device.
(&00): Mnemonic device name
(&01): Index of virtual machine
(&02): Name of virtual machine

### Response

If the affected device is a disk device that is connected via
multiple fibre channels, please check the zoning and LUN masking
of all respective ports.

## VMS4032

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4032 DEVICE '(&00)' CANNOT BE SHARED WITH OTHER VIRTUAL MACHINES

### Meaning

(&00): Mnemonic device name

## VMS4033

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4033 Maximum number of sharers already reached for device '(&00)'. Command rejected for this device

### Meaning

A shared device can only be assigned to at most 16 systems.
(&00): Mnemonic device name

## VMS4034

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4034 DEVICE '(&00)' ALREADY ASSIGNED AS SHARED DEVICE

### Meaning

A device already assigned as shared device cannot be assigned
exclusively to a VM. If the command /START-VM has been entered,
the IPL unit has to be assigned exclusively to the VM.
(&00): Mnemonic device name

## VMS4035

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4035 NO CORRESPONDING DEVICE FOUND

## VMS4036

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4036 IPL IN PROGRESS FOR VIRTUAL MACHINE ((&00),(&01))

### Meaning

An IPL for the virtual machine has just been initiated by the
SE manager, or the previous IPL has not been terminated properly.
(&00): Index of the virtual machine
(&01): Name of the virtual machine.

### Response

Please check the state of the virtual machine.

## VMS4037

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4037 I/O ERROR DURING BOOTREADING FOR VIRTUAL MACHINE ((&00),(&01)). CC=(&02), CSB=(&03), USB=(&04), SENSE=(&05)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Condition code (CC)
(&03): Channel status byte (CSB)
(&04): Unit status byte (USB)
(&05): Sense bytes.

### Response

Check the device status with the help of the information displayed.

## VMS4038

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4038 TIMEOUT ERROR AT MICROKERNEL INITIALIZATION OR AT STARTING OF THE IPL CPU. /(&00) REJECTED FOR VIRTUAL MACHINE ((&01),(&02))

### Meaning

(&00): Command
(&01): Index of the virtual machine
(&02): Name of the virtual machine.

## VMS4039

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4039 DEVICE '(&00)' ASSIGNED TO VIRTUAL MACHINE ((&01),(&02)) (&03)

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine
(&03): Special type of the device, if defined.

## VMS4040

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4040 DEVICE '(&00)' NOT ASSIGNED TO A VIRTUAL MACHINE

### Meaning

(&00): Mnemonic device name.

## VMS4043

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4043 CPU (&00) NOT IN SYSTEM

### Meaning

(&00): Number of the real CPU

### Response

Correct the command.

## VMS4044

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4044 CPU (&00) ATTACHED

### Meaning

(&00): Number of the real CPU

## VMS4045

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4045 CPU (&00) DETACHED

### Meaning

(&00): Number of the real CPU

## VMS4046

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4046 CPU (&00) ALREADY ATTACHED

### Meaning

(&00): Number of the real CPU

## VMS4047

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4047 CPU (&00) ALREADY DETACHED

### Meaning

(&00): Number of the real CPU

## VMS4048

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4048 CPU (&00) IS THE LAST AVAILABLE NORMAL CPU. NO RECONFIGURATION POSSIBLE

### Meaning

(&00): Number of the real CPU

## VMS4049

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4049 Memory Reconfiguration for virtual machine ((&00),(&01)) has been rejected due to a busy device '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine.
(&02): Mnemonic of the first or only busy device.

### Response

If the guest system is in STARTUP, retry the command after SYSTEM READY
of the guest system.
Otherwise, check the I/O-state of the device (DETACH for the device may
be necessary) and try again.

## VMS4050

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4050 X2000 RSC activity for virtual machine ((&00),(&01)) could not be stopped. /(&02) rejected

### Meaning

"Remote System Call" facility of X2000 did not respond within
a time limit.
(&00): Index of the virtual machine
(&01): Name of the virtual machine.
(&02): Command

### Response

Retry the command later.

## VMS4052

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4052 NO TERMINATION INTERRUPT FOR IPL DEVICE '(&00)'

### Meaning

(&00): Mnemonic device name.

## VMS4060

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4060 ONLY ONE DEVICE OF TYPE 'VIRTUAL CONSOLE' CAN BE ASSIGNED TO A VIRTUAL MACHINE

## VMS4064

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4064 NO CHANNEL PATH AVAILABLE FOR DEVICE '(&00)'. ASSIGNMENT REJECTED

### Meaning

(&00): Mnemonic device name.

### Response

The channel path must be made available in the monitor system.

## VMS4065

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4065 Device '(&00)' added to VM2000 configuration

## VMS4066

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4066 Device '(&00)' removed from VM2000 configuration

## VMS4067

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4067 HARDWARE RESOURCES EXHAUSTED. DEVICE '(&00)' COULD NOT BE ASSIGNED TO VM ((&01),(&02))

### Meaning

The storage capacity for the devices in the harware is exhausted.

### Response

Remove possible devices from VMs and retry the command.

## VMS4068

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4068 DEVICE '(&00)' ALREADY ASSIGNED TO THE SPECIFIED VM ((&01),(&02))

## VMS4069

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4069 DEVICE '(&00)' ALREADY ASSIGNED TO THE TARGET VM ((&01),(&02))

### Meaning

The command /SWITCH-VM-DEVICE was not processed for the issued device.

## VMS4071

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4071 Invalid memory size or location specified for virtual machine ((&00), (&01)). /(&02) rejected

### Meaning

Possible reasons:
- If an address is specified for LOCATION, it has to be a multiple
of 1 MB.
- On an SU x86 it is only permitted to specify multiples
of 2 MB for MEMORY-SIZE, MIN-MEMORY-SIZE, MAX-MEMORY-SIZE and
NEW-MEMORY-SIZE, NEW-MIN-MEMORY-SIZE respectively.
(&00): Index of virtual machine
(&01): Name of virtual machine
(&02): Command

## VMS4072

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4072 CPU (&00) is defect. Command rejected

### Meaning

(&00): Number of the real CPU

## VMS4073

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4073 CPU (&00) not attached due to CPU attribute

### Meaning

(&00): Number of the real CPU

## VMS4074

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4074 No additional CPU available

## VMS4075

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4075 EXTRA-CPU (&00) attached

### Meaning

(&00): Number of the real EXTRA-CPU

## VMS4077

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4077 EXTRA-CPU (&00) detached

### Meaning

(&00): Number of the real EXTRA-CPU

## VMS4078

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4078 CPU (&00) NOT DETACHED DUE TO CPU ATTRIBUTE

### Meaning

(&00): Number of the real CPU

## VMS4079

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4079 No CPU with the specified attribute attached

## VMS4080

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4080 DURING IPL THE DEVICE '(&00)' COULD NOT BE RESET

### Meaning

During IPL the Hypervisor could not reset one or several devices.
(&00): Mnemonic device name of the first or only concerned device.

### Response

If the concerned device is a disk device and the virtual machine does
not have the I/O-reset-privilege, the command /MODIFY-VM-ATTRIBUTES
with the operand IO-RESET=*YES should be issued by the VM2000
administrator before you can repeat the command /START-VM.
Otherwise, contact the service technician.

## VMS4081

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4081 /SWITCH-VM-DEVICES FAILED. DEVICE '(&00)' ONLY REMOVED

### Meaning

(&00): Mnemonic device name.

### Response

Assign the device with /ADD-VM-DEVICE to the new VM.

## VMS4082

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4082 WARNING: THE HARD-COPY DEVICE '(&00)' IS NOT ASSIGNED.

### Meaning

VM was started without assignment of the hard-copy device.
(&00): Mnemonic device name of the hard-copy device.

### Response

Assign the concerned hard-copy device to the VM.

## VMS4083

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4083 WARNING: ALL CPUS OF VIRTUAL MACHINE ((&00),(&01)) ARE STOPPED

## VMS4084

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4084 I/O CONFIGURATION UPDATE IN PROGRESS. COMMAND REJECTED

### Meaning

As long as the I/O configuration update is not completed, a guest system
cannot be started.

### Response

Terminate the I/O configuration update and then start the guest system.

## VMS4085

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4085 Device '(&00)' still attached in guest system. Device not removed

### Meaning

(&00): Mnemonic device name

### Response

Retry the command with FORCE=*YES if necessary.

## VMS4086

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4086 State of device '(&00)' in guest system unknown. Device not removed

### Meaning

(&00): Mnemonic device name

### Response

Retry the command with FORCE=*YES if necessary.

## VMS4087

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4087 Device '(&00)' remains assigned to VM ((&01),(&02)) until detach in guest system has been done

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS4088

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4088 Device '(&00)' already assigned 'BY GUEST' to VM ((&01),(&02)). Device assigned now 'BY VM-ADMIN'

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine

## VMS4089

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4089 Device '(&00)' generated as virtual console. Assignment only possible with TYPE=*VC

### Meaning

(&00): Mnemonic device name

## VMS4091

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4091 MEMORY-RECONFIGURATION FOR VIRTUAL MACHINE ((&00),(&01)) HAS BEEN REJECTED BECAUSE NO APPROPRIATE GUEST SYSTEM IS RUNNING

### Meaning

possible causes:
- The guest system is not completely loaded.
- The loaded guest system does not support memory-reconfiguration.
- The requested memory size is not supported by the loaded guest system.
(&00): Index of the virtual machine.
(&01): Name of the virtual machine.

## VMS4092

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4092 A MEMORY-RECONFIGURATION ORDER IS STILL BEING PROCESSED; THE REQUEST FOR VIRTUAL MACHINE ((&00),(&01)) HAS BEEN REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4093

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4093 INCORRECT OPERAND VALUE(S) SPECIFIED CONCERNING THE MEMORY-SIZE FOR THE VIRTUAL MACHINE ((&00),(&01))

### Meaning

possible causes:
- The total memory size of a VM cannot be smaller than its minimal
memory size.
- The total memory size of a VM cannot be larger than its maximal
memory size.
- The minimal memory size of the VM is too small.
- The maximal memory size of the VM is too large.
- The minimal memory size of a VM cannot be reduced.
- The specified memory size is in contradiction with the selected
function (extend or reduce memory size).
(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Reenter the corrected command.

## VMS4094

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4094 MEMORY-RECONFIGURATION FOR VIRTUAL MACHINE ((&00),(&01)) HAS BEEN SUCCESSFULLY PROCESSED. CURRENT MEMORY SIZES: (&02) / (&03)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Minimal memory size of the VM in megabytes
(&03): Total memory size of the VM in megabytes

## VMS4095

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4095 MEMORY-RECONFIGURATION FOR VIRTUAL MACHINE ((&00),(&01)) HAS BEEN PARTIALLY PROCESSED OR ERRONEOUSLY COMPLETED. CURRENT MEMORY SIZES: (&02) / (&03) / (&04)

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Minimal memory size of the VM in megabytes
(&03): Total memory size of the VM in megabytes
(&04): Memory size used by the guest system in megabytes

## VMS4100

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4100 MSCF COORDINATED MOVE NOT SUPPORTED BY GUEST SYSTEM ON VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Where applicable reenter the command without MSCF-COORDINATED=*YES.

## VMS4101

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4101 MSCF COORDINATED MOVE REJECTED BY GUEST SYSTEM ON VIRTUAL MACHINE ((&00), (&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Where applicable reenter the command without MSCF-COORDINATED=*YES.

## VMS4102

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4102 MSCF COORDINATION NOT CONFIRMED IN TIME BY GUEST SYSTEM ON VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

Where applicable reenter the command without MSCF-COORDINATED=*YES.

## VMS4103

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4103 RELEASE OF CLUSTER RECOVERY LOCK NOT CONFIRMED IN TIME BY GUEST SYSTEM ON VIRTUAL MACHINE ((&00),(&01))

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4143

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4143 Guest system in STARTUP processing. Command rejected

### Meaning

During STARTUP processing of the guest system it is not possible
to remove the devices assigned.

### Response

Retry command after SYSTEM READY of the guest system
or remove the devices with FORCE=*YES.

## VMS4144

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4144 VM ((&00),(&01)) in WAIT STATE. Command rejected

### Meaning

For a VM in WAIT STATE, it is not possible to remove the
devices assigned.
(&00): Index of the virtual machine
(&01): Name of the virtual machine

### Response

If necessary, resume the VM and retry the command or remove the
devices with FORCE=*YES.

## VMS4150

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4150 CPU (&00) could not be attached due to its state

### Meaning

(&00): Number of the real CPU.

### Response

Contact the service technician.

## VMS4151

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4151 CPU (&00) could not be detached due to its state

### Meaning

(&00): Number of the real CPU.

### Response

Contact the service technician.

## VMS4159

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4159 Device pair specified for the main console is not checked

### Meaning

It has not been checked whether the pair of mnemonic device names
specified for the main console corresponds to the combination
output path/input path of a KVP console.

## VMS4160

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4160 Device pair specified for the main console does not correspond to a KVP console

### Meaning

The pair of mnemonic device names specified for the main console
does not correspond to the combination output path/input path
of a KVP console.

### Response

Correct the specification and reenter the command.

## VMS4161

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4161 The first device specified for the KVP console does not correspond to an output path

### Meaning

The pair of mnemonic device names corresponds to a KVP console
but the output path is not specified first.

### Response

Specify a KVP console as a pair of device mnemonic names
in the sequence: (KVP output path,KVP input path).

## VMS4170

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4170 Switch to indirect I/O failed. Assignment of device '(&00)' rejected

### Meaning

Because of intensive I/O with this device, switching to indirect I/O
is currently not possible.
(&00): Mnemonic device name

### Response

Retry command later if necessary.

## VMS4171

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4171 ASSIGN-BY-GUEST not allowed for virtual consoles. Attribute of device '(&00)' not changed

### Meaning

(&00): Mnemonic device name

## VMS4172

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4172 Device '(&00)' currently assigned to several sharers. Exclusive usage not possible

### Meaning

(&00): Mnemonic device name

## VMS4180

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4180 The set of devices specified by the UNITS operand is empty

## VMS4190

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4190 Command '/(&01)' not processed for PAV alias device '(&00)'

### Meaning

(&00): Mnemonic device name
(&01): VM2000 command name

## VMS4191

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4191 PAV base device '(&00)' not assigned to VM ((&01),(&02)). Alias device '(&03)' will be removed

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine
(&03): Mnemonic device name

## VMS4192

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4192 Assignment by VM-ADMIN not allowed for PAV alias devices. Alias device '(&00)' will be removed

### Meaning

(&00): Mnemonic device name

## VMS4195

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4195 Command '/(&01)' not processed for CRD '(&00)'

### Meaning

(&00): Mnemonic device name
(&01): VM2000 command name

## VMS4200

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4200 ASSIGNMENT SET '(&00)' NOT INITIALIZED. /(&01) REJECTED

### Meaning

(&00): Name of the assignment set
(&01): Command

## VMS4201

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4201 ASSIGNMENT SET '(&00)' CREATED

### Meaning

(&00): Name of the assignment set

## VMS4202

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4202 ASSIGNMENT SET '(&00)' EXISTS ALREADY. COMMAND REJECTED

### Meaning

(&00): Name of the assignment set

## VMS4203

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4203 NO DEVICE ASSIGNED TO ASSIGNMENT SET '(&00)'

### Meaning

(&00): Name of the assignment set

## VMS4204

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4204 ASSIGNMENT SET '(&00)' NOT EMPTY. COMMAND REJECTED

### Meaning

(&00): Name of the assignment set

### Response

All devices assigned to the specified assignment set have to
be reassigned to another or no assignment set by the command
/MODIFY-VM-DEVICE-ATTRIBUTES and the name of the specified
assignment set has to be removed from all VM-related lists of
the privileg ASSIGN-BY-GUEST by the command /MODIFY-VM-ATTRIBUTES.
Afterwards the command can be repeated.

## VMS4205

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4205 ASSIGNMENT SET '(&00)' DELETED

### Meaning

(&00): Name of the assignment set

## VMS4210

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4210 MAXIMUM NUMBER ((&00)) OF ASSIGNMENT SETS ALREADY REACHED. COMMAND REJECTED

### Meaning

(&00): Maximum number of assignment sets allowed

## VMS4211

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4211 NUMBER OF ASSIGNMENT SETS SPECIFIED EXPLICITLY FOR VM ((&00),(&01)) EXCEEDS ALLOWED MAXIMUM ((&02)).COMMAND REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Maximum number of explicitly specified assignment
sets per virtual machine

## VMS4220

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4220 PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' ASSIGNED TO VM ((&02),(&03))

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the virtual machine
(&03): Name of the virtual machine

## VMS4221

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4221 PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' ASSIGNED TO VM ((&02),(&03)) WITH ERRORS

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the virtual machine
(&03): Name of the virtual machine

### Response

Check the hardware state of the pubset devices that could not
be assigned to the VM and try to assign them individually. Besides,
the assignment of the whole pubset will be retried during the pubset
attachment in BS2000.

## VMS4222

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4222 ONLY PUBRES DEVICE '(&00)' ASSIGNED PRELIMINARY TO VM ((&01),(&02))

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): Index of the virtual machine
(&02): Name of the virtual machine

### Response

Only the PUBRES device was assigned to the VM. The remaining
devices of the pubset could not be determined yet. Their assignment
will be retried during the pubset attachment in BS2000.

## VMS4223

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4223 VM2000 COMMAND '/(&01)' FOR PUBSET SPECIFIED BY PUBRES DEVICE OR CATID '(&00)' REJECTED

### Meaning

(&00): Specified mnemonic device name of PUBRES or specified CATID
(&01): Command

## VMS4224

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4224 ASSIGNMENT OF PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' TO VM ((&02),(&03)) WILL BE UPDATED BY SYSTEM

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the virtual machine
(&03): Name of the virtual machine

### Response

The assignment of all pubset devices will be updated as a result
of a pubset reconfiguration (/MODIFY-PUBSET-PROCESSING) or a VM
assignment discrepancy detected during the pubset attachment in
BS2000.

## VMS4225

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4225 PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' REMOVED FROM VM ((&02),(&03))

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the virtual machine
(&03): Name of the virtual machine

## VMS4226

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4226 PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' REMOVED FROM VM ((&02),(&03)) WITH ERRORS

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the virtual machine
(&03): Name of the virtual machine

### Response

Check the hardware state of the pubset devices that could not
be removed from the VM and try to remove them individually
(possibly with FORCE=*YES).

## VMS4227

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4227 ASSIGNMENT OF PUBSET DEVICE '(&00)' TO VM ((&01),(&02)) WILL BE CHANGED BY SYSTEM

### Meaning

(&00): Mnemonic device name of a volume having been removed from
a pubset
(&01): Index of the virtual machine
(&02): Name of the virtual machine

### Response

The explicit assignment of the specified pubset device will be
changed to the implicit one as a result of a pubset reconfiguration
(/MODIFY-PUBSET-PROCESSING).

## VMS4228

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4228 PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' SWITCHED FROM VM ((&02),(&03)) TO VM ((&04),(&05))

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the source virtual machine (FROM-VM)
(&03): Name of the source virtual machine (FROM-VM)
(&04): Index of the target virtual machine (TO-VM)
(&05): Name of the target virtual machine (TO-VM)

## VMS4229

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4229 PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' SWITCHED FROM VM ((&02),(&03)) TO VM ((&04),(&05)) WITH ERRORS

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the source virtual machine (FROM-VM)
(&03): Name of the source virtual machine (FROM-VM)
(&04): Index of the target virtual machine (TO-VM)
(&05): Name of the target virtual machine (TO-VM)

### Response

Check the hardware state of the pubset devices that could not be
switched to the VM and try to reassign or remove them individually
(possibly with FORCE=*YES). Besides, the assignment of the whole
pubset will be retried during the pubset attachment in BS2000.

## VMS4230

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4230 DEVICE USAGE OF PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' MODIFIED

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES

## VMS4231

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4231 DEVICE USAGE OF PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' MODIFIED WITH ERRORS

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES

### Response

If necessary, remove the reason of the failure and modify the
device usage of the respective pubset devices individually.

## VMS4234

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4234 DEVICE '(&00)' ALREADY ASSIGNED TO VM ((&01),(&02)). DEVICE USAGE MODIFIED BY SYSTEM

### Meaning

(&00): Mnemonic device name
(&01): Index of the virtual machine
(&02): Name of the virtual machine

### Response

The specified pubset device was already assigned to the target VM
but its device usage had to be modified to meet the usage required
to the whole pubset (operand TYPE of command /ADD-VM-DEVICES).

## VMS4235

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4235 SOME DEVICES OF PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' REMAIN ASSIGNED TO VM ((&02),(&03)) UNTIL DETACH IN GUEST SYSTEM HAS BEEN DONE

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the virtual machine
(&03): Name of the virtual machine

## VMS4236

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4236 PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' NOT ASSIGNED TO VM ((&02),(&03))

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES
(&02): Index of the virtual machine
(&03): Name of the virtual machine

## VMS4237

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4237 ONLY PUBRES DEVICE '(&00)' REMOVED FROM VM ((&01),(&02))

### Meaning

Only the PUBRES device was removed from the VM. The remaining
devices of the pubset could not be determined yet.
(&00): Mnemonic device name of PUBRES
(&01): Index of the virtual machine
(&02): Name of the virtual machine

### Response

Retry the command later on if necessary.

## VMS4238

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4238 ONLY INFORMATION ABOUT PUBRES DEVICE '(&00)' AVAILABLE

### Meaning

Only the information about the PUBRES device was displayed. The
remaining devices of the pubset could not be determined yet.
(&00): Mnemonic device name of PUBRES

### Response

Retry the command later on if necessary.

## VMS4240

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4240 DEVICE ATTRIBUTES OF PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' MODIFIED

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES

## VMS4241

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4241 DEVICE ATTRIBUTES OF PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' MODIFIED WITH ERRORS

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES

## VMS4242

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4242 ONLY DEVICE ATTRIBUTES OF PUBRES DEVICE '(&00)' MODIFIED

### Meaning

(&00): Mnemonic device name of PUBRES

### Response

Only the device attributes of the PUBRES device were modified. The
remaining devices of the pubset could not be determined yet. Their
modification will be retried during the pubset attachment in BS2000.

## VMS4244

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4244 DEVICE ATTRIBUTES OF PUBSET '(&01)' WITH PUBRES DEVICE '(&00)' WILL BE UPDATED BY SYSTEM

### Meaning

(&00): Mnemonic device name of PUBRES
(&01): CATID found on PUBRES

### Response

The device attributes of all pubset devices will be updated as a
result of a pubset reconfiguration (/MODIFY-PUBSET-PROCESSING) or
a device attribute discrepancy (between a pubset device and the
corresponding PUBRES device) detected during the pubset attachment
in BS2000.

## VMS4245

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4245 DEVICE ATTRIBUTES OF PUBSET DEVICE '(&00)' SET TO DEFAULT VALUES BY SYSTEM

### Meaning

(&00): Mnemonic device name

### Response

The device attributes of the specified pubset device were set to
the default values as a result of device attribute discrepancy
(between non-default values of the specified pubset device and
default values of the corresponding PUBRES device) detected during
a pubset reconfiguration (/MODIFY-PUBSET-PROCESSING) or during the
the pubset attachment in BS2000.

## VMS4250

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4250 DEVICE '(&00)' IS NOT PUBRES DEVICE

### Meaning

(&00): Mnemonic device name

## VMS4251

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4251 DEVICE LIST OF PUBSET SPECIFIED BY PUBRES DEVICE OR CATID '(&00)' IS INCONSISTENT

### Meaning

(&00): Specified mnemonic device name of PUBRES or specified CATID

## VMS4252

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4252 DEVICE LIST OF PUBSET SPECIFIED BY PUBRES DEVICE OR CATID '(&00)' CANNOT BE DETERMINED. REASON: (&01)

### Meaning

(&00): Specified mnemonic device name of PUBRES or specified CATID
(&01): Reason for failure: IO-ERROR or TIMEOUT or INTERNAL

## VMS4253

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4253 PUBRES DEVICE OF PUBSET SPECIFIED BY CATID '(&00)' CANNOT BE DETERMINED. REASON: (&01)

### Meaning

(&00): Specified CATID
(&01): Error code reported by $STAM in the monitor system:
NFND MRSCAT entry cannot be found
CINV CATID invalid
NINI MRSCAT not initialized
INTE Internal error
NPUB Name of PUBRES device not in MRSCAT
CINC CATID inconsistent (specified CATID different from the
CATID obtained from the PUBRES device determined by
MRSCAT)

### Response

Check and update MRSCAT entry in the monitor system (!) or
specify the pubset by its PUBRES mn.

## VMS4270

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4270 No EXTRA-CPU in the configuration

## VMS4340

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4340 Opening of MONJV rejected by subsystem JV (JVS(&00)). /(&01) rejected

### Meaning

(&00): JV return code
(&01): Command

### Response

The cause of the JV error message can be detected with
/HELP-MSG-INFORMATION JVS(&00).

## VMS4342

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4342 MONJV '(&01)' could not be updated. Reason: JVS(&00)

### Meaning

(&00): JV return code
(&01): Name of the MONJV

### Response

The cause of the JV error message can be detected with
/HELP-MSG-INFORMATION JVS(&00).

## VMS4343

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4343 Catalog '(&00)' not accessible. MONJV could not be updated

### Meaning

(&00): Catalog identifier

### Response

The corresponding pubset should be imported.

## VMS4344

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4344 Monitoring by MONJV '(&00)' is stopped

### Meaning

The correctness of the JV content is no longer guaranteed
because the MONJV protection has been lifted previously.
(&00): Name of the MONJV

## VMS4400

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4400 VM GROUP '(&00)' NOT INITIALIZED. /(&01) REJECTED

### Meaning

(&00): Name of the VM group
(&01): Command

## VMS4401

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4401 VM GROUP '(&00)' CREATED

### Meaning

(&00): Name of the VM group

## VMS4402

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4402 VM GROUP '(&00)' EXISTS ALREADY. COMMAND REJECTED

### Meaning

(&00): Name of the VM group

## VMS4403

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4403 VM GROUP '(&00)' IS EMPTY

### Meaning

(&00): Name of the VM group

## VMS4404

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4404 VM GROUP '(&00)' NOT EMPTY. COMMAND REJECTED

### Meaning

(&00): Name of the VM group

### Response

The members of the VM group have to be removed from the group
with the command /REMOVE-VM-FROM-VM-GROUP. After this the command
could be repeated.

## VMS4405

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4405 VM GROUP '(&00)' DELETED

### Meaning

(&00): Name of the VM group

## VMS4410

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4410 MAXIMUM NUMBER ((&00)) OF VM GROUPS ALREADY REACHED. /(&01) REJECTED

### Meaning

(&00): Allowed maximum number of VM groups
(&01): Command

### Response

Where appropriate remove all virtual machines from a VM group and
then delete this VM group.

## VMS4411

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4411 NO VM GROUP INITIALIZED

## VMS4422

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4422 VM GROUP '(&00)' NOT ASSIGNED TO CPU POOL '(&01)'. /(&02) REJECTED

### Meaning

The virtual machine has to be assigned to the same
CPU pool as the VM group.
(&00): Name of the VM group
(&01): Name of the CPU pool
(&02): Command

## VMS4424

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4424 VIRTUAL MACHINE ((&00),(&01)) ALREADY ASSIGNED TO A VM GROUP

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4425

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4425 VIRTUAL MACHINE ((&00),(&01)) ASSIGNED TO VM GROUP '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the VM group

## VMS4427

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4427 VIRTUAL MACHINE ((&00),(&01)) NOT ASSIGNED TO VM GROUP '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the VM group

## VMS4428

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4428 VIRTUAL MACHINE ((&00),(&01)) NOT ASSIGNED TO ANY VM GROUP

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4429

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4429 VIRTUAL MACHINE ((&00),(&01)) REMOVED FROM VM GROUP '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the VM group

## VMS4450

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4450 CPU-QUOTA OF VIRTUAL MACHINE ((&00),(&01)) HAS TO BE SPECIFIED VIA MEMBER-CPU-QUOTA. /(&02) REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Command

### Response

If a virtual machine is a member of a VM group CPU-QUOTA has to
be specified via the sub-operand MEMBER-CPU-QUOTA to determine the
virtual machine's portion of the CPU-QUOTA of the VM group.

## VMS4503

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4503 Resources for command processing not yet totally initialized. Command rejected

### Meaning

VM2000 commands cannot be entered before VM2000 READY has been displayed.

### Response

Reenter the command after VM2000 READY has been displayed.

## VMS4504

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4504 MONITOR MEMORY SHORTAGE. VM2000 COMMAND REJECTED

### Meaning

Due to a shortage of memory, the VM2000 command cannot be processed.

### Response

Check the system state and retry later, if necessary.

## VMS4505

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4505 Command '/(&00)' temporarily not executable

### Response

Retry after a short time of waiting!

## VMS4506

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4506 Asynchronous processing step at /(&00) not acknowledged in time

### Meaning

The VM2000 agent (SU x86) or the VM2000 hypervisor (SU /390)
did not acknowledge the execution of an asynchronous request
before expiry of a time limit.
Possibly, the request has been executed in the meantime or
will be executed later on.
On SU x86, a running live migration with the local SU as
target SU could cause a delay of the execution.
(&00): Command

### Response

Please check with the help of VM2000 information services
if the purpose of the command has been achieved in the meantime.
Possibly, the command processing will be terminated successfully
somewhat later, or you have to repeat the command.
If repeating the command does not help, please contact the service.

## VMS4507

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4507 Internal error in VM2000 agent or administration component of VM system. /(&00) failed

### Meaning

(&00): Command

### Response

Diagnosis data of the VM2000 agent and the administration
component of the VM system must be created and stored.
Please contact the service.

## VMS4508

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4508 INTERNAL ERROR '(&00)' DURING COMMAND PROCESSING

### Meaning

(&00): Error code

### Response

Contact the system administrator

## VMS4509

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4509 MEMORY SHORTAGE. THE RUNTIME-TRACE-BUFFER COULD NOT BE ALLOCATED

## VMS4510

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4510 AUTOMATIC VM2000-DUMP INITIATED BY VIRTUAL MACHINE ((&00),(&01))

### Meaning

A virtual machine has initiated an automatic VM2000-DUMP because
of a system crash or need of diagnosis information.
Send the file containing the VM2000-DUMP together with other diagnosis
data to the support center.
(&00): Index of the virtual machine; 0 means the hypervisor
(&01): Name of the virtual machine or *HYPERVISOR

## VMS4511

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4511 AUTOMATIC VM2000-DUMP CANNOT BE CREATED. VMDUMP NOT INSTALLED

### Meaning

A VM tried to create an automatic VM2000-DUMP. This failed because
of incorrect installation of the release unit VM2000-UTIL.

### Response

Check installation of the release unit VM2000-UTIL.

## VMS4512

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4512 AUTOMATIC VM2000-DUMP FOR VM ((&00),(&01)) COULD NOT BE TAKEN. REPLY (EOT); BEFORE, TAKE A MANUAL VM2000-DUMP IF NEEDED

### Meaning

(&00): Index of the virtual machine; 0 means the hypervisor
(&01): Name of the virtual machine or *HYPERVISOR

## VMS4513

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4513 HYPERVISOR MEMORY EXHAUSTED. COMMAND REJECTED

### Response

Please check the specification of the hypervisor main memory size
in the startup parameter file of BS2000.
If there is specified HYPERVISOR-SIZE=*BY-SYSTEM (default value),
please take a VMDUMP and contact the service.
If there is specified an explicit value for the hypervisor main
memory size, this value may be too small. Possibly you can free
some space for the hypervisor by deleting a VM (of less importance).

## VMS4514

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4514 WARNING: HYPERVISOR MEMORY EXHAUSTED

### Meaning

The hypervisor cannot process its internal orders because its memory
is exhausted. For this reason, the smooth operating of the guest system
can be hindered.

### Response

Please check the specification of the hypervisor main memory size
in the startup parameter file of BS2000.
If there is specified HYPERVISOR-SIZE=*BY-SYSTEM (default value),
please take a VMDUMP and contact the service.
If there is specified an explicit value for the hypervisor main
memory size, this value may be too small. Possibly you can free
some space for the hypervisor by deleting a VM (of less importance).

## VMS4600

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4600 CPU POOL '(&00)' NOT INITIALIZED. /(&01) REJECTED

### Meaning

(&00): Name of the CPU pool
(&01): Command

## VMS4601

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4601 CPU POOL '(&00)' CREATED

### Meaning

(&00): Name of the CPU pool

## VMS4602

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4602 CPU POOL '(&00)' EXISTS ALREADY. COMMAND REJECTED

### Meaning

(&00): Name of the CPU pool

## VMS4603

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4603 NO CPU ASSIGNED TO CPU POOL '(&00)'

### Meaning

(&00): Name of the CPU pool

## VMS4604

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4604 CPU ASSIGNED TO CPU POOL '(&00)'. COMMAND REJECTED

### Meaning

(&00): Name of the CPU pool

### Response

All CPUs assigned to the specified CPU pool have to be assigned
to other CPU pools by the command /SWITCH-VM-CPU.
Afterwards the command can be repeated.

## VMS4605

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4605 CPU POOL '(&00)' DELETED

### Meaning

(&00): Name of the CPU pool

## VMS4606

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4606 SWITCH OF CPU '(&00)' FROM CPU POOL '(&01)' TO CPU POOL '(&02)' REJECTED. COMMAND ABORTED

### Meaning

A grave error (e.g. CPU failure) has occured in the source CPU pool
during the switching of CPUs.
(&00): CPU identification
(&01): Identification of the source CPU pool
(&02): Identification of the target CPU pool

## VMS4607

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4607 CPU '(&00)' NOT ASSIGNED TO CPU POOL '(&01)'

### Meaning

(&00): CPU identification
(&01): Identification of the CPU pool

## VMS4608

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4608 CPU '(&00)' SWITCHED FROM CPU POOL '(&01)' TO CPU POOL '(&02)'

### Meaning

(&00): CPU identification
(&01): Identification of the source CPU pool
(&02): Identification of the target CPU pool

## VMS4609

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4609 MULTIPLE CPU POOLS EXIST. /(&00) REJECTED

### Meaning

Besides the standard CPU pool there exists another CPU pool.
The VM2000 administrator has to specify the CPU pool by name
(or *STDPOOL).
(&00): Command

## VMS4610

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4610 MAXIMUM NUMBER ((&00)) OF CPU POOLS ALLOWED ALREADY REACHED. COMMAND REJECTED

### Meaning

(&00): Maximum number of CPU pools allowed

## VMS4611

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4611 SELECTED CPUS NOT AVAILABLE IN CPU POOL '(&00)'. /(&01) REJECTED

### Meaning

(&00): Identification of the CPU pool
(&01): Command

## VMS4612

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4612 INSUFFICIENT NUMBER OF ATTACHED CPUS IN CPU POOL '(&00)'. /(&01) REJECTED

### Meaning

- The number of attached virtual CPUs of a virtual machine,
which is in state RUNNING or IN-HOLD and which is or should be
assigned to the CPU pool, is too great compared to the number of
attached real CPUs of the CPU pool.
- On an SU x86 there has to be at least one attached real
CPU in a CPU pool to which a virtual machine is assigned.
- There is no attached real CPU in the CPU pool. A virtual machine
assigned to this CPU pool cannot be started.
(&00): Identification of the CPU pool
(&01): Command

## VMS4613

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4613 NO VIRTUAL MACHINE ASSIGNED TO CPU POOL '(&00)'

### Meaning

(&00): Identification of the CPU pool

## VMS4614

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4614 VIRTUAL MACHINE ASSIGNED TO CPU POOL '(&00)'. COMMAND REJECTED

### Meaning

(&00): Name of the CPU pool

### Response

All virtual machines assigned to the specified CPU pool have to be
assigned to other CPU pools by the command /ASSIGN-VM-TO-CPU-POOL.
Afterwards the command can be repeated.

## VMS4615

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4615 VIRTUAL MACHINE ((&00),(&01)) ASSIGNED TO CPU POOL '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Identification of the CPU pool

## VMS4616

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4616 VIRTUAL MACHINE ((&00),(&01)) ALREADY ASSIGNED TO CPU POOL '(&02)'. COMMAND REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Identification of the CPU pool

### Response

If the virtual machine should get another value for CPU-QUOTA
the command /MODIFY-VM-ATTRIBUTES has to be used.

## VMS4617

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4617 CPU '(&00)' IS LAST ATTACHED CPU OF ACTIVE CPU POOL '(&01)'. COMMAND REJECTED

### Meaning

A CPU pool to which a started VM is assigned to has to contain
at least one attached CPU.
(&00): CPU identification
(&01): Identification of the CPU pool

## VMS4618

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4618 CPU POOL ASSIGNMENT OF VIRTUAL MACHINE ((&00),(&01)) CHANGED FROM CPU POOL '(&02)' TO CPU POOL '(&03)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Identification of the source CPU pool
(&03): Identification of the target CPU pool

## VMS4619

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4619 VIRTUAL MACHINE ((&00),(&01)) REMOVED FROM CPU POOL '(&02)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Identification of the CPU pool

## VMS4620

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4620 IMPLICIT ATTACH-DEVICE FOR VIRTUAL CPUS ON VIRTUAL MACHINE ((&00),(&01)) STARTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4621

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4621 IMPLICIT DETACH-DEVICE FOR VIRTUAL CPUS ON VIRTUAL MACHINE ((&00),(&01)) STARTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4622

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4622 VIRTUAL MACHINE ((&00),(&01)) ASSIGNED TO VM GROUP '(&02)'. COMMAND REJECTED

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Name of the VM group

### Response

A virtual machine which is member of a VM group can only be assigned
to another CPU pool by assigning the whole VM group to this CPU pool.

## VMS4623

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4623 NO VM GROUP ASSIGNED TO CPU POOL '(&00)'

### Meaning

(&00): Name of the CPU pool

## VMS4624

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4624 VM GROUP ASSIGNED TO CPU POOL '(&00)'. COMMAND REJECTED

### Meaning

(&00): Name of the CPU pool

### Response

All VM groups assigned to the specified CPU pool have to
be assigned to other CPU pools by the command
/ASSIGN-VM-GROUP-TO-CPU-POOL. Afterwards the command can be
repeated.

## VMS4625

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : YES

VMS4625 VM GROUP '(&00)' ASSIGNED TO CPU POOL '(&01)'

### Meaning

(&00): Name of the VM group
(&01): Name of the CPU pool

## VMS4626

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4626 VM GROUP '(&00)' ALREADY ASSIGNED TO CPU POOL '(&01)'. COMMAND REJECTED

### Meaning

(&00): Name of the VM group
(&01): Name of the CPU pool

### Response

If the VM group should get another value for CPU-QUOTA
the command /MODIFY-VM-GROUP-ATTRIBUTES has to be used.

## VMS4627

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4627 CPU POOL ASSIGNMENT OF VM GROUP '(&00)' CHANGED FROM CPU POOL '(&01)' TO CPU POOL '(&02)'

### Meaning

(&00): Name of VM group
(&01): Identification of the source CPU pool
(&02): Identification of the target CPU pool

## VMS4628

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4628 CPU-ID '(&00)' BELONGS TO SPARE CPU. /(&01) REJECTED

### Meaning

Spare CPUs are not assigned to any CPU pool.
(&00): CPU identification
(&01): Command

## VMS4629

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : YES

VMS4629 VM GROUP '(&00)' REMOVED FROM CPU POOL '(&01)'

### Meaning

(&00): Name of the VM group
(&01): Name of the CPU pool

## VMS4701

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4701 INTERNAL ERROR IN THE VIRTUAL MACHINE SYSTEM. DIAGNOSTIC INFORMATION (SYSTEMDUMP OR SOFTWARE LOGGING ENTRY) HAS BEEN GENERATED

### Response

Contact the system administrator.

## VMS4800

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4800 Current VM2000 configuration saved in file '(&00)'

### Meaning

(&00): Name of the generated configuration file

## VMS4801

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4801 VM2000 configuration restored from file '(&00)'

### Meaning

(&00): Name of the configuration file

## VMS4802

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4802 Restore of VM2000 configuration from file '(&00)' only partially processed

### Meaning

For each configuration component, which could not be restored,
a message VMS4803 was issued.
(&00): Name of the configuration file

## VMS4803

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4803 Reconfiguration of (&00) '(&01)' has been partially processed or erroneously completed. Processing of /RESTORE-VM-CONFIGURATION continues

### Meaning

(&00): Type of configuration component:
CPU-POOL, REAL-CPU, VM-GROUP, ASSIGNMENT-SET, VM or DEVICE
(&01): Specification of the component of which reconfiguration has been
partially processed or erroneously completed.

## VMS4810

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4810 VM2000 version (&00) too old

### Meaning

(&00): Version of running VM2000 subsystem

## VMS4811

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4811 Main memory size (&00) too small. Processing of /RESTORE-VM-CONFIGURATION continues

### Meaning

(&00): Current main memory size

## VMS4812

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4812 Current number of the real, operational (&00)-CPUs too small

### Meaning

(&00): CPU attribute: NORMAL or EXTRA

## VMS4813

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4813 Current number of the real, operational (&00)-CPUs too small. Processing of /RESTORE-VM-CONFIGURATION continues

### Meaning

(&00): CPU attribute: NORMAL or EXTRA

## VMS4814

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4814 At the restore of the VM2000 configuration from file '(&00)' an Extra-CPU will be attached

### Meaning

(&00): Name of the configuration file

## VMS4816

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4816 Unfit configuration of Monitor VM ((&00),(&01)). Processing of /RESTORE-VM-CONFIGURATION continues

### Meaning

Possible reasons:
- In the saved configuration, the VM index belongs to a Guest VM
but not to the Monitor VM.
- In the saved configuration, the VM name is used for a Guest VM.
- The location of the Monitor VM prevents the creation of a Guest VM.
- The main memory size is greater than the saved main memory size of
the Monitor VM.
- On an SU x86, the maximum main memory size is greater than the
corresponding saved size of the Monitor VM.
(&00): Index of the Monitor VM
(&01): Name of the Monitor VM

## VMS4817

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4817 Configuration of persistent VM ((&00),(&01)) is not saved. Processing of /SAVE-VM-CONFIGURATION continues

### Meaning

The configuration data of a persistent VM is permanently available
(i.e. also after the restart of the Server Unit) and does not need
to be included in the backup of the VM2000 configuration.
(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4818

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4818 Warnings occured at the saving of the VM2000 configuration

### Response

Please consider preceding VM2000 messages VMS4814 and VMS4817.

## VMS4830

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4830 Virtual machine ((&00),(&01)) has not yet reached SYSTEM READY

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4831

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4831 Memory reconfiguration of virtual machine ((&00),(&01)) in process

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS4832

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4832 Device reconfiguration during the processing of /(&00)

### Meaning

(&00): VM2000 command name

### Response

Please retry the command.

## VMS4840

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4840 Creation of configuration file '(&00)' rejected. Reason: DMS(&01)

### Meaning

(&00): Name of the configuration file
(&01): DMS return code

### Response

The cause of the DMS error message can be detected with
/HELP-MSG-INFORMATION DMS(&01).

## VMS4841

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4841 Configuration file '(&00)' could not be written. Reason: DMS(&01)

### Meaning

(&00): Name of the configuration file
(&01): DMS return code

### Response

The cause of the DMS error message can be detected with
/HELP-MSG-INFORMATION DMS(&01).

## VMS4842

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4842 Configuration file '(&00)' could not be read. Reason: DMS(&01)

### Meaning

(&00): Name of the configuration file
(&01): DMS return code

### Response

The cause of the DMS error message can be detected with
/HELP-MSG-INFORMATION DMS(&01).

## VMS4843

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4843 Incomplete configuration file '(&00)' could not be deleted. Reason: DMS(&01)

### Meaning

(&00): Name of the configuration file
(&01): DMS return code

### Response

The cause of the DMS error message can be detected with
/HELP-MSG-INFORMATION DMS(&01).

## VMS4844

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4844 Missing record '(&01)' in configuration file '(&00)'

### Meaning

The record is mandatory. It is missing or not at the expected location.
(&00): Name of the configuration file
(&01): Specification of the mandatory record

## VMS4845

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4845 Missing record with tag '(&01)' for (&02) '(&03)' in configuration file '(&00)'

### Meaning

The record with the tag is mandatory for the component.
It is missing or not at the expected location.
(&00): Name of the configuration file
(&01): Tag of mandatory record for the specified component
(&02): Type of configuration component:
VM2000, REAL-CPU, VM-GROUP, VM or DEVICE
(&03): Specification of configuration component

## VMS4846

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4846 (&01) '(&02)' is missing in configuration file '(&00)'

### Meaning

The component is referenced in the configuration file,
although it is not defined there.
(&00): Name of the configuration file
(&01): Type of configuration component:
CPU-POOL, VM-GROUP, ASSIGNMENT-SET or VM WITH (MONITOR-)VM-INDEX
(&02): Specification of configuration component

## VMS4847

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4847 Erroneous data record '(&01)' in configuration file '(&00)'

### Meaning

Possible reasons:
- Erroneous start or end tag
- Start or end tag in higher level is missing
- The value between the start and the end tag breaches its
required range.
(&00): Name of the configuration file
(&01): Erroneous data record

## VMS4848

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4848 (&01) '(&02)' in configuration file '(&00)' erroneous

### Meaning

The records of the specified configuration component do not fit
together.
(&00): Name of the configuration file
(&01): Type of configuration component:
VM2000, REAL-CPU, VM-GROUP, VM or DEVICE
(&02): Specification of configuration component

## VMS4900

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4900 Performance quota of VM2000 deceleration feature changed to (&00)

### Meaning

(&00): New value of performance quota in percent

## VMS4901

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS4901 VM2000 deceleration feature not activated. Command rejected

### Meaning

The VM2000 deceleration feature must be activated by the
startup parameter service.

## VMS4910

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4910 Check of disk configuration started

## VMS4911

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 70

Warranty : NO

VMS4911 Check of disk configuration already started

## VMS4912

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS4912 Check of disk configuration completed

## VMS5000

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5000 VM2000-SPECIFIC HARDWARE/FIRMWARE COMPONENTS NOT AVAILABLE. ((&00))

### Meaning

(&00): Firmware components not available.

## VMS5002

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5002 DIAGNOSE INSTRUCTION FAILED. VM2000 STARTUP ABORTED

## VMS5003

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5003 PHYSICAL MEMORY SIZE TOO SMALL FOR VM2000. MINIMUM SIZE: (&00) MEGABYTES. STARTUP ABORTED. GENERATE A NEW SYSTEM

### Meaning

(&00): Minimum value of megabytes for the physical memory space.

## VMS5004

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5004 EVM-FIRMWARE NOT AVAILABLE. VM2000 STARTUP ABORTED

## VMS5005

Destination: CONSOLE Routing code: 9 Weight: 98

Warranty : NO

VMS5005 ENTER VM2000 HYPERVISOR FILE NAME. REPLY (<FILE NAME>; EOT(USE STANDARD FILE))

### Meaning

In conjunction with a dialog startup this message is displayed to ask for
the file name of the VM2000 hypervisor.

## VMS5006

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5006 WRONG VERSION OF LOADED HYPERVISOR; VM2000 STARTUP ABORTED

### Meaning

The Version of the loaded Hypervisor is different from the version
specified in the Startup parameter service or is different from the
default version.

## VMS5007

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5007 STARTUP ABORTED DUE TO INTERNAL INCONSISTENCY. TAKE SLED

## VMS5008

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5008 THE VM2000 HYPERVISOR AND MONITOR VM VERSIONS ARE INCOMPATIBLE. STARTUP ABORTED

### Response

Link either a new hypervisor or a new monitor system.

## VMS5010

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5010 DMS ERROR CODE '(&00)'. VM2000 CONFIGURATION FILE NOT ACCESSIBLE

### Meaning

The cause of the DMS error code can be detected with /HELP-MSG DMS(&00).

## VMS5011

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5011 THE ATTRIBUTES OF THE VM2000 CONFIGURATION FILE DO NOT CORRESPOND TO THE REQUIRED FILE ATTRIBUTES. INPUT IGNORED

### Meaning

The configuration file
- is not a SAM-file,
- does not have BLOCKSIZE (STD,1), or
- is an empty file.

## VMS5012

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5012 INCONSISTENCY WITHIN THE VM2000 CONFIGURATION FILE. COMMAND PROCESSING ABORTED

### Meaning

The file could not be read.

### Response

Issue the commands which have not been processed at the console and/or
create a new VM2000 configuration file.

## VMS5013

Destination: CONSOLE Routing code: 9 Weight: 98

Warranty : NO

VMS5013 ILLEGAL REPLY

### Meaning

None of the possible answers to VMS5005 or VMS5027 has been given.

## VMS5014

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5014 FILE '(&00)' IS USED AS VM2000 CONFIGURATION FILE

### Meaning

(&00): File name.

## VMS5015

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5015 VM2000 HYPERVISOR LOADED FROM FILE '(&00)'

### Meaning

(&00): File name.

## VMS5016

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5016 TOTAL MAIN MEMORY FOR VM2000: (&00) MB; MONITOR VM SIZE: (&01) MB; HYPERVISOR SIZE: (&02) MB

## VMS5017

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5017 THE HYPERVISOR LOAD MODULE HAS AN INVALID FORMAT OR A WRONG FILE NAME

### Response

Contact the system administrator.

## VMS5018

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5018 HYPERVISOR FILE NAME NOT CATALOGED

### Response

Correct the input or create a hypervisor file.

## VMS5020

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5020 STARTUP OF THE MONITOR SYSTEM IN (&00) MODE

### Meaning

(&00): Multiprocessor mode of the monitor system

## VMS5021

Destination: CONSOLE Routing code: 9 Weight: 98

Warranty : NO

VMS5021 ISSUE VM2000 COMMAND (MAX. 70 CHARACTERS) OR 'END'. REPLY (DESIRED INPUT; EOT=END)

## VMS5022

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5022 INVALID VALUE OF OPERAND (&00) IN COMMAND /CREATE-VM FOR MONITOR VM; DEFAULT VALUE (&01) TAKEN

### Meaning

The command was either issued at the console or was read
from the configuration file.
(&00): Operand name.
(&01): Operand default value.

## VMS5023

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5023 DEFAULT VALUES USED FOR THE MONITOR VM

### Meaning

Because no valid /CREATE-VM has been specified for the Monitor VM
default values have been used.
Possible default values being used:
- VM-NAME = VM0001
- MEMORY-SIZE = 512
- CPU-QUOTA = 14
- MAX-CPU-UTILIZATION = 100
- PROCESSOR = *MAXIMUM

## VMS5024

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5024 OPERAND NOT PERMITTED FOR THE MONITOR VM. 'ADMIN-PRIVILEGES=STD' IS SET

### Meaning

The operand ADMIN-PRIVILEGES=MAX is not permitted in the command
/CREATE-VM.

## VMS5026

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5026 I/O ERROR WHILE LOADING THE HYPERVISOR LINK MODULE

### Response

Correct the input or take SLED.

## VMS5027

Destination: CONSOLE Routing code: 9 Weight: 98

Warranty : NO

VMS5027 SPECIFY VM2000 CONFIGURATION FILE NAME. REPLY (EOT(USE STANDARD FILE); FN=<FILE NAME>(,VOL=<VSN>); CONS(CONSOLE CMD INPUT); END(END OF INPUT))

### Meaning

Possible replies are:
- P.FN=<filename>(,VOL=<vsn>): The file <filename> on a public volume
set or on a private disk with the volume
serial number <vsn> is read
- P.CONS : VM2000 commands are to be issued from
console
- P.END : End of input
- P.EOT : Standard file name

## VMS5028

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5028 VIRTUAL CONSOLES ARE NOT PERMITTED FOR THE MONITOR VM. /ADD-VM-DEVICES REJECTED

### Meaning

Command /ADD-VM-DEVICES specified during startup or in the
configuration file has not been processed due to the TYPE=VC operand.

### Response

Allocate the appropriate device after SYSTEM READY.

## VMS5029

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5029 INVALID DEVICE '(&00)'. DEVICE IGNORED

### Meaning

(&00): Mnemonic device name.

## VMS5030

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5030 COMMAND NOT PERMITTED DURING VM2000 STARTUP. /(&00) IGNORED

### Meaning

Only the commands /CREATE-VM and /ADD-VM-DEVICES are
allowed. The next command will be read.

## VMS5031

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5031 VM2000 COMMAND '/(&00)' REJECTED BECAUSE OF ERRONEOUS OR MISSING OPERAND

## VMS5032

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5032 REPLY TOO LONG

### Meaning

The reply is limited to 70 characters.

## VMS5033

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5033 CPU QUOTA OF THE MONITOR SYSTEM HAS BEEN CORRECTED TO (&00)

### Meaning

The value of the operand CPU-QUOTA in the command /CREATE-VM is invalid.
Instead, the value (&00) displayed in the message has been used.

## VMS5034

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5034 Device '(&00)' cannot be assigned. Error cause: condition code: (&01)

### Meaning

Error during assignment of device (&00).
(&00) : Mnemonic device name
(&01) : Condition code

## VMS5036

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5036 MAX-CPU-UTILIZATION OF THE MONITOR SYSTEM HAS BEEN CORRECTED TO (&00)

### Meaning

The value of the operand MAX-CPU-UTILIZATION in the command /CREATE-VM
is invalid. Instead, the value (&00) displayed in the message has been
used.
(&00): New, corrected value

## VMS5037

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5037 REQUESTED MEMORY SIZE FOR THE MONITOR VM IS INCORRECT. VALUE CORRECTED TO: (&00) MB

### Meaning

Possible reasons:
1.) The requested memory size (together with the Hypervisor
size) exceeds real memory size. The default value is used
instead of the specified value.
2.) The requested minimum memory size for the Monitor VM
exceeds its memory size. The default value of minimum
memory size is used instead of the specified value.

## VMS5038

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5038 REQUESTED MEMORY SIZE FOR MONITOR VM IS TOO SMALL. DEFAULT VALUE USED: (&00) MB

### Meaning

The requested (minimum) memory size for the Monitor VM is
less than the permitted minimum value.
(&00): Number of megabytes.

## VMS5039

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5039 INVALID VM-INDEX USED IN THE COMMAND '/CREATE-VM'. DEFAULT VALUE '1' TAKEN

## VMS5041

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5041 HOME-PUBSET DEVICE '(&00)' CANNOT BE USED IN SHARED-MODE

### Meaning

The device has been exclusively assigned.
(&00): Mnemonic device name

## VMS5043

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5043 UNRECOVERABLE ERROR OCCURED DURING REP-PROCESSING IN HYPERVISOR. STARTUP ABORTED

## VMS5044

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5044 SPECIFIED HYPERVISOR SIZE IS INCORRECT. DEFAULT VALUE TAKEN: (&00) MB

### Meaning

Possible reasons:
- The specified Hypervisor size is not within valid range.
- Together with the minimum size of the Monitor VM the Hypervisor size
exceeds real memory size.

## VMS5045

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5045 INVALID VALUE GIVEN TO THE PARAMETER SERVICE: (&00)

### Meaning

(&00): Name of the faulty operand

## VMS5047

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5047 CPU (&00) COULD NOT BE STARTED BECAUSE OF HW-MALFUNCTION

### Meaning

(&00): Number of the real CPU

## VMS5048

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5048 CPU (&00) IS OFFLINE AND HAS NOT BEEN STARTED

### Meaning

(&00): Number of the real CPU

## VMS5049

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5049 NUMBER OF REAL CPU(s) RUNNING: (&00)

## VMS5050

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5050 Number of available Spare-CPU(s): (&00)

## VMS5053

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5053 Number of available Extra-CPU(s): (&00)

## VMS5054

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5054 Performance quota of VM2000 deceleration feature set to (&00)

### Meaning

(&00): Initial value of the performance quota in percent

## VMS5055

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5055 VM2000 parameter (&00) specified by BS2000 parameter service ignored

### Meaning

(&00): Name of the VM2000 parameter ignored

### Response

Move the parameter from the BS2000 parameter file to the parameter
file of subsystem VM2-MON.

## VMS5110

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5110 DMS ERROR CODE '(&00)'. VM2000 PARAMETER FILE NOT ACCESSIBLE. SUBSYSTEM START ABORTED

### Meaning

The cause of the DMS error code can be detected with /HELP-MSG DMS(&00).

## VMS5111

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5111 THE ATTRIBUTES OF THE VM2000 PARAMETER FILE DO NOT CORRESPOND TO THE REQUIRED FILE ATTRIBUTES. SUBSYSTEM START ABORTED

### Meaning

The parameter file
- is not a SAM-file,
- does not have BLOCKSIZE (STD,1), or
- is an empty file.

## VMS5112

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5112 INCONSISTENCY WITHIN THE VM2000 PARAMETER FILE. SUBSYSTEM START ABORTED

### Meaning

The file could not be read.

## VMS5145

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5145 INVALID VALUE OF OPERAND (&00) IN PARAMETER FILE. DEFAULT VALUE TAKEN

### Meaning

(&00): Name of the faulty operand

## VMS5224

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5224 DEVICE '(&00)' CANNOT BE USED IN SHARED-MODE. ASSIGNMENT REJECTED

### Meaning

(&00): Mnemonic device name

### Response

Assign the device exclusively after System Ready.

## VMS5225

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5225 DEVICE OR CHANNEL TYPE MISMATCH. DEVICE '(&00)' INCORRECTLY GENERATED IN THE MONITOR SYSTEM

### Meaning

(&00): Mnemonic device name

## VMS5226

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5226 DEVICE '(&00)' NOT GENERATED IN THE MONITOR SYSTEM

### Meaning

(&00): Mnemonic device name

## VMS5227

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5227 DEVICE '(&00)' IMPLICITLY REMOVED BY VM2000

### Meaning

(&00): Mnemonic device name

## VMS5541

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5541 *** VIRTUAL MACHINE SYSTEM VM2000 (&00) READY ***

## VMS5550

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5550 RECONFIGURATION ERROR FOR DEVICE '(&00)'. STARTUP CONTINUES

### Meaning

(&00): Mnemonic device name.

### Response

The specified device could not be logically detached in the monitor
system. This has no consequences for the VM2000 startup.

## VMS5551

Destination: CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS5551 INTERNAL ERROR DURING VM2000 STARTUP. STARTUP ABORTED. TAKE DUMP

## VMS6000

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS6000 VM2000 AGENT NOT AVAILABLE

### Meaning

The VM2000 mode continues. But most of the VM2000 commands can not
be processed until the VM2000 agent becomes available again and
the message VMS6004 is issued.

### Response

Please call the service.

## VMS6001

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS6001 ADMINISTRATION COMPONENT OF VM SYSTEM NOT AVAILABLE

### Meaning

The VM2000 mode continues. But most of the VM2000 commands can not
be processed until the failed administration component becomes
available again and the message VMS6005 is issued.

### Response

Please call the service.

## VMS6002

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS6002 VM2000 AGENT STARTED

## VMS6003

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS6003 VM2000 AGENT STOPPED

## VMS6004

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS6004 VM2000 AGENT AVAILABLE AGAIN

## VMS6005

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS6005 ADMINISTRATION COMPONENT OF VM SYSTEM AVAILABLE AGAIN

## VMS6018

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS6018 CPU POOL ASSIGNMENT OF VIRTUAL MACHINE ((&00),(&01)) CHANGED BY SYSTEM ADMINISTRATION FROM CPU POOL '(&02)' TO CPU POOL '(&03)'

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Identification of the source CPU pool
(&03): Identification of the target CPU pool

## VMS6020

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS6020 VIRTUAL MACHINE ((&00),(&01)) CREATED BY SYSTEM ADMINISTRATION

### Meaning

Possible reasons:
- system administrator command
- automatic take over (failover) of the high available VM from another
Server Unit of the HA cluster
- take over of the VM from another Server Unit within a migration
(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS6021

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : YES

VMS6021 VIRTUAL MACHINE ((&00),(&01)) TERMINATED BY SYSTEM ADMINISTRATION

### Meaning

Possible reasons:
- system administrator command
- transfer of the VM to another Server Unit within a migration
(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS6023

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS6023 GUEST SYSTEM ON VM ((&00),(&01)) STARTED BY SYSTEM ADMINISTRATION

### Meaning

(&00): Index of the virtual machine
(&01): Name of the virtual machine

## VMS6094

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS6094 MEMORY OF VIRTUAL MACHINE ((&00),(&01)) HAS BEEN RECONFIGURED. CURRENT MEMORY SIZES: (&02) / (&03)

### Meaning

The memory reconfiguration has not been initiated via the VM2000 CLI
in the Monitor VM.
(&00): Index of the virtual machine
(&01): Name of the virtual machine
(&02): Minimal memory size of the VM in megabytes
(&03): Total memory size of the VM in megabytes

## VMS9001

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS9001 FUNCTION NOT AVAILABLE FOR THE CURRENT INPUT MEDIUM OR THE CURRENT GUEST SYSTEM

## VMS9002

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS9002 SPECIFIED ADDRESS/AREA NOT DEFINED/NOT ACCESSIBLE

## VMS9004

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS9004 FUNCTIONALITY NOT SUPPORTED ON THE CURRENT HSI OR WITH THE CURRENT PARAMETER ASSIGNMENT

## VMS9005

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS9005 COMMAND COULD NOT BE OR ONLY PARTIALLY BE PROCESSED SUCCESSFULLY

## VMS9006

Destination: USER-TASK, CONSOLE Routing code: 9 Weight: 99

Warranty : NO

VMS9006 SPECIFIED HW-RESOURCES NOT USEFUL OR NOT AVAILABLE FOR /START-VM

©2025 Fujitsu | BS2000 System Messages