## CAN0DMP

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0DMP DUMP PROCESSING PROHIBITS TERMINATION OF TASK. RETRY COMMAND LATER

### Meaning

A DUMP is currently generated for the task specified in /CANCEL-JOB
or /FORCE-JOB-CANCEL command.
Task termination is temporarily prohibited.

## CAN0HOL

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0HOL TASK IN 'HOLD' STATE: COMMAND REJECTED

### Meaning

The specified task has been put into a wait state by the system
administrator or the operator via the /HOLD-TASK command. It must be
released from that state via the /RESUME-TASK command, otherwise it
cannot be cancelled.

### Response

Enter the /RESUME-TASK command or ask the system administrator or
operator to do so, then repeat the command to cancel the task.

## CAN0INT

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0INT INTERNAL SYSTEM ERROR: COMMAND PROCESSING ABORTED

### Meaning

An internal system subroutine indicated an error situation.
For more detailed information see the SERSLOG entry.

### Response

Note the command operands, circumstances (time, TSN of your own task) and
characteristics of the task that should have been cancelled and contact
the system administrator.

## CAN0KIL

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0KIL ABNORMAL TASK TERMINATION ENFORCED BY COMMAND

### Meaning

Abnormal task termination has been enforced by the system administrator
or the operator via the /FORCE-JOB-CANCEL command or an equivalent older
command.
This emergency measure is taken when normal termination via the
/CANCEL-JOB
command is unsuccessful.
During this procedure, it is not usual to wait until the terminated task
has left all the system tables in a consistent state.
A system dump of the task is created by default to analyze why
it was not possible to end the task normally, and to record
inconsistencies
in system tables caused by subsequent errors.

## CAN0KI1

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0KI1 /FORCE-JOB-CANCEL ALREADY ISSUED: COMMAND REJECTED

### Meaning

The /FORCE-JOB-CANCEL command or an equivalent older command cannot be
issued more than once for a particular task.

## CAN0LOG

Destination: CONSOLE Routing code: J Weight: 99

Warranty : NO

CAN0LOG TASK WITH USER ID '(&00)', JOB NAME '(&01)', TERMINAL '(&02)' CANCELLED TSN '(&03)' VIA COMMAND

### Meaning

A task cancellation via the /CANCEL-JOB or /FORCE-JOB-CANCEL command is
logged at the console using this message.
This message is suppressed if the command was issued by a local task with
the OPERATING privilege.
If the command was issued in a local interactive task, (&02) will
designate
the terminal in the form 'procname/statname'. If this is not the case,
BATCH is stated. If the cancellation was requested on an MSCF partner
system, *sendname will be output.
procname: BCAM name of the terminal processor
statname: terminal name
sendname: BCAM name of the MSCF partner system which sent the command.

## CAN0NAU

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0NAU CALLER WITHOUT AUTHORIZATION: COMMAND NOT PROCESSED

### Meaning

Possible reasons:
- the user is not authorized to cancel jobs with a foreign
user identification.
- the operator cannot enter /FORCE-JOB-CANCEL unless the system
parameter NRTKILL permits this.

## CAN0NCA

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0NCA TERMINATION OF TASK TEMPORARILY NOT POSSIBLE. RETRY COMMAND LATER

### Meaning

A system process temporarily prevented termination of the task
via /CANCEL-JOB or /FORCE-JOB-CANCEL command.

### Response

Contact the system administrator if task termination proves unsuccessful
after repeated attempts.

## CAN0NKI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0NKI /CANCEL-JOB NECESSARY FIRST: COMMAND REJECTED

### Meaning

An attempt must first be made to cancel using the /CANCEL-JOB command as
this is the safe way to cancel. Only then is it permissible to input the
/FORCE-JOB-CANCEL command or an equivalent older command.

## CAN0NOP

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0NOP CANCEL PROCESSING FOR SPECIFIED TASK IS ALREADY STARTED: COMMAND IGNORED

### Meaning

CANCEL-JOB commands have already been issued on the specified job.
A further CANCEL-JOB is only effective, if the operand STEPS gets
a stronger value in the following sense:
*CURRRENT-STEP < *ALL-STEPS < *ALL-CALENDAR-REPETITIONS
DUMP processing is informed if the value of the operand DUMP is
*CANCEL-RUNNING-DUMP.

## CAN0OPD

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0OPD OPERAND INVALID: COMMAND REJECTED

### Meaning

A syntax error occurred in one operand of the /CANCEL-JOB command.

## CAN0OPR

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0OPR OPERATOR RESPONSE FOR TASK WITH TSN '(&00)' NOT YET ARRIVED. TASK TERMINATION DEFERRED

### Meaning

The operator still has to answer a question from the task to be cancelled.
The task will start terminating as soon as it receives the reply.

## CAN0OWN

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0OWN USER CANNOT ABORT OWN TASK VIA /CANCEL-JOB: COMMAND REJECTED

### Response

Use the /EXIT-JOB command to terminate your own task or specify correct
TSN if the TSN of own task was specified by mistake.

## CAN0PND

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0PND TASK PERMANENTLY PENDED DUE TO SYSTEM ERROR: COMMAND REJECTED

### Meaning

The /CANCEL-JOB command is not permitted for a permanently pending task.

### Response

Later repetition of the command may be successful in some cases.
Otherwise, contact the system administrator to have the whole system
memory dumped (SLED) at system shutdown for diagnostic purposes.

## CAN0PRO

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0PRO DO YOU INSIST ON CANCELLING PROTECTED JOB? REPLY (Y=YES; N=NO)

### Meaning

The job cannot be cancelled inadvertently as it is protected by the
PROTECT
operand in the /ENTER-JOB or /SET-LOGON-PARAMETERS command.

### Response

Check the /SHOW-JOB-STATUS output displayed on the screen for this job,
then answer the question.
Y: job is cancelled.
N: job continues.

## CAN0TRM

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0TRM JOB WITH TSN '(&00)' IS ALREADY TERMINATING: COMMAND IGNORED

## CAN0TSN

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0TSN SPECIFIED TSN NOT FOUND IN SYSTEM: COMMAND REJECTED

### Meaning

Possible reasons:
- the system does not recognize the TSN operand specified in the
/CANCEL-JOB command.
- the corresponding job may already be terminated.

### Response

Check the TSN and retry the command with the correct TSN.

## CAN0TXT

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0TXT TEXT: '(&00)'

### Meaning

(&00): additional text, specified in the TEXT operand of the /CANCEL-JOB
command or an equivalent older command.

## CAN0WIT

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN0WIT CANCEL REQUEST WITHDRAWN BY USER: COMMAND NOT EXECUTED

## CAN00BY

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN00BY CANCELLED BY '(&00)'

### Meaning

(&00): Attributes of the task that caused the cancellation.
The first four characters classify the cancel caller type.
- OPR <ci> tsn
termination via real (physical) operator console
- ATOP a-id procname statname
termination via automated operating ($CONSOLE application,
logical console)
- DIAL tsn userid jobname procname statname
termination via dialog task
- BTCH tsn userid jobname
termination via batch task
- SUBT tsn userid jobname subtorig
termination via subtask, created to execute some job issued by
a user, e.g. ARCHIVE action
- USER*tsn sendname userid
termination via user task in an unknown MSCF partner system that
sent no further data
- SYST tsn hextid <userid> <jobname>
termination via system task.
An * instead of a blank after the caller type indicates that the
cancel order came from a different system. In this case, sendname will be
inserted after the *. The other attributes will be moved 9 characters
further on.
sendname: BCAM name of MSCF partner system that requested the
cancellation
ci: console identification
a-id: application identification, a 4 character string under which
the corresponding $CONSOLE application is registered
tsn: TSN (task sequence number)
procname: BCAM name of the terminal processor
statname: station name or abbreviated program name
userid: user identification
jobname: job name
subtorig: subtask origin, an 8 character identification of the system
component which created the subtask (e.g. $ARCHIVE, $HSMS)
hextid: task identification in hexadecimal notation.

## CAN00OK

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CAN00OK CANCEL PROCESSING STARTED FOR TSN '(&00)' WITH USER ID '(&01)'

### Meaning

The task with the specified TSN has been given the signal to terminate.

©2025 Fujitsu | BS2000 System Messages