## FEI0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0001 FDEXIM READY. VER (&00), CR-DATE (&01)

### Meaning

FDEXIM is ready:
(&00): Version no., (&01): Creation date.

### Response

None.

## FEI0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0002 FDEXIM CMD PROCESSING

### Meaning

This message indicates that an action (EXPORT, IMPORT
or LIST) processing starts.

### Response

None.

## FEI0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0003 FDEXIM CMD PROCESSING COMPLETED

### Meaning

The command has been executed without error.

### Response

None.

## FEI0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0004 FDEXIM INVALID CMD. CMD REJECTED

### Meaning

The command entered is not a valid command for FDEXIM.

### Response

Reissue the corrected command.

## FEI0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0005 INCONSISTENCY BETWEEN PARAM. CMD REJECTED

### Meaning

The values of the parameters NAMES, RENAMES,
EXCEPT of the command F<ILES>, are inconsistent.

### Response

Submit a new FILES command with correct parameters.

## FEI0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0006 FDEXIM CMD PROCESSING TERM WITH ERROR(S)

### Meaning

One or several errors occurred during CMD processing.
Refer to the message displayed during the run.

### Response

None.

## FEI0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0007 FDEXIM PARAMETER SYNTAX ERROR. CMD REJECTED

### Meaning

A parameter syntax error has been detected while
scanning the parameter(s) of the command.

### Response

Submit a new command with corrected parameter(s).

## FEI0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0008 CMD SEQUENCE ERROR. CMD REJECTED

### Meaning

An EXPORT or IMPORT has been requested without a
FILES command or more than one FILES command has
been given for one action command.

### Response

Submit a FILES command followed by an EXPORT
or an IMPORT command.

## FEI0009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0009 FILE (&00) DOES NOT EXIST. CMD REJECTED

### Meaning

File (&00) does not exist. As a consequence, the EXPORT
command is rejected.

### Response

Check the catalog. Correct the wrong value and reenter
a new FILES command and a new EXPORT command.

## FEI0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0010 DMS ERROR (&00) ON FILE (&01). FILE NOT PROCESSED

### Meaning

A DMS error, with error code (&00), is detected while
processing file (&01). Processing continues with the
next file.

### Response

Remove the DMS error (see manual System Messages) and
restart the processing for file (&01).

## FEI0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0011 DMS ERROR (&00). FILE (&01) CANNOT BE ERASED

### Meaning

In an EXPORT run, the file (&01) cannot be erased due to
a DMS error; error code=(&00). The EXPORT run continues.

### Response

None.

## FEI0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0012 DMS ERROR (&00) ON FILE (&01). PROCESSING CONTINUES

### Meaning

An error (&00), other than open, occurred while
processing file (&01). The processing continues for this file
according to the user's request to accept errors
(ERROR=ACCEPT).

### Response

Check file (&01) for wrong records. Nonreadable PAM-
records have been processed like 'binary 0'.

## FEI0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0013 DMS ERROR (&00) ON FILE (&01). FILE IS SKIPPED

### Meaning

An error (&00), other than open, occurred while
processing the file (&01). The file (&01) is skipped.

### Response

Remove error (see manual System messages) and restart
the operation for file (&01).

## FEI0014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0014 DMS ERROR (&00) ON FILE (&01). CMD PROCESSING TERMINATED

### Meaning

An error (&00), other than open, occurred while
processing file (&01). The processing of the IMPORT or
EXPORT command is terminated.

### Response

Remove the error and restart the processing for file (&01).

## FEI0015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0015 PASSWORD GIVEN DOES NOT MATCH WITH VOLUME'S PASSWORD. CMD TERMINATED

### Meaning

The password, given with parameter SVPASS, doesn't match
with the volume's password. The access is forbidden
and the IMPORT or LIST command processing is terminated.

### Response

Submit correct password and restart the IMPORT or LIST
operation.

## FEI0016

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0016 FILE (&00) TO BE IMPORTED ALREADY EXISTS. FILE NOT REPLACED

### Meaning

The parameter REPLACE=NO has been specified and a
file to be imported already exists. The file is not
imported from the floppy disk.

### Response

1) Submit IMPORT command with REPLACE=YES.
2) Rename or erase file (&00).

## FEI0017

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0017 DMS ERROR (&00) ON FILE (&01). FILE CANNOT BE REPLACED

### Meaning

A DMS error, code=(&00), is detected while attempting
specified and the erase is unsuccessful.

### Response

Change access to file (&01) by CAT command and reissue
the IMPORT command.

## FEI0018

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0018 INTERNAL ERROR. RUN OF FDEXIM IS STOPPED

### Meaning

An internal error of FDEXIM, such as unsuccessful REQM
or RELM, has been detected. The processing cannot be
continued.

### Response

Try another run of FDEXIM and inform the
system support staff.

## FEI0019

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0019 THE FLOPPY DISK HAS NOT BEEN CREATED WITH FDEXIM OR HAS BEEN ALTERED. CMD TERMINATED

### Meaning

The contents of the floppy disk was not created by
FDEXIM or has been altered. The processing of the
IMPORT or LIST command is terminated.

### Response

Check the contents of FD. Use correct FD and restart
IMPORT or LIST.

## FEI0020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0020 RDATA ERROR WHEN READING CMD. FDEXIM ABNORMAL TERM

### Meaning

An error has been detected while reading a command
submitted by the user. The run of FDEXIM cannot
continue.

### Response

Restart the FDEXIM run.

## FEI0021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0021 SYSDTA MAY ONLY BE ASSIGNED TO (SYSCMD) OR (PRIMARY)

### Meaning

The user has assigned SYSDTA to something else than
(SYSCMD) or (PRIMARY).
The run of FDEXIM cannot continue.

### Response

Assign correctly SYSDTA before executing FDEXIM.

## FEI0022

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0022 FILE (&00) NOT IMPORTED

### Meaning

The filename specified (&00) has not been imported
either because of an error which has been specified
in a previous message or because the specified file
has not been found on the floppy disc.

### Response

The user can give a LIST CMD to list the contents of
the floppy disk if he isn't sure of the filenames or, if
possible, take the action to suppress any eventual
error on the files given by previous messages.

## FEI0023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0023 DMS ERROR (&00) ON FILE (&01). CMD REJECTED

### Meaning

A DMS error, with error code = (&00), is detected
for the file (&01). The EXPORT command is rejected.

### Response

Remove error (see manual System Messages).
Reissue the FILES and EXPORT command.

## FEI0024

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0024 TOO MANY FILE NAMES GENERATED FOR THE PARTIALLY QUALIFIED FILENAME (&00). CMD REJECTED

### Meaning

The buffer for the list of filenames is not large
enough; more than about 700 filenames are generated from
the partially qualified filename (&00) given.
The command is rejected.

### Response

Try again with, for example, several partially qualified
filenames in the FILES command, to process these files.

## FEI0025

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0025 RENAME TOO LONG FOR FILE (&00)

### Meaning

The filename built from user's FILES command with
RENAME option is too long.
The command is rejected for an EXPORT command.
For an IMPORT command processing the filename is
truncated to maximal length.

### Response

None.

## FEI0026

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0026 ERROR WHEN SWITCHING FLOPPY DISKS. FLOPPY DISK FILE '(&00)' CLOSED

### Meaning

IMPORT or LIST processing of FDEXIM has been aborted because of
an error when switching file (&00) to a continuation floppy disk.

### Response

Check the order of the floppy disks in the IMPORT or LIST statements;
correct any error that is detected and re-enter the statement.
If necessary, check for operator errors.

## FEI0027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FEI0027 READ ERROR ON FLOPPY DISK FILE (&00)

### Meaning

An error occurred while reading the floppy disk with
RDATA macro. (&00) is the current data set filename.
The IMPORT or LIST processing is terminated.

### Response

Verify the actions of the operator.
Retry a new run of FDEXIM.

©2024 Fujitsu | BS2000 System Messages