## PVRCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVRCOPY Copyright (C) (&00) (&01). All rights reserved

## PVRLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVRLOAD Program (&00), Version (&01) of (&02) loaded from file (&03)

## PVR0000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0000 ***** P V S R E N VERSION '(&00)' *****

## PVR0100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0100 PVSREN NOT EXECUTABLE IN PRESENT BS2000 VERSION. PVSREN NOT LOADED

### Response

Use a PVSREN version which supports the BS2000 version.

## PVR0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0101 PVSREN ONLY EXECUTABLE UNDER $TSOS. PVSREN NOT LOADED

### Response

Call PVSREN under the system administrator ID.

## PVR0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0102 SDF NOT AVAILABLE. PVSREN NOT LOADED

### Meaning

SDF has not been loaded.

### Response

Load SDF and then call PVSREN again.

## PVR0103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0103 PVSREN NOT DEFINED IN ACTIVE SYNTAX FILE

### Response

Activate a syntax file in which PVSREN has been defined.

## PVR0107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0107 SPECIFY OPERAND 'NEW-CATID' HAS SMALLER OR SAME LENGTH THAN OPERAND 'CATID'. CMD 'CHECK-FILENAME-LENGTH' REJECTED

### Meaning

The CHECK-FILENAME-LENGTH statement cannot be executed unless the
NEW-CATID operand is longer than the CATID operand.

### Response

Ensure that the specification fulfils this condition.

## PVR0108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0108 OPERAND 'CATID' MUST CONSIST OF ONE CHARACTER IN PRESENT BS2000 VERSION

### Meaning

Only single-character catalog IDs are permitted in BS2000 versions earlier
than V10.0.

### Response

Specify a single-character catalog ID.

## PVR0109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0109 INVALID CHARACTER IN OPERAND OR OPERAND LENGTH INVALID

### Meaning

Either the operand contains an invalid character (#, @, $) or the
operand length is invalid.

## PVR0110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0110 PREFIX 'PUB' NOT PERMITTED FOR VSN IN POINT REPRESENTATION. STATEMENT REJECTED

### Meaning

The VSN of the pub representation is identified by the prefix 'PUB'.
For this reason this prefix is not permitted for the VSN of the
point representation.

### Response

Specify a catalog ID that differs from the prefix 'PUB'.

## PVR0111

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0111 VALUE FROM 65 THROUGH 192 MUST BE SPECIFIED FOR SYSID FOR THIS CONVERSION TYPE. STATEMENT REJECTED

### Meaning

SYSID=*SAME must not be specified when converting the pubset from
pubset representation to point representation. SYSID has different
value ranges in the two forms of representation.

### Response

Specify a valid value for SYSID and start conversion again.

## PVR0112

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0112 SYSID NOT YET INITIALIZED. SPECIFICATION 'SYSID=*SAME' IGNORED. PROCESSING CONTINUES

### Meaning

The SYSID was not initialized when generating the pubset.

### Response

If desired, dynamically initialize the SYSID using the
/SET-PUBSET-ATTRIBUTES command.

## PVR0113

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0113 'DUAL-RECORDING-BY-VOLUME' BIT SET FOR DISK WITH VSN '(&00)'. PROCESSING ABORTED

### Meaning

The NKDINF macro reports that the DUAL-RECORDING-BY-VOLUME bit is set
in the system volume label of the disk.

### Response

Cancel the bit setting for the disk.

## PVR0114

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0114 'INCONSISTENCY' BIT SET FOR DISK WITH VSN '(&00)'. PROCESSING ABORTED

### Meaning

The NKDINF macro reports that the INCONSISTENCY bit is set in the
system volume label of the disk.

### Response

Cancel the bit setting for the disk.

## PVR0115

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0115 PUBSET OR VOLUME-SET WITH CATALOG ID '(&00)' AVAILABLE. PROCESSING ABORTED

### Meaning

The pubset or volume-set must not be available when this statement is
executed, otherwise other users could make unwanted changes to the
file catalog during program execution.

### Response

Export the pubset from the catalog using the /EXPORT-PUBSET command and
repeat the statement.

## PVR0116

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0116 VOLUME '(&00)' OF PUBSET OR VOLUME-SET NOT ONLINE. PROCESSING ABORTED

### Meaning

The terminal of the specified volume has not been attached to
the installation.

### Response

Attach the volume terminal by means of the command /ATTACH <mn>
and initiate conversion again.

## PVR0117

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0117 PUBSET WITH CATALOG ID '(&00)' NOT AVAILABLE. 'MODIFY-JOINFILE' STATEMENT NOT PROCESSED

### Meaning

The MODIFY-JOINFILE statement cannot be executed unless the pubset
is available.

### Response

Ready the pubset in the current BS2000 system using the command
/IMPORT-PUBSET.

## PVR0118

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0118 NO ENTRY WITH DEFAULT CATALOG ID '(&00)' FOUND

### Meaning

There is no default catalog ID (&00) in the user catalog of the
specified pubset.

## PVR0119

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0119 PUBSET METADATA CANNOT BE MODIFIED. PUBSET NOT AVAILABLE

### Meaning

If the pubset was to be renamed/created then this was accomplished
and the pubset now is in a consistent state. For the purpose of
adapting the user catalog, IMON-SCI data or volumesetlist entries
it was necessary to import the pubset. This was impossible.

### Response

Analyze the messages on the console and dynamically update the
user catalog of the pubset with the aid of the PVSREN statement
MODIFY-JOINFILE if necessary. It is not possible to modify the
user catalog entries acting on a slave host.

## PVR0120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0120 ERROR IN MACRO '(&00)'. RETURN CODE: '(&01)'. PROCESSING ABORTED

### Meaning

System interface '(&00)' returned error '(&01)'.

### Response

Check with your system administrator whether there are global
problems, e.g. memory shortage or loss of communication between
SHC-OSD and StorMan.
If not, please contact your service provider.

## PVR0121

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0121 ERROR IN MACRO '(&00)'. RETURN CODE: '(&01)'. PROCESSING CONTINUED

### Meaning

An error occurred during processing of the (&00) macro. However, it
was not serious enough to affect processing.

### Response

Take appropriate action in accordance with the return code.

## PVR0122

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0122 ERROR WHEN PROCESSING '(&00)' COMMAND.

### Meaning

- The userid has not the privilege "USER-ADMINISTRATION". The
default-catid could not be updated by using the command
'MODIFY-USER'.
- Some other error occured.

### Response

Check the message on the terminal and on the console.
Grant the privilege "USER-ADMINISTRATION" for the userid and convert
the user catalog using the PVSREN statement MODIFY-JOINFILE.

## PVR0123

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0123 ERROR IN SDF MACRO '(&00)'. RETURN CODE: '(&01)'. STATEMENT PROCESSING ABORTED

### Response

Take appropriate action in accordance with the return code.

## PVR0124

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0124 ERROR WHEN OPENING VOLUME '(&00)'. RETURN CODE: '(&01)'. PROCESSING ABORTED

### Response

Take appropriate action in accordance with the return code.

## PVR0125

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0125 ERROR WHEN READING BLOCK. RETURN CODE: '(&00)'. PROCESSING ABORTED

### Response

Take appropriate action in accordance with the return code.

## PVR0126

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0126 ERROR WHEN WRITING BLOCK. RETURN CODE: '(&00)'. PROCESSING ABORTED. PUBSET OR VOLUME-SET INCONSISTENT

### Response

See message PVR0129.
Take appropriate action in accordance with the return code.

## PVR0127

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0127 ERROR WHEN CLOSING VOLUME '(&00)'. RETURN CODE: '(&01)'

### Response

Take appropriate action in accordance with the return code.

## PVR0128

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0128 PUBSET OR VOLUME-SET SHOULD HAVE ID '(&00)' AFTER RENAMING, BUT THIS ID IS ALREADY IN USE. STATEMENT REJECTED

### Meaning

Possible reasons:
- A pubset or volume-set with the new name is already imported.
- Current pubset contains a standard net-storage volume, and a
net-storage volume with the new standard name already exists.

### Response

Use another name for the new CATID, or rename / delete the existing
net-storage volume.

## PVR0129

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0129 PUBSET OR VOLUME-SET INCONSISTENT. STATEMENT PROCESSING ABORTED

### Meaning

The program terminated abnormally during an earlier conversion of
the pubset or volume-set. VSN-ENTRIES in SVL/OLC of PUBRES incorrect.

### Response

The pubset or volume-set can only be converted if the operands are
given the same values as they had before the abnormal program
termination. Please correct the wrong entries written into the
SVL/OLC of the PUBRES during the last conversion of the pubset.

## PVR0130

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0130 PROGRAM ERROR '(&00)'. PROGRAM ABORTED

### Meaning

The program has detected an error.
(&00): error code, important for the maintenance staff.

### Response

Forward the console log for diagnosis.

## PVR0131

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0131 NO MRSCAT ENTRY FOUND FOR PUBSET WITH CATID '(&00)'. PROCESSING ABORTED

### Response

Please create a MRSCAT entry for this pubset with the Command
/ADD-MASTER-CATALOG-ENTRY and try again. For a volume set the renaming
was completly executed by SHC-OSD. There is no further action necessary.

## PVR0132

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0132 HSMS-FILE OR ARCHIVE-SAVE LOCATED IN FILE-CATALOG

### Meaning

During the filenamelength-check, in the TSOSCAT of the PVS to be
converted, a HSMS/ARCHIVE-SAVE - catalog-entry was found.
To save these CE's, the CMD 'CONVERT-PUBSET' isn't allowed at the moment.

### Response

Erase all HSMS/ARCHIVE-SAVE - catalog-entries before starting PVSREN
again.

## PVR0133

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0133 PUBSET OR VOLUME-SET HAS TOO MANY DISCS. RENAMING IS NOT POSSIBLE

### Meaning

The new name of the pubset or volume-set defines the maximum number
of disc.
Catid = A : maximum number of disc = 32
Catid = AB : maximum number of disc = 255
Catid = ABC : maximum number of disc = 255
Catid = ABCD : maximum number of disc = 36

### Response

Use a name with two or three characters.

## PVR0134

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0134 FOLLOWING OBJECT NAMES EXCEED MAXIMUM LENGTH OF '(&00)' OR '(&01)' CHARACTERS:

### Meaning

The check carried out, prior to conversion, of the file and job variable
names (maximum length (&00)) or of the file group names (maximum
length (&01)) detected excessively long names.

### Response

Correct the lengths of the object names and start conversion (again).

## PVR0135

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0135 LENGTH OF OBJECT NAMES ACCEPTED. CONVERSION CAN BE STARTED

### Meaning

The object name check failed to find any names that exceeded the
maximum permissible length.

### Response

Conversion is started or the CONVERT-PUBSET statement can be
processed.

## PVR0136

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0136 FILE CATALOG 'TSOSCAT' SUCCESSFULLY UPDATED

### Meaning

The file catalog of the pubset or volume-set was successfully updated.

## PVR0137

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0137 VOL1 LABELS SUCCESSFULLY UPDATED

### Meaning

The VOl1 labels of the pubset or volume-set were successfully updated.

## PVR0138

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0138 USER CATALOG 'TSOSJOIN' SUCCESSFULLY UPDATED

### Meaning

The user catalog of the pubset was successfully updated.

## PVR0139

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0139 PUBSET OR VOLUME-SET '(&00)' HAS BEEN RENAMED TO THE NEW NAME '(&01)'

### Meaning

The pubset or volume set was successfully renamed.

## PVR0140

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0140 All volumeset lists on the new sm pubset '(&00)' habe been adapted or have been deleted together with all storage class definitions.

### Meaning

Either all volumeset list habe been adapted or all all volumeset lists
and all storage class definitions have been deleted.

### Response

Response
- none

## PVR0142

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0142 RENAMING WITH PUBSET-PAR=*SAME FAILED, CONTINUING WITH PUBSET-PAR=*STD

### Response

Set desired pubset parameters manually using the
/MODIFY-MASTER-CATALOG-ENTRY command.

## PVR0143

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0143 STATEMENT COULD NOT BE PROCESSED WITHOUT ERRORS

### Response

The appropriate action is indicated in the previous PVR message.

## PVR0144

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0144 PVSREN TERMINATED ABNORMALLY

### Response

The appropriate action is indicated in the previous PVR message.

## PVR0145

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0145 PVSREN TERMINATED NORMALLY

### Meaning

The program was terminated normally via the END statement.

## PVR0146

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0146 CAT-ID '(&00)' is invalid.

### Meaning

There is no pubset or volume set with this cat-id.

### Response

Response
- none

## PVR0147

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0147 An error occurred while the device type of the target discs was updated.

### Meaning

More detailed information on the detected errror(s) may be found in the
preceding messages.

### Response

Response
- none

## PVR0150

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0150 'SYSID=*SAME' IS NOT ALLOWED, IF CATID FOR 'NAME' OR 'NEW-NAME' HAS ONLY ONE CHARACTER.

### Response

Use *STD.
Use <integer 65..195>, if CATID for 'NEW-NAME' has more than one
character.

## PVR0151

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0151 'SYSID=<INTEGER 65..192>' IS NOT ALLOWED, IF CATID FOR 'NEW-NAME' HAS ONLY ONE CHARACTER

### Response

Use *STD.

## PVR0152

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0152 STATEMENT 'CONVERT-PUBSET' IS ONLY ALLOWED FOR SF-PUBSETS. USE STATEMENT 'RENAME-PUBSET-OR-VOLUME-SET'.

### Meaning

The statement 'CONVERT-PUBSET' may not be used to rename a SM-Pubset or
a Volume-Set. It is only allowed for SF-Pubsets.

### Response

Use statement 'RENAME-PUBSET-OR-VOLUME-SET'.

## PVR0153

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0153 INFORMATIONS IN THE MRSCAT-ENTRY '(&00)' DO NOT AGREE WITH THE INFORMATIONS IN THE SVL OF DISK '(&01)'.

### Meaning

Pubset type, CATID of the Control-Volume-Set or CATID of the SM-Pubset
in the MRSCAT-Entry &00 does not agree with the information in the
SVL of the disk &01.

### Response

Check MRSCAT-Entry and corresponding disk. Remove the conflict and
repeat the renaming.

## PVR0154

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0154 PUBSET '(&00)' IS LOCKED. RENAMING IS NOT POSSIBLE AT THE TIME.

### Meaning

The SF-Pubset or SM-Pubset &00 is locked through an active PVSREN run
or a PVSREN run, that has been terminated abnormally.
A volume-set, that belongs to a SM-Pubset, can only be renamed, if
the SM-Pubset is not locked.
A SM-Pubset is locked, if the SM-Pubset or a volume-Set, that belongs
to the SM-Pubset, is renamed.

### Response

In case of an active PVSREN run, wait until the run has been finished.
In case of an abnormal terminated PVSREN run, use the statement
'RESTART-RENAMING', to remove the lock. This statement requires the
logging file SYSLOG.PVSREN.<catid-old>.<catid-new>, that is created
by PVSREN.

## PVR0155

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0155 VOLUME-SET '(&00)' IS DEFECT OR DEFINED ONLY. RENAMING IS NOT PROCESSED.

### Meaning

It is not possible to rename a defect volume set.
If a SM-pubset contains a defect volume set, it is not possible to
rename the SM-pubset or the control-volume-set.
For a defined only volume set there is only an entry in the
configuration file of the pubset.

### Response

Remove the defect volume set from the pubset. All files of this
volume set will be lost.
For a defined only volume set the Configuration can be changed with
the command 'MODIFY-PUBSET-PROCESSING'.

## PVR0156

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0156 THE CATID OF THE SM-PUBSET IN THE SVL OR IN THE PUBSET CONFIGURATION FILE FOR THE VOLUME SET '(&00)' IS NOT CORRECT.

### Meaning

The configuration of the SM-pubset is inconsistent.
The CATID of the SM-Pubset, to which the volume set belongs, is stored
in the pubset configuration file. This information does not agree with
the information that ist stored in the SVL of the volume set.

### Response

Check and correct the configuration. Repeat the PVSREN run.

## PVR0157

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0157 EXCLUSIVE ALLOCATION NOT POSSIBLE FOR DISK '(&00)'. RETURNCODE '(&01)'. PROCESSING ABORTED.

### Meaning

Returncode &01 comes from the interface $NKAADS.

### Response

Check the returncode. Repeat the run.

## PVR0158

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0158 DISK '(&00)' GETS THE VSN '(&01)' AFTER RENAMING. THIS DISK ALLREADY EXISTS. PROCESSING ABORTED.

### Meaning

A disk with the VSN &01 allready exists.
It is not possible to rename the pubset, because this would lead to two
disks with the same VSN.

### Response

Use an other name for the new CATID.

## PVR0159

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0159 THE USERID HAS NOT THE PRIVILEG 'USER-ADMINISTRATION'. STATEMENT 'MODIFY-JOINFILE' CAN NOT BE PROCESSED.

### Meaning

Without the privilege 'USER-ADMINISTRATION' it is not possible, to
change the default-Catid.

### Response

Grant the privilege for the userid and repeat the PVSREN run.

## PVR0160

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0160 INVALID STATEMENT '(&00)'. PROCESSING CONTINUES.

### Meaning

The statement is unknown to this version of PVSREN and is
therefore not processed.

### Response

Check, if the right version of PVSREN is installed.
Check the syntaxfile.

## PVR0161

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0161 STATEMENT 'CHECK-FILENAME-LENGTH' IS NOT ALLOWED FOR VOLUME-SETS.

### Meaning

The renaming of a volume-set has no effect to the length of the
filenames placed on this volume-set, because files are adressed
with the pubset-ID. Therefore the statement CHECK-FILENAME-LENGHT
is not allowed for volume-sets.

### Response

Use statement CHECK-FILENAME-LENGTH with the SM-pubset, that includes
this volume-set.

## PVR0162

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0162 DISK CONFIGURATION FOR VSN '(&00)' IS NOT CORRECT.

### Meaning

Possible reasons:
- There are more than two disks with the same VSN.
- There are two disks with the same VSN that do not belong to a
DRV-pubset or DRV-volume-set.
- The discs do not have the same DRV state.
- The pubset or volume set is not running in DRV-DUAL mode.
- With CREATE-PUBSET-FROM-MIRROR there are not exactly two discs with
the same mentioned VSN in the state 'attached'.

### Response

Check and corret the disc configuration and repeat the PVSREN run.

## PVR0163

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0163 RENAMING COULD NOT BE PROCESSED WITHOUT ERRORS. PUBSET OR VOLUME-SET IS IN AN INCONSISTENT CONDITION.

### Meaning

The renaming has been aborted in a phase, where already changes have
been made. It is not possible to import the pubset at the moment.

### Response

Correct the reason, that lead to the error and restart the renaming
with the statement RESTART-RENAMING.
The pubset may not be imported, the disc configuration may not be
changed.

## PVR0164

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0164 LOGGINGFILE '(&00)' IS LOCKED. RENAMING IS NOT POSSIBLE AT THE MOMENT.

### Meaning

A renaming is already processed for the pubset or volume-set. Therefore
the loggingfile is locked.

### Response

Wait, until the renaming has been ended.

## PVR0165

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0165 FILE '(&00)' DOES NOT EXIST OR IS NO LOGGINGFILE.

### Meaning

The statement RESTART-RENAMING could not be processed.

### Response

Check, if the loggingfile exists. The filename is "SYSLOG.PVSREN.
<catid-old>.<catid-new>". The file is placed on the home pubset at
the userid TSOS.

## PVR0166

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0166 SEQUENCE NUMBER OF VSN '(&00)' IS TO GREAT. RENAMING CAN NOT BE PROCESSED.

### Meaning

The format of the VSN depends on the length of the CATID of the pubset
or volume-set.
CATID = A : VSN = PUBAxx
CATID = AB : VSN = AB.xxx
CATID = ABC : VSN = ABC.xx
CATID = ABCD : VSN = ABCD.x
The VSN &00 of the old pubset or volume-set can not be changed to the
VSN of the new pubset or volume-set.

### Response

Use a CATID for the new pubset or volume-set, that makes it possible,
to change the VSN.

## PVR0167

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0167 SOME DATA IN PUBSET CONFIGURATION FILE OF SM-PUBSET '(&00)' DIFFER FROM CORRESPONDING DATA IN MRSCAT ENTRY OR STANDARD VOLUME LABEL.

### Meaning

One or more of the following data items in the pubset
configuration file do
not agree with the corresponding items in the MRSCAT entry or in the SVL
of the volume:
CATID of the SM-pubset
CATID of the control volume set
Device code of the control volume set

### Response

Check configuration of the SM-pubset.

## PVR0168

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0168 SUBSYSTEM 'DRV' IS NOT AVAILABLE. RENAMING IS NOT POSSIBLE.

### Meaning

Subsystem DRV is necessary for the following actions:
- renaming of a DRV pubset or DRV volume set.
- renaming of a SM pubset, that contains a DRV volume set.

## PVR0169

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0169 CONTROL VOLUME SET '(&00)' DOES NOT BELONG TO SM-PUBSET '(&01)'.

### Meaning

The catid of the SM pubset in the SVL of the control volume set does not
agree with already available information. The catid of the control volume
set comes from the MRSCAT entry of the SM pubset or from the SVL of the
volume set.

### Response

Check the MRSCAT entry of the SM pubset or the SVL of the volume set.

## PVR0171

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0171 Syntax error in statement '(&00)'

### Response

- Correct statement.

## PVR0172

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0172 FILE 'TSOSCAT.(&00)' ALREADY EXISTING. RENAMING IS NOT POSSIBLE.

### Meaning

At renaming of a volume set, the name of the catalog file has to be
changed. A file with the new name already exists, so the renaming is
not possible.

### Response

Use a catid, that allowes the renaming

## PVR0173

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0173 AN ENTRY WITH THE NEW NAME '(&00)' ALREADY EXISTS IN THE PUBSET CONFIGURATION FILE

### Meaning

The renaming is not processed, because this would lead to
two entries with the same CATID.

### Response

Use another name for the new CATID.

## PVR0174

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0174 Volume '(&00)' is not mounted on emulated target disk of disk emulation. Command rejectd.

### Meaning

During processing of the command /FINISH-DISK-EMULATION certain data
structures on the target device are adapted to the new (native) device
type. Onyl the target device maust be on-line.

### Response

Make sure the target discs are on-line:
- Check status of target discs with command /SHO-DISC-STATUS
- If necessary attach target discs with command /ATTACH-DEVICE
- If necessary detach source disks with command /DETACH-DEVICE

## PVR0175

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0175 Check of volume '(&00)' returned error code '(&01)'. Processing aborted.

### Meaning

During processing of the command /FINISH-DISK-EMULATION a check of a
volume with interface NKLMCAL resulted in a negative error code.

### Response

- Check status of target discs with command /SHOW-DISC-STATUS
- Contact system administrator

## PVR0176

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0176 SNAPSET CATALOG FOUND FOR PUBSET '(&00)'. RENAMING NOT ALLOWED.

### Meaning

A snapset catalog was found for the pubset (&00). Renaming of the
specified SF pubset, SM pubset or volumeset
is not allowed because after renaming access
to the snapsets would not be possible anymore.

### Response

On an imported pubset the snapset catalog can be deleted by the command
DELETE-SNAPSET <Pubset-Id>,SNAPSET=*ALL.

## PVR0177

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0177 Volume information for device '(&00)' is in unexpected state

### Meaning

It was tried to attach or detach device '00'. The macro NKDINF
returns an unexpected VSN or an unexpected attachment state after
several trials.

### Response

Eventually correct the VM assignment state of the device.

## PVR0178

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0178 VSNs of pubset '(&00)' could not determined due to DPSVLST error '(&01)'

### Meaning

The macro DPSVLST delivered a returncode.

### Response

Check whether there are already attached mirrors (BCVs, SNAPs or
CLONEs) of the original pubset or not. If so, deallocate those mirrors.

## PVR0180

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0180 NO VALID PUBLIC VSN GIVEN

### Meaning

The selected function is support for public volumes, only

## PVR0181

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0181 VOLUME '(&00)' NOT ONLINE. PROCESSING ABORTED

## PVR0182

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0182 VOLUME '(&00)' OF PUBSET OR VOLUME-SET NOT ONLINE. PROCESSING CONTINUES WITH NEXT DISK

## PVR0183

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0183 LABELS OF PUBSET / VOLSET '(&00)' SUCCESSFULLY RESTORED

## PVR0184

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0184 LABELS OF PUBSET '(&00)' SUCCESSFULLY RESTORED

## PVR0185

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0185 LABELS OF PUBSET / VOLSET '(&00)' PARTIALLY RESTORED

### Meaning

Possible reasons:
- not all disks of pubset / volset are available
- one or more disks have not the expected VSN

## PVR0186

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0186 CONTROL VOLUMESET '(&00)' NOT AVAILABLE; PROCESSING ABORTED

## PVR0187

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0187 LABELS OF PUBSET '(&00)' PARTIALLY RESTORED

### Meaning

Possible reasons:
- not all disks of pubset / volset are available
- one or more disks have not the expected VSN

## PVR0188

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0188 PROCESSING OF PUBSET/VOLSET '(&00)' TERMINATED ABNORMALLY

## PVR0189

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0189 Disk '(&00)' not available; all following disks are skiped

## PVR0190

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0190 RENAMING OF CATID IN IMON SCI OF THE HOME PUBSET SUCCESSFULLY COMPLETED

## PVR0191

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0191 RENAMING OF CATID IN IMON SCI OF HOME-PUBSET NOT SUCCESSFULLY COMPLETED; /HELP-MSG '(&00)'

### Meaning

The implicit called command /MODIFY-IMON-SCI has signaled an error.
The entries for this pubset are not or not completely renamed in the
IMON SCI of the Home-Pubset. The execution continues.

### Response

Please correct error and try the command /MODIFY-IMON-SCI again after
termination of PVSREN.

## PVR0192

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0192 RENAMING OF CATID IN IMON-SCI OF PUBSET '(&00)' NOT SUCCESSFULLY COMPLETED; /HELP-MSG '(&01)'

### Meaning

The implicit called command /MODIFY-IMON-SCI has signaled an error. The
entries for this pubset are not or not completely renamed in the IMON SCI.
The execution continues.

### Response

Please correct error and try the command /MODIFY-IMON-SCI again after
termination of PVSREN.

## PVR0193

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0193 CONVERSION OF CATALOG '(&00)' TO EXTRA-LARGE FORMAT HAS NOT BEEN COMPLETED. PROCESSING IS ABORTED.

### Meaning

(&00): Pubset id or volume set id

### Response

Import pubset; conversion of catalog to extra-large format is completed
as part of import processing. After exporting the pubset repeat aborted
PVSREN statement.

## PVR0194

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0194 NET-STORAGE VOLUME '(&00)' COULD NOT BE ADAPTED TO RENAMED PUBSET '(&01)'

### Meaning

A Net-Storage volume indicated within a TSOSCAT could not be adapted to
the catid of the renamed pubset. The PVSREN processing proceeds normally.

### Response

The adaption must be made later and outside of PVSREN or the
Net-Storage volume must be removed from the pubset.

## PVR0195

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0195 RENAMING OF CATID IN IMON-SCI OF PUBSET '(&00)' SUCCESSFULLY COMPLETED

### Meaning

NO FURTHER INFORMATION

### Response

NONE

## PVR0199

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0199 INTERNAL PROGRAM ERROR '(&00)'. PROCESSING ABORTED.

### Meaning

The parameter &00 marks the place, where the error has been occured.

### Response

Compile error documents and send them to the systems engineer.

## PVR0200

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

PVR0200 USER CATALOG 'TSOSJOIN' CANNOT BE UPDATED. START CONVERSION NEVERTHELESS ? (Y=YES; N=NO)

### Meaning

- A BS2000 version < V10.0 is used to rename a pubset with
a catalog ID comprising more than one character.
The pubset must be readied before the user catalog is updated, but
the multi-character catalog ID of the pubset in the present BS2000
version prevents this.
- A BS2000 version >= V10.0 is used and the userid has not the
privilege "USER-ADMINISTRATION".

### Response

Y: - dynamically convert the user catalog to a BS2000 version >= V10.0
using the PVSREN statement MODIFY-JOINFILE.
- grant the privilege "USER-ADMINISTRATION" for the userid and convert
the user catalog using the PVSREN statement MODIFY-JOINFILE.
N: - perform the entire conversion with a BS2000 version >= V10.0.
- grant the privileg "USER-ADMINISTRATION" for the userid and repeat
the entire conversion.

## PVR0201

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

PVR0201 CHANGE DEFAULT CATALOG ID ENTRY '(&00)' TO DEFAULT CATALOG ID ENTRY '(&01)' IN USER CATALOG OF HOME PUBSET ? (Y=YES; N=NO)

### Meaning

The conversion may result in invalid default catalog ID entries in
the user catalog of the home pubset.

### Response

Y: the user catalog is searched for default catalog ID entry (&00) and,
if it is found, it is changed to default catalog ID entry (&01).
N: the user catalog is not processed.

## PVR0202

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

PVR0202 CHANGE DEFAULT CATALOG ID ENTRY '(&00)' TO DEFAULT CATALOG ID ENTRY '(&01)' IN USER CATALOG OF NEW PUBSET ? (Y=YES; N=NO)

### Meaning

The user catalog of the modified pubset contains the old catalog ID
as the default catalog ID.

### Response

Y: the user catalog is searched for default catalog ID entry (&00) and,
if it is found, it is changed to default catalog ID entry (&01).
To this end the pubset is imported using the command /IMPORT-PUBSET.
N: the user catalog is not processed.
The pubset is not imported.

## PVR0203

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

PVR0203 READY PUBSET IN THIS BS2000 SYSTEM ? (Y=YES; N=NO)

### Meaning

The user's response to the query in message PVR0202 determines
whether or not the pubset is available.
Accordingly, and depending on the response to the present
message, the following measures are taken in the program:

### Response

Y and pubset is available : the pubset remains available.
Y and pubset is not available: the pubset is made available
N and pubset is available : the pubset is not made available
N and pubset is not available: the pubset remains unavailable.

## PVR0204

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0204 SAME LABEL. CONTINUE RENAMING? (Y=YES; N=NO)

### Meaning

As the answer is, the pubset will be renamed or it won't be renamed.

### Response

No further information.

## PVR0205

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0205 MRSCAT-ENTRY '(&00)' ALREADY EXISTS. CONTINUE RENAMING ? (Y=YES; N=NO)

### Meaning

The mrscat entry for the new name already exists. If the renaming
continues, the entry will be deleted and created with new values.

### Response

Reply = Y : renaming continues and the mrscat entry will be deleted.
Reply = N : renaming will be aborted.

## PVR0206

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0206 CHANGE CATID ENTRY '(&00)' IN STANDARD IMON SCI OF HOME PUBSET TO CATID '(&01)' ? (Y=YES; N=NO)

### Meaning

This function changes all entries in the IMON SCI of the home pubset
related to the renamed pubset from the old catid to the new one.

## PVR0207

Destination: USER-TASK Routing code: Weight:

Warranty : NO

PVR0207 Adapt all volumeset lists on the new SM pubset '(&00)' to the new volumeset names or delete them together with all storage class definitions? (Y=ADAPT; D=DELETE; N=NO)

### Meaning

A volumeset list is a named list of volumset names. After renaming or
splitting to a new sm pubset the volumeset lists on the new sm pubset now
still contain the volumeset names of the original sm pubset. It has to be
taken decision now on how to proceed with those volumeset lists and the
storage class definitions on the new sm pubset.

### Response

Reply = Y : All volumeset lists on the new sm pubset will be adapted to
the volumeset names of the new sm pubset. The storage class
definitions on the new sm pubset remain unchanged.
Reply = D : All volumeset lists and all storage class definitions on the
new sm pubset will be deleted.
Reply = N : All volumeset lists and all storage class definitions on the
new sm pubset remain unchanged

## PVR0301

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0301 Creation of an SM-Pubset from a Pubset Mirror: Catid '(&00)' is not a unique source catid.

### Response

- Correct source catids of corresponding statements in mapping file.

## PVR0302

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0302 Creation of an SM-Pubset from a Pubset Mirror: Catid '(&00)' is not unique as a new catid of a volume set.

### Response

- Correct source catids of corresponding statements in mapping file.

## PVR0303

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0303 Creation of an SM-Pubset from a Pubset Mirror: Catid '(&00)' occurs both as a source catid and a new catid.

### Response

- Correct catids of corresponding statements in mapping file.

## PVR0304

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0304 Creation of an SM-Pubset from a Pubset Mirror: Catid '(&00)' of control volume set is missing as a source catid

### Response

- Add corresponding statement for missing source catid to mapping file.

## PVR0305

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0305 Creation of a Pubset from a Pubset Mirror: Catids '(&00)' of source pubset and '(&01)' of new pubset differ in length.

### Response

- For the new pubset choose a catid with the same length as the source
catid.

## PVR0306

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0306 Creation of an SM-Pubset from a Pubset Mirror: New Pubset is assigned the catid '(&00)' of source pubset.

### Response

- Select a fidderent catid for the new pubset.

## PVR0307

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0307 Creation of an SM-Pubset from a Pubset Mirror: New Pubset '(&00)' could not be created. The mirror of the source pubset '(&01)' was restore to its initial state.

### Response

- none

## PVR0308

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0308 Creation of an SM-Pubset from a Pubset Mirror: Volume set with catid '(&00)' was not found in the configuration file of the SM pubset.

### Response

- Correct statements in mapping file so that the its source catids agree
with the catids of the volume sets in the configuration file.

## PVR0309

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0309 Creation of an SM-Pubset from a Pubset Mirror: The catid '(&00)' of the new SM pubset coincides with a catid of one of the new volume sets.

### Response

- Choose different catids for new pubst and ist new volume sets.

## PVR0310

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0310 Creation of an SM-Pubset from a Pubset Mirror: The catid '(&00)' of the source SM pubset coincides with a catid of one of the volume sets of the new SM pubset.

### Response

- Choose different catids for new pubset and ist new volume sets.

## PVR0311

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0311 File '(&00)' is catalogued on source pubset. Catalogue for corresponding volume set of new pubset cannot be created.

### Meaning

No futher information.

### Response

Action:re the target discs are on-line:
- Choose a diferent catid fo the new volume set.
- Erase file, if possible.

## PVR0312

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0312 File '(&00)' is catalogued on source pubset. Catalogue for control volume set of new pubset cannot be created.

### Meaning

No futher information.

### Response

Action:re the target discs are on-line:
- Choose a diferent catid fo the new control volume set.
- Erase file, if possible.

## PVR0313

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0313 For the sourc volume set with catid '(&00)' no volumes were on-line. The volume set is not in state DEFINED_ONLY.

### Meaning

If a volume set is not in state DEFINED_ONLY there must be at least one
volume belonging to it.

### Response

Make sure the source discs are on-line:
- If necessary attach source disks with command /ATTACH-DEVICE

## PVR0314

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0314 The number of volume sets in the pubset configuration file of SM pubset '(&00)' does not agree with the number of volume sets for which the statement SET-NAME-OF-NEW-VOLUME-SET has been specified.

### Meaning

For the catid of each of the volume sets of a SM pubset, from the mirror
volumes of which a new pubset is to be created, a new catid for the
corresponding volume set in the SM pubset to be created has to be
specified by means of the statement SET-NAME-OF-NEW-VOLSET. Therefore the
number of SET-NAME-OF-NEW-VOLSET has to be equal to the number of volume
sets in the configuration file.

### Response

Response:
- Correct the file in which the renaming of the volume sets is specified.

## PVR0333

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

PVR0333 New Volume Set '(&01)' cannot be created from mirror with catid '(&00)': Maximum number of volumes is exceeded.

### Meaning

The number of volumes required for the new volume set exceeds the
maximum number of volumes possible catid.

### Response

Action:
- Choose a different catid that permits a larger maximum number
of volumes.
A catid with the same number of characters as the corresponding
source catid is a safe choice.

©2025 Fujitsu | BS2000 System Messages