## CMS0001

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0001 SLOT MANAGER ERROR

### Meaning

An internal error occurred when requesting or releasing an MRSCAT
entry slot.

### Response

Produce diagnostic material.

## CMS0002

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

CMS0002 DISK ERROR. ELEMENTS CONCERNED: '(&00)'

### Meaning

The MRSCAT in the main memory has been updated correctly, but
an error occurred during the modification of the disk MRSCAT.
The elements concerned could not be updated.
(&00) = TSOSCAT : TSOSCAT part of MRSCAT
ORIGINAL : system file containing the disk MRSCAT
(the file name is: SYSTEM.MRSCAT)
DUPLICATE : copy of that system file
(the file name is: SYSTEM.MRSCAT.COPY)
The session can continue with the consistent elements of the
MRSCAT.

### Response

Check whether the elements concerned are in use.
Produce diagnostic material if necessary.
A repair of the corrupted elements is attempted automatically
during the next /ADD-, /MODIFY- or /REMOVE-MASTER-CATALOG-ENTRY
command.
It is, however, not certain that the corrupted elements have
really been repaired if the subsequent command leads to an error.

## CMS0003

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0003 MRSCAT ENTRY CANNOT BE DELETED

### Meaning

As the specified pubset is currently in use, the corresponding
MRSCAT entry cannot be deleted.

### Response

Retry the command later.

## CMS0004

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0004 MRSCAT ENTRY ALREADY EXISTS

### Meaning

The new MRSCAT entry could not be inserted, as an entry
with the specified catalog ID already exists.

## CMS0005

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0005 TOO MANY ENTRIES IN THE MRSCAT

### Meaning

The current number of MRSCAT entries exceeds the maximum number
permitted by the class 2 option DMCMAXP. No new entry can be
inserted.

### Response

Delete MRSCAT entries until their current number is lower than
their permitted maximum. Retry the command.

## CMS0006

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0006 INVALID CLASS 2 OPTION

### Meaning

The value of the class 2 option DMCMAXP is not in the permitted
range or an invalid catalog ID was found in the paging pubset
table.

### Response

Produce diagnostic material.

## CMS0007

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0007 NO RECONSTRUCTION REQUIRED

### Meaning

As all the elements are o.k., there is no reason to repair
the disk MRSCAT.

## CMS0010

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0010 COMMAND RESTRICTED TO SYSTEM ADMINISTRATOR

## CMS0011

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0011 SYNTAX ERROR

### Meaning

At least one of the specified operands was invalid.

### Response

Correct and retry.

## CMS0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

CMS0012 MRSCAT ENTRY CANNOT BE MODIFIED

### Meaning

The following restrictions apply for the modifications:
- The BCAM name of the host computer or the device name of the
pubset cannot be modified if the pubset is not inaccessible
or if /IMPORT-PUBSET or /EXPORT-PUBSET is being processed.
- The WAIT status cannot be modified for the local home pubset
or for paging pubsets.
- The static information share/exclusive, buffer class or buffer
number cannot be modified if /IMPORT-PUBSET is being processed.
- The name of the control volume set of the system managed pubset
cannot be modified if the pubset is not inaccessible or if /IM-
PORT-PUBSET or /EXPORT-PUBSET is being processed.

## CMS0013

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0013 THE SPECIFIED PUBSET IS NOT IN THE SELECTED STATE

### Meaning

The error occured when a catalog ID (or #) was specified for the
/SHOW-MASTER-CATALOG-ENTRY command in conjunction with the SELECT
operand.
An MRSCAT entry does exist with the specified catalog ID, but the
corresponding pubset is not in the state specified in the SELECT
operand.
No output is displayed.

## CMS031A

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS031A MRSCAT NOT INITIALIZED

### Meaning

During startup /SHOW-MASTER-CATALOG-ENTRY can be
performed only with the local home catalog ID,
as long as the MRSCAT is not initialized.

### Response

Retry the command later.

## CMS031B

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS031B TRANSMISSION ERROR

### Meaning

An internal error occurred on attempting to exchange
data with a remote computer.
The error could happen during AQUIRE or DEALLOCATE or
during the MSCF connection.

### Response

Contact the system administrator.

## CMS031C

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS031C INVALID HOST NAME

### Meaning

The value of the operand HOST is not correct:
- The BCAM name specified is unknown.
- The BCAM name specified is not the name of a sharer of the
pubset.
- The pubset is an exclusive one and the BCAM name specified
is the name of a remote computer.
- The local computer is not the master of the shared pubset
and the BCAM name specified is the name of a remote computer.

### Response

Correct and retry.

## CMS031F

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS031F MRSCAT OPERAND ERROR

### Meaning

An internal error occured on processing the basic
MRSCAT access function.

### Response

Contact the system administrator.

## CMS0310

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0310 SRPM ERROR

### Meaning

An error occurred on checking the user privileges.

### Response

Contact the system administrator.

## CMS0311

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0311 OPERAND ERROR IN STAM

### Meaning

An internal error occurred during processing of the STAM function.
For more detailed information see the manual 'Executive Macros'.

### Response

Contact the system administrator, if necessary.

## CMS0312

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0312 MRSCAT ENTRY NOT FOUND

### Meaning

No MRSCAT entry exists corresponding to either:
- the specified catalog ID, or
- the specified wildcard, or
- the specified SELECT operand.

## CMS0313

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0313 REQM OR RELM ERROR

### Meaning

An error occurred when memory space was requested or
released.

### Response

Check the available memory space and contact the system
administrator if necessary.

## CMS0314

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0314 SYNTAX ERROR IN ENTRY NAME OR WILDCARD

## CMS0315

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0315 NO MEMORY SPACE TO BE RELEASED

### Meaning

Data in main memory are corrupted.

## CMS0316

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0316 AREA TOO SMALL

### Meaning

An internal error occured during command processing.
The requested memory size is insufficient.

### Response

Contact the system administrator.

## CMS0317

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0317 MRSCAT LOCK CONFLICT. TAKE SYSTEM DUMP

### Meaning

A system module has not released an MRSCAT lock
previously set for the current task.

### Response

Contact the system administrator.

## CMS0318

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0318 SYNCHRONIZATION ERROR DUE TO TASK LOCK MANAGER PROBLEM

### Response

Contact the system administrator.

## CMS0319

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0319 PUBSET TYPE CONFLICT

### Meaning

A wrong pubset type was specified for the MRSCAT entry.

### Response

Correct and retry.

## CMS0320

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0320 VOLUME SET NOT FOUND

### Meaning

The volume set which is specified for the system managed
pubset could not be found in the MRSCAT.
A wrong catalog ID was specified for the volume set or
there is no existing MRSCAT entry for the volume set.

### Response

Correct the catalog ID or create a MRSCAT entry for the
volume set. Retry.

## CMS0321

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

CMS0321 PUBSET NOT ACCESSIBLE

### Meaning

As the specified system managed pubset is not accessible,
with the command /MODIFY-PUBSET-CACHE-ATTRIBUTES no update
of the configuration file of the pubset is possible.
At the moment only the values for FORCE-IMPORT and SIZE-
TOLERANCE can be modified.

### Response

Retry the command when the pubset is in accessible state.

©2025 Fujitsu | BS2000 System Messages